FCA CANADA
2017 Jeep® Wrangler Unlimited
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

General Information		
Vehicle Type	Four-door sport-utility vehicle	
Assembly Plant	Toledo, Ohio, USA	
EPA Vehicle Class	Multipurpose vehicle	
Introduction Date	2007 	
		
BODY/CHASSIS		
Layout	Longitudinal front engine, four-wheel drive	
Construction	Ladder-type frame, open steel body	
		
Engine:  3.6-LITRE PENTASTAR V6	
Availability	Standard — all models	
Type and Description	60-degree, V-type, liquid-cooled	
Displacement 	3,604 cu cm (220 cu in) 	
Bore x Stroke 	96 x 83 (3.78 x 3.27) 	
Valve System	Chain-driven DOHC, 24 valves and hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Aluminum deep-skirt block, aluminum alloy heads 	
Compression Ratio	10.2:1	
Power (SAE net) (hp / kW@rpm)	285 hp (209 kW) at 6,400 rpm	
Torque (SAE net) (lb-ft / N•m)	260 lb-ft (353 N•m) at 4,800 rpm	
Max. Engine Speed (rpm)	6,600 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R + M)/2	
Fuel Tank Capacity litres (imperial gallons)	85.2 (18.7)	
Oil Capacity 	5.7 litres (6.0 quarts) 	
Coolant Capacity 	13.25 litres (14 quarts) 	
Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors
and internal engine features	

EnerGuide (2016) Fuel Consumption Ratings L/100 km (MPG – imperial gallon) city/hwy/combined 	15.0/11.4/13.4 (19/25/21) — manual
14.8/11.7/13.4 (19/24/21)  — automatic 	
Engine Assembly Plant	Trenton, Mich., USA	
Based on 2016 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information, please visit the Government of Canada website: www.vehicles.nrcan.gc.ca 	
		
Transmission: W5A580 automatic, five-speed overdrive	
Availability	Optional — all models	
Description	Adaptive electronic control or Electronic Range Select (ERS) 
driver-interactive manual control and electronically modulated 
torque converter clutch	
Gear Ratios Automatic		
1st	3.59	
2nd	2.19	
3rd	1.41	
4th	1	
5th	0.83	
Reverse	3.16	
Final Drive Ratio	3.06:1	
Overall Top Gear	2.54	
		
Transmission: NSG 370 Manual, Six-speed with overdrive	
Availability	Standard — all models	
Description	Synchronized in all forward gears and Reverse, 
multi-rail shift system with top-mounted shift lever	
Clutch	Hydraulic actuation	
Gear Ratios		
1st	4.46	
2nd	2.61	
3rd	1.72	
4th	1.25	
5th	1	
6th	0.797	
Reverse	4.06	
Final Drive ratio	3.21 standard, 3.73 optional (4.10 Rubicon)	
Overall Top Gear	2.53 standard, 2.95 optional (3.24 Rubicon)	
	
TRANSFER CASE: NV241 command-trac	
Available	Standard — Sport, Sport S, Willys Wheeler and Sahara	
Type	Part-time	
Operating Modes	2WD High; 4WD High; Neutral; 4WD Low	
Center Differential Type	None	
Low Range Ratio	2.72:1	
	
TRANSFER CASE: NV241OR Rock-trac	
Available	Standard — Rubicon	
Type	Part-time	
Operating Modes	2WD High; 4WD High; Neutral; 4WD Low	
Center Differential Type	None	
Low Range Ratio	4.0:1	
Axle Ratio 
	3.21 standard, 3.73 optional (3.73 standard Rubicon with automatic) 
4.10 standard Rubicon with manual (optional for automatic)	
Overall Top-gear		2.53 standard, 2.95 optional  (2.95 standard Rubicon with automatic)
3.24 standard Rubicon with manual (optional for automatic)	
		
Axles		
Front   	Dana 30 (Sport, Sport S, Willys Wheeler, Sahara), Dana 44 (Rubicon)	
Differential Type	Open (Dana 30) or Tru-Lok electronic locking (Dana 44)	
Axle Ratios 	3.21, 3.73, 4.10	
Rear  	Dana 44	
Differential Type	Open (Sport, Sport S, Willys Wheeler and Sahara) with available Trac-Lok anti-spin, Tru-Lok electronic locking (Rubicon)	
Axle Ratios 	3.21, 3.73, 4.10	
		
Electrical System		
Alternator	160 amp	
Battery	600 CCA, maintenance free	
		
Suspension		
Front	Live axle, link coil, leading arms, track bar, coil springs, stabilizer bar	
Stabilizer bar	Electronic Sway-Bar Disconnect System — standard, Rubicon	
Shock type	Low-pressure (on 16-inch wheel packages) gas-charged shock absorbers — standard
Monotube high-pressure (on 17- and 18-inch wheel packages) 
gas-charged shock absorbers — standard	
Rear	Live axle, link coil, trailing arms, track bar, coil springs, stabilizer bar	
Shock type	Low-pressure (on 16-inch wheel packages) gas-charged shock absorbers — standard
Monotube high-pressure (on 17- and 18-inch wheel packages) 
gas-charged shock absorbers — standard	
		
STEERING		
Type	Power, recirculating ball with damper	
Overall Ratio	16.7:1 overall	
Turning Diameter (curb-to-curb) 	12.4 m (40.8 ft.) 	
Steering Turns (lock-to-lock)	3.5	
P/S pump	Hydraulic	
		
BRAKES		
Type	Power-assisted, anti-lock braking system 	
Availability	Standard	
Front		
Rotor size and type	302 x 28 (11.9 x 1.1)  vented rotor	
Caliper size and type	254 (10) single-diaphragm vacuum	
Rear		
Rotor size and type	302 x 28 (11.9 x 1.1) vented rotor	
Caliper size and type	66 (2.6) single-piston floating caliper	
		
Dimensions and Capacities		
Wheelbase	2,947 (116) 	
Overhang — Front 	679 (26.7) 	
Overhang — Rear	778 (30.6) 	
Track — Front	1,572 (61.9)	
Track — Rear	1,572 (61.9) 	
Overall Length (includes spare tire)	4,697 (184.9) 	
Overall Width	1,873 (73.7) 	
Overall Height	1,844 (72.6) 	
Liftover Height 	706 (27.8) 	
Cargo Width at Swing-Gate Opening	1,491 (58.7) 	
Cargo Height at Swing-Gate Opening	942 (37.1) 	
Load Floor Height	706 (27.8) 	
		
CLEARANCES		
	P225/75R16
Standard on Sport	P255/75R17
Optional on Sport	P255/70R18
Standard on Sahara	LT255/75R17
Standard on Rubicon, Optional on Sport	
Approach Angle (degrees)	38.5	41.3	41.7	42.2	
Breakover Angle (degrees)	17.8	20.4	20.7	21.2	
Departure Angle (degrees)	29.2	31.8	32.1	32.5	
Ground Clearance (inches)	8.2	9.5	9.7	10	
		
CURB WEIGHT		
Wrangler Sport, 
Manual Transmission, kg (lbs.)	1,848 (4,075) 	
Wrangler Sport, 
Automatic Transmission, kg (lbs.)	1,860 (4,100) 	
Wrangler Sahara, 
Manual Transmission, kg (lbs.)	1,936 (4,269) 	
Wrangler Sahara, 
Automatic Transmission, kg (lbs.)	1,948 (4,294) 	
Wrangler Rubicon, 
Manual Transmission, kg (lbs.)	1,957 (4,315) 	
Wrangler Rubicon, 
Automatic Transmission, kg (lbs.)	1,969 (4,340) 	
		
Accommodations		
Seating Capacity (front/rear) 	2/3	
SAE Total Interior Passenger Volume, litres (cu. ft.)	2,945 (104) 	
Front		
Headroom	1,048 (41.3)	
Legroom	1,041 (41.0) 	
Shoulder Room	1,417 (55.8) 	
Hip Room	1,413 (55.6) 	
Seat Travel	240 (9.4) 	
EPA Front Volume Index, litres 
(cu. ft.)	1,546 (54.6)	
Rear		
Headroom	1,025 (40.4) 	
Legroom	1,041 (37.2) 	
Knee Clearance	1,566 (61.6)	
Shoulder Room	1,443 (56.8) 	
Hip Room	1,440 (56.7) 	
EPA Rear Seat Volume Index, 
litres (cu. ft.)	1,399 (49.4) 	
Liftover Height	798 (31.4) 	
Maximum Cargo Width at Liftgate Opening	1,491 (58.7) 	
Minimum Cargo Width at Liftgate Opening	1,047 (41.2) 	
Maximum Cargo Height at Liftgate Opening	942 (37.1) 	
Minimum Cargo Height at Liftgate Opening	940 (37.0) 	
Distance between Wheelhouse Interior Trim	1,135 (44.7) 	
SAE Cargo Volume		
Rear Seat Folded, litres (cu. ft.)	1,999 (70.6)	
Rear Seat Upright, litres (cu. ft.)	892 (31.5)	
Total Passenger plus Cargo Volume, litres (cu. ft.)	4,259 (150.4)	
		
WHEELS		
Availability	Standard — Wrangler Unlimited Sport S	
Type and Material	Polished aluminum 	
Size	17 x 7.5 inch	
		
Availability	Standard — Wrangler Unlimited Willys Wheeler	
Type and Material	High-Gloss Black painted aluminum	
Size	17 x 7.5 inch	
	
Availability		Standard — Wrangler Unlimited Sahara 		
Type and Material	Painted and polished cast-aluminum	
Size	18 x 7.5 inch	
		
Availability	Standard — Wrangler Unlimited Rubicon 	
Type and Material	Painted and polished cast-aluminum	
Size	17 x 7.5 inch	
		
TIRES		
Availability	Standard — Wrangler Unlimited Sport S	
Size and Type 	P225/75R17, on/off-road, OWL	
Mfr. and Model	Goodyear 	
		
Availability	Standard — Wrangler Unlimited Sahara	
Size and Type	P255/70R18, on/off-road, OWL	
Mfr. and Model	Bridgestone Dueler 693	
		
Availability	Standard — Wrangler Unlimited Willys Wheeler and Rubicon	
Size and Type	LT255/75R17, on/off-road, black sidewall BSW	
Mfr. and Model 	BF Goodrich Mud Terrain 	
		
Availability	Standard — Wrangler Unlimited Rubicon	
Size and Type	LT255/75R17, on/off-road, black sidewall	
Mfr. and Model	BF Goodrich Mud Terrain	
		
Parking Brake Type	Drum-in-hat	
Power-assist Type		
Four–wheel Anti-lock Brakes 	Standard	
Electronic Stability Control 	Standard	
All-speed Traction Control 	Standard	

Towing Capacities (kg. lb)	
WRANGLER UNLIMITED SPORT 4WD 	
Engine	Trans
Type	Transmission	Axle
Ratio	Payload	Base Wt.	Base Wt.
Front	Base Wt.
Rear	GAWR
Front	GAWR
Rear	GCWR	Max 
Trailer	
3.6-litre V6 gas (EGT) 	M6	NSG370 6-speed  Manual (DEH)	3.21	453.5 (1,000)	453.5 (4,277)	1,015.4 (2,238)	984.8 (2,039)	1,258 (2,775)	1,451.4 (3,200)	2,915.2 (6,427)	907.1 (2,000)	
3.6-litre V6 gas (EGT)	M6	NSG370 6-speed  Manual (DEH)	3.73	453.5 (1,000)	453.5 (4,277)	1015.1 (2,238)	984.8 (2,039)	1,258 (2,775)	1,451.4 (3,200)	3,595.6 (7,927)	1,587.5 (3,500)	
3.6-litre V6 gas (EGT)	A5	WA580 5-speed Automatic (DGL)	3.21	453.5 (1,000)	2,232.1 (4,921)	1014.6 (2,237)	931.6 (2,054)	1,258 (2,775)	1,451.4 (3,200)	2921.5
(6,441)	907.1 (2,000)	
3.6-litre V6 gas (EGT)	A5	WA580 5-speed Automatic (DGL)	3.73	453.5 (1,000)	2,232.1 (4,291)	1014.6 (2,237)	931.6 (2,054)	1,258 (2,775)	1,451.4 (3,200)	3,601.9 (7,941)	1,587 (3,500)	
1. GCWR = Base Weight + Maximum Trailer Weight + 68 kg / 150 lb for driver.	
WRANGLER UNLIMITED SAHARA 4WD	
Engine	Trans
Type	Transmission	Axle
Ratio	Payload	Base Wt.	Base Wt.
Front	Base Wt.
Rear	GAWR
Front	GAWR
Rear	GCWR	Max 
Trailer	
3.6-litre V6 gas (EGT) 	M6	NSG370 6-speed Manual (DEH)	3.21	399.1 (880)	1,994.4 (4,397)	1031.0  (2,273)	963.4 (2,124)	1,258.7 (2,775)	1,451.4 (3,200)	2,969.6 (6,547(	9.07.1 (2,000)	
3.6-litre V6 gas (EGT)	M6	NSG370 6-speed Manual (DEH)	3.73	399.1 (880)	1,994.4 (4,397)	1031.0
(2,273)	963.4 (2,124)	1,258.7 (2,775)	1,451.4 (3,200)	3650.0 (8,047)	1,587.5 (3,500)	
3.6-litre V6 gas (EGT)	A5	WA580 5-speed Automatic (DGL)	3.21	399.1 (880)	2,000.7 (4,411)	1030.5
(2,272)	970.2 (2,139)	1,258.7 (2,775)	1,451.4 (3,200)	2976.0 (6,561)	907.1 (2,000)	
3.6-litre V6 gas (EGT)	A5	WA580 5-speed Automatic (DGL)	3.73	399.1 (880)	2,000.7 (4,411)	1030.5 (2,272)	970.2 (2,139)	1,258.7(2,775)	1,451.4 (3,200)	3,656.4 (8,061)	1,587.5 (3,500)	
1. GCWR = Base Weight + Maximum Trailer Weight + 68 kg / 150 lb for driver.	
	
WRANGLER UNLIMITED RUBICON 4WD	
Engine	Trans
Type	Transmission	Axle
Ratio	Payload	Base Wt.	Base Wt.
Front	Base Wt.
Rear	GAWR
Front	GAWR
Rear	GCWR	Max 
Trailer	
3.6-litre V6 gas (EGT)	M6	NSG370 6-speed  Manual (DEH)	4.10	404.6 (892)	2,050.6 (4,521)	1,066.8 (2,352)	984.2 (2,170)	1,258.7(2,775)	1,451.4 (3,200)	3,706.3 (8,171)	1,587.5 (3,500)	
3.6-litre V6 gas (EGT)	A5	WA580 5-speed Automatic (DGV)	3.73	404.6 (892)	2,057.0
(4,535)	1,065.9 (2,350)	991.0 (2,185)	1,258.7 (2,775)	1,451.4 (3,200)	3,712.6 (8,185)	1,587.5 (3,500)	
3.6-litre V6 gas (EGT)	A5	WA580 5-speed Automatic (DGV)	4.10	404.6 (892)	2,057.0 (4,535)	1,065.9 (2,350)	991.0
(2,185)	1,258.7 (2,775)	1,451.4 (3,200)	3,712.6 (8,185)	1,587.5 (3,500)	
1.	GCWR = Base Weight + Maximum Trailer Weight + 68 kg / 150 lb for driver.