FCA CANADA
2017 Ram 1500
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION		
Vehicle Type	Regular Cab, Quad Cab and Crew Cab, 2WD, 4WD	
Assembly Plant	Regular Cab: Saltillo, Coahuila, Mexico
Quad Cab: Warren, Michigan
Crew Cab: Warren, Michigan and Saltillo, Coahuila, Mexico	
EPA Vehicle Class	Standard Pickup	
		
BODY/CHASSIS		
Layout	2WD — Longitudinal, front engine
4WD — Longitudinal, front engine, transfer case	
Construction	2WD — Ladder-type frame, steel cab, double-wall steel pickup box
4WD — Ladder-type frame, steel cab, double-wall steel pickup box	
		
ENGINE: 3.6-LITRE PENTASTAR V6	
Type and Description	60-degree V-type, liquid-cooled	
Displacement	3,604 cu. cm (220 cu. in.) 	
Bore x Stroke	96 x 83 (3.78 x 3.27) 	
Valve System	Chain-driven DOHC, 24 valves and hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Aluminum deep-skirt block, aluminum alloy heads	
Compression Ratio	10.2:1	
Power 	305 hp (224 kW) at 6,400 rpm	
Torque 	269 lb.-ft. (364 N•m) at 4,175 rpm	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2, E85-compatible	
Oil Capacity	5.7 litres (6.0 quarts) 	
Coolant Capacity	13.25 litres (14.0 quarts) 	
Emission Controls	Dual three-way catalytic converters, heated oxygen sensors	

EnerGuide (2016) Fuel Consumption 
Ratings L/100 km (MPG – imperial gallon) city/hwy	13.9/9.5 (20/30) – 4x2 models
14.6/10.1 (19/28) – 4x4 models	
Based on 2016 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information, please visit the Government of Canada website: www.vehicles.nrcan.gc.ca	
	
ENGINE: 3.0-LITRE ECODIESEL V6	
Type and Description	60-degree V-type, liquid-cooled	
Displacement	2,999 cu. cm (182 cu. in.) 	
Bore x Stroke	83 x 92 (3.27 x 3.60)	
Valve System	Chain-driven DOHC, 24 valves	
Fuel Injection	Common-rail, 2,000 bar, solenoid injectors	
Construction	Cast-iron block, aluminum alloy heads	
Compression Ratio	16.5:1	
Power 	240 hp (179 kW) at 3,600 rpm	
Torque 	420 lb.-ft. (569 N•m) at 2,000 rpm	
Max. Engine Speed	4,800 rpm (electronically limited)	
Fuel Requirement	Ultra-low sulfur diesel	
Oil Capacity	10 litres (10.5 quarts) 	
Coolant Capacity	11.4 litres (12 quarts) 	
Emission Controls	Cooled EGR, oxidation catalyst, diesel particulate filter, SCR w/urea injection	
EnerGuide (2016) Fuel Consumption Ratings L/100 km (MPG – imperial gallon) city/hwy	11.3/8.0 (25/35) – 4x2 HFE models
11.6/8.4 (24/34) – 4x2 non-HFE models
12.1/8.8 (23/32) – 4x4 models 	
		
ENGINE: 5.7-LITRE HEMI® V8		
Type and Description	90-degree V8, liquid-cooled	
Displacement	5,654 cu. cm (345 cu. in.) 	
Bore x Stroke	99.5 x 90.9 (3.92 x 3.58) 	
Valve System	Variable-cam timing, pushrod-operated overhead valves, 16 valves, hydraulic lifters with roller followers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps, aluminum alloy heads with hemispherical combustion chambers	
Compression Ratio	10.5:1	
Power 	395 hp (291 kW) @ 5,600 rpm	
Torque 	410 lb.-ft. (556 N•m) @ 3,950 rpm	
Max. Engine Speed	5,800 rpm	
Fuel Requirement	Unleaded mid-grade, 89 octane (R+M)/2 — recommended 
Unleaded regular, 87 octane (R+M)/2 — acceptable	
Oil Capacity	6.6 litres (7.0 quarts) 	
Coolant Capacity	13.3 litres (14.0 quarts) 	
Emission Controls	Three-way catalytic converters, heated oxygen sensors  and internal engine features	
EnerGuide (2016) Fuel Consumption Ratings L/100 km (MPG – imperial gallon) city/hwy	15.8 (18) / 10.9 (26) ― 4x2 models
16.2 (17) / 11.5 (25) ― 4x4 models 	
EnerGuide (2016) Fuel Consumption Ratings L/100 km (MPG – imperial gallon) city/hwy	17.1 (17) / 12.0 (24) ― 4x2 models
17.7 (16) / 12.7 (22) ― 4x4 models 	
	
TRANSMISSION: 65RFE AUTOMATIC SIX-SPEED	
Availability	Available with 5.7-litre HEMI V8 equipped trucks	
Description	Three planetary gear sets, one overrunning clutch, full electronic control, electronically controlled converter clutch	
Gear Ratios		
1st	3.00	
2nd	1.67 	
3rd   	1.50	
4th	1.00	
5th	0.75	
6th	0.67	
Reverse	3.00	
Axle Gear Ratios	3.21, 3.55, 3.92, 	
	
TRANSMISSION: TORQUEFLITE 845RE EIGHT-SPEED AUTOMATIC 	
Availability	Standard with 3.6-litre Pentastar V6	
Description	Adaptive electronic control, automatic or Electronic Range Select (ERS) manual control. Five clutch-pack design with only two open clutches in any gear. Torque converter lock with turbine torsional damper for low lock-up speeds in 1st through 
8th gear	
Gear Ratios		
1st	4.71	
2nd 	3.14	
3rd 	2.10	
4th 	1.67	
5th 	1.29	
6th 	1.00	
7th 	0.84	
8th 	0.67	
Reverse 	3.30	
Axle Gear Ratios	3.21, 3.55, 3.92 (Rebel only)	
	
TRANSMISSION: TORQUEFLITE 8HP70 EIGHT-SPEED AUTOMATIC	
Availability	Standard with 3.0-litre EcoDiesel V6 and select 5.7-litre HEMI V8 equipped trucks	
Description	Adaptive electronic control, automatic or ERS manual control. Five clutch-pack design with only two open clutches in any gear. Torque converter lock with turbine torsional damper for low lock-up speeds in 1st through 8th gear	
Gear Ratios		
1st	4.71	
2nd	3.14	
3rd	2.10	
4th	1.67	
5th	1.29	
6th	1.00	
7th	0.84	
8th	0.67	
Reverse	3.30	
Axle Gear Ratios	3.21 (excluding 3.0-litre EcoDiesel V6), 3.55 (excluding 5.7-litre HEMI V8), 3.92	
		
TRANSFER CASE: BW 44-45 PART-TIME	
Availability	3.0-litre EcoDiesel V6  4x4, 3.6-litre Pentastar V6 4x4 and 5.7-litre HEMI V8 4x4	
Shift Mechanism	Electric	
Available Speeds	Two-speed	
Operating Modes	2WD High; 4WD High, Locked; Neutral; 4WD Low, Locked	
Low-range Ratio	2.64	
Center Differential Type	None	
		
TRANSFER CASE: BW 44-44 ON-DEMAND	
Availability	3.0-litre EcoDiesel V6 4x4, 3.6-litre Pentastar V6 4x4  and 5.7-litre HEMI V8 4x4	
Shift Mechanism	Electric	
Available Speeds	Two-speed	
Operating Modes	2WD High; 4WD Auto; 4WD High, Locked; Neutral; 4WD Low, Locked	
Low-range Ratio	2.64	
Center Differential Type	None	
		
AXLES		
Front	ZF 215 mm	
Rear	C235 mm (available limited slip)	
Available Ratios	3.21, 3.55, 3.92	
		
ELECTRICAL SYSTEM		
Architecture	Powernet	
Alternator	160-amp, 180-amp, 220-amp (Stop-start system and Special Services Package) 
230-amp (3.0-liter EcoDiesel V6)	
Battery	Group 65, low-maintenance 730 CCA (Stop-start features 800 CCA absorbed glass mat)	
		
SUSPENSION		
Front	Upper and lower A-arms, coil springs, twin-tube shock absorbers, stabilizer bar. Optional air suspension replaces twin-tube shock absorbers and coil springs. Rebel features Bilstein monotube shocks with air suspension	
Rear	Five-link with track bar, coil springs, stabilizer bar, twin-tube shock absorbers, solid axle. Optional air suspension replaces twin-tube shock absorbers and coil springs. Rebel features Bilstein monotube shocks with air suspension	
		
BRAKES		
Front		
Size and Type	336 x 28 (13.2 x 1.1) vented disc with 54 (2.13) 
Two-piston pin-slider caliper and anti-lock braking system (ABS)	
Swept Area	1,884 sq. cm (292 sq. in.) 	
Rear		
Size and Type	352 x 22 (13.8 x 0.87) disc with 54 (2.13) 
Single-piston pin-slider caliper and ABS	
Swept Area	1,768 sq. cm (274 sq. in.) 	
Power-assist		Dual-rate, tandem diaphragm vacuum	
AIR BAGS	
Regular Cab	6	
Quad Cab	6	
Crew Cab	6	

STEERING					
Power-assist					
Regular Cab	2WD	2WD	4WD	4WD	
Box Length	6-ft. 4-in.	8-ft.	6-ft. 4-in.	8-ft.	
Wheelbase (nominal)	3,061 (120.5) 	3,569.2 (140.5) 	3,061 (120.)5 	3,569.2 (140.5)	
Overall Steering Ratio 	19.1:1	17.9:1	19.1:1	17.9:1	
Steering Wheel Turns (lock-to-lock)	3.5	3.3	3.5	3.3	
Turning Diameter – 17-in. Tire -m (ft.)	12.0 (39.5) 	13.7 (45.1) 	12.1 (39.8) 	13.8 (45.4) 	
Turning Diameter – 20-in. Tire - m (ft.) 	12.0 (39.3) 	13.7 (44.9) 	12.1 (39.8) 	13.9 (45.5) 	
					
Quad Cab	2WD		4WD		
Box Length	6-ft. 4-in.		6-ft. 4-in.		
Wheelbase (nominal)	3,569.2 (140.5) 		3,569.2 (140.5) 		
Overall Steering Ratio 	17.9:1		17.9:1		
Steering Wheel Turns (lock-to-lock)	3.3		3.3		
Turning Diameter – 17-in. Tire – m (ft.)	13.7 (45.1) 		13.8 (45.4) 		
Turning Diameter – 20-in. Tire – m (ft.)	13.7 (44.9) 		13.9 (45.5) 		
					
Crew Cab	2WD	2WD	4WD	4WD	
Box Length	5-ft. 7-in.	6-ft. 4-in.	5-ft. 7-in.	6-ft. 4-in.	
Wheelbase (nominal) 	3,569.2 (140.5) 	3,797.3 (149.5) 	3,569.2 (140.5)	3,797.3 (149.5) 	
Overall Steering Ratio 	19.1:1	17.9:1	19.1:1	17.9:1	
Steering Wheel Turns (lock-to-lock)	3.5	3.3	3.5	3.3	
Turning Diameter – 17-in. Tire -m (ft.)	12.0 (39.5) 	13.7 (45.1) 	12.1 (39.8) 	13.8 (45.4) 	
Turning Diameter – 20-in. Tire – m (ft.) 	12.0 (39.3) 	13.7 (44.9) 	12.1 (39.8) 	13.9 (45.5) 	

DIMENSIONS AND CAPACITIES				
Cargo Box				
Nominal Box Size 	5-ft. 7-in. (Crew)	6-ft. 4-in. (Regular, Quad or Crew)	8-ft. (Regular)	
SAE volume, litres (cu. ft.)  	1,424 (50.3) 	1,628 (57.5) 	2,115 (74.7) 	
Length at Floor, Tailgate Closed	1,712.4 (67.4) 	1,938.5 (76.3)	2,496.5 (98.3)	
Cargo Width	1,686.9 (66.4) 	1,686.9 (66.4)	1,686.9 (66.4)	
Distance Between Wheelhouses	1,295.4 (51) 	1,295.4 (51)	1,295.4 (51)	
Depth  	508.6 (20.0) 	511.1 (20.1) 	513.0 (20.2) 	
Tailgate Opening Width	1,535.3 (60.4) 	1,535.3 (60.4) 	1,535.3 (60.4)	

Regular Cab Pickup					
Model – Tire Size 	2WD –265/70R17	4WD –265/70R17	
Box Length 	6-ft. 4-in.	8-ft.	6-ft. 4-in.	8-ft.	
Wheelbase (nominal) 	3,061.2 (120.5) 	3,569.2 (140.5) 	3,062.5 (120.5) 	3,570.2 (140.5) 	
Track, Front 	1,728.2 (68.0) 	1,728.2 (68.0) 	1,732.3 (68.2) 	1,732.3 (68.2) 	
Track, Rear 	1,714.7 (67.5) 	1,714.7 (67.5)	1,714.7 (67.5) 	1,714.7 (67.5) 	
Overall Length 	5,308.5 (209.0) 	5,866.5 (231.0) 	5,308.5 (209.0) 	5,866.5 (231.0) 	
Overall Width 	2,017.4 (79.4) 	2,017.4 (79.4)	2,017.4 (79.4) 	2,017.4 (79.4) 	
Overall Height 	1,894.2 (74.6)	1,889.2 (74.4) 	1,910.4 (75.2) 	1,906 (75.0) 	
Ground Clearance					
Front Axle 	229.3 (9.0) 	229.2 (9.0) 	232.6 (9.2) (232.6)	232.7 (9.2) 	
Rear Axle 	221.2 (8.7) 	221.5 (8.7) 	219.2 (8.6) (219.2)	219.5 (8.6) 	
Open Tailgate to Ground 	883.4 (34.8) 	878.3 (34.6) 	889.6 (35.0) (889.6)	885.3 (34.9) 	
Pickup Body Height 	511.1 (20.1) 	513.0 (20.2) 	511.1 (20.1) (511.1)	513.0 (20.2) 	
Approach Angle (degrees) 	15.6	15.7	17.7	17.8	
Departure Angle (degrees)	25.2	24.1	25.6	24.4	
Box Length 	6-ft. 4-in.	8-ft.	6-ft. 4-in.	8-ft.	
Ramp Breakover Angle (degrees) 	21.5	19.2	22.9	20.5	
Fuel-Tank Capacity 	98 litres (26 gal.) (standard)	121 litres (32 gal.)  (standard)	98 litres (26 gal.) (standard)	121 litres (32 gal.)  (standard)	

Quad Cab 6-ft. 4-in. Box Pickup			
Model – Tire Size 	2WD –265/70R17	4WD –265/70R17	
Box Length	6-ft. 4-in. 	6-ft. 4-in. 	
Wheelbase (nominal)	3,569.2 (140.5) 	3,570 (140.5) 	
Track, Front 	1,728.2 (68.0) 	1,732.3 (68.2) 	
Track, Rear 	1,714.7 (67.5) 	1,714.7 (67.5) 	
Overall Length 	5,816.5 (229.0) 	5,816.5 (229.0) 	
Overall Width 	2,017.4 (79.4) 	2,017.4 (79.4) 	
Overall Height 	1,960.2 (77.2) 	1,974.8 (77.7) 	
Box Length 	6-ft. 4-in.	6-ft. 4-in.	
Ground Clearance			
Front Axle 	248.5 (9.8) 	248.5 (9.8)	
Rear Axle 	235.0 (9.3) 	235.0 (9.3)	
Open Tailgate to Ground 	847.2 (33.4) )	904.1 (35.6) 	
Pickup Body Height 	508.6 (20.0) )	508.6 (20.0)	
Approach Angle (degrees) 	16.6	22.9	
Departure Angle (degrees)	19.4	22.2	
Ramp Breakover Angle without Skid Plate	17.1	22.5	
Ramp Breakover Angle with Skid Plate	13.8	18.7	
Ground Clearance without Skid Plate	187.2 (7.4) 	269.5 (10.6) 	
Ground Clearance with Skid Plate	169.3 (6.7) 	252.8 (9.9) 	
Fuel-Tank Capacity	98 litres  (standard)	98 litres (standard)	
	121 litres (optional)	121 litres (optional)	

Quad Cab 6-ft. 4-in. Box Pickup - Air Suspension 4x2 and 4x4	
Tire Size 	265/70R17	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal)  	3,569.4 (140.5)	3,569.4 (140.5))	3,569.4 (140.5)	3,569.4 (140.5)	
Track, Front 	1,728.2 (68.0) 	1,728.2 (68.0)	1,728.2 (68.0)	1,728.2 (68.0)	
Track, Rear 	1,714.7 (67.5) 	1,714.7 (67.5)	1,714.7 (67.5)	1,714.7 (67.5)	
Overall Length 	5,816.5 (229.0) 	5,816.5 (229.0)	5,816.5 (229.0)	5,816.5 (229.0)	
Overall Width 	2,017.4 (79.4) 	2,017.4 (79.4)	2,017.4 (79.4)	2,017.4 (79.4)	
Overall Height 	1,909.0 (75.2) 	1,962.0 (77.2) 	1,986.6 (78.2) 	2,013.0 (79.2) 	

Ground Clearance					
Front Axle 	232.3 (9.1) 	232.3 (9.1)	232.3 (9.1)	232.3 (9.1)	
Rear Axle 	220.0 (8.7) 	220.0 (8.7)	220.0 (8.7)	220.0 (8.7)	
Open Tailgate to Ground 	832.8 (32.8) 	871.2 (34.3) 	889.6 (35.0) 	922.2 (36.3) 	
Pickup Body Height 	508.6 (20.0) 	508.6 (20.0)	508.6 (20.0)	508.6 (20.0)	
Approach Angle (degrees) 	13.8	18.3	20.9	22.5	
Departure Angle (degrees)	23.0	24.8	25.6	27.1	
Ramp Breakover Angle (degrees) 	15.9	19.4	21.4	23.0	
Ground Clearance without Skid Plate	171.0 (6.7) 	223.5 (8.8) 	254 (10.0) 	274.3 (10.8) 	
Ground Clearance with Skid Plate	153.1 (6.0) 	205.7 (8.1) 	236.2 (9.3) 	256.5 (10.1) 	
Fuel-Tank Capacity 	98 litres  (standard)	98 litres (standard)	98 litres (standard)	98 litres (standard)	
	121 litres  (optional)	121 litres (optional)	121 litres (optional)	121 litres (optional)	

Quad Cab 6-ft. 4-in. Box Pickup - Air Suspension 4x2 and 4x4	
Tire Size 	275/60R20	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal)  	3,569.4 (140.5) 	3,569.4 (140.5)	3,569.4 (140.5)	3,569.4 (140.5)	
Track, Front 	1,742.2 (68.6) 	1,742.2 (68.6)	1,742.2 (68.6)	1,742.2 (68.6)	
Track, Rear 	1,727.4 (68.0)	1,727.4 (68.0)	1,727.4 (68.0)	1,727.4 (68.0)	
Overall Length 	5,816.5 (229.0) 	5,816.5 (229.0)	5,816.5 (229.0)	5,816.5 (229.0)	
Overall Width 	2,017.4 (79.4) 	79.4 (2,017.4) 2,017.4 (79.4)	2,017.4 (79.4)	2,017.4 (79.4)	
Overall Height 	1,924.4 (75.8)	1977.4 (77.8) 	2002.0 (78.8) 	2,028.4 (79.9) 	
Ground Clearance					
Front Axle 	248.5 (9.8) 	248.5 (9.8)	248.5 (9.8)	248.5 (9.8)	
Rear Axle 	235.0 (9.3) 	235.0 (9.3)	235.0 (9.3)	235.0 (9.3)	
Open Tailgate to Ground 	847.2 (33.4) 	885.7 (34.9) 	904.1 (35.6) 	936.7 (36.9) 	
Pickup Body Height 	508.6 (20.0) 	508.6 (20.0)	508.6 (20.0)	508.6 (20.0)	
Approach Angle (degrees) 	15.2	19.8	22.4	23.9	
Departure Angle (degrees)	23.7	25.5	26.4	27.8	
Ramp Breakover Angle (degrees) 	17.1	20.6	22.5	24.2	
					
Quad Cab 6-ft. 4-in. Box Pickup - Air Suspension 4x2 and 4x4 (continued)	
Tire Size 	275/60R20	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Ground Clearance without Skid Plate	187.2 (7.4) 	239.8 (9.4) 	269.5 (10.6) 	290.8 (11.4) 	
Ground Clearance with Skid Plate	169.3 (6.7) 	222.8 (8.8) 	252.8 (9.9) 	273.7 (10.8) 	
Fuel-Tank Capacity 	98 litres (standard)	98 litres (standard)	98 litres (standard)	98 litres (standard)	
	121 litres (optional)	121 litres (optional)	121 litres (optional)	121 litres (optional)	

Crew Cab Pickup					
Model – Tire Size 	2WD –265/70R17	4WD –265/70R17	
Box Length 	5-ft. 7-in.	6-ft. 4-in.	5-ft. 7-in.	6-ft. 4-in.	
Wheelbase (nominal) 	3,569.2 (140.5) 	3,795.3 (149.4) (3,795.3)	3,570.2 (140.5) (3,570.2)	3,795.2 (149.4) (3,795.2)	
Track, Front 	1,728.2 (68.0) (1,728.2)	1,728.2 (68.0)	1,732,3 (68.2) 	1,732.3 (68.2) 	
Track, Rear 	1,714,7 (67.5) 	1,714,7 (67.5)	1,714,7 (67.5)	1,714,7 (67.5)	
Overall Length 	5,816.5 (229.0) 	6,042.6 (237.9) 	5,816.5 (229.0) 	6,042.6 (237.9) 	
Overall Width 	2,017.4 (79.4) 	2,016.6 (79.4) 	2,017.4 (79.4) 	2,016.6 (79.4)	
Overall Height 	1,953.8 (76.9) 	1,950.6 (76.8) 	1,967.9 (77.5) 	1,965.1 (77.4) 	
Ground Clearance					
Front Axle 	229.2 (9.0) 	231.1 (9.1) 	232.7 (9.2) 	235.2 (9.2) 	
Rear Axle 	221.5 (8.7) 	220.5 (8.7) 	219.5 (8.6) 	218.3 (8.6) 	
Open Tailgate to Ground 	878.3 (34.6) 	874.0 (34.4) 	885.3 (34.9) 	880.8 (34.7) 	
Box Length	5-ft. 7-in.	6-ft. 4-in.	5-ft. 7-in.	6-ft. 4-in.	
Pickup Body Height 	508.6 (20.0) 	511.1 (20.1) 	508.6 (20.0) 	511.1 (20.1) 	
Approach Angle (degrees) 	15.7	16.0	17.8	18.0	
Departure Angle (degrees)	25.1	24.9	24.7	25.2	
Ramp Breakover Angle (degrees) 	19.2	18.5	20.5	19.7	
Fuel-Tank Capacity 	98 litres  (standard)	98 litres (standard)	98 litres (standard)	98 litres (standard)	
	121 litres (optional)	121 litres (optional)	121 lites (optional)	121 litres (optional)	

Crew Cab 5-ft. 7-in. Box Pickup - Air Suspension 4x2 and 4x4	
Tire Size 	265/70R17	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal)  	3,569.4 (140.5) 	3,569.4 (140.5)	3,569.4 (140.5)	3,569.4 (140.5)	
Track, Front 	1,728.2 (68.0) (1,728.2)	1,728.2 (68.0)	1,728.2 (68.0)	1,728.2 (68.0)	
Track, Rear 	1,714.7 (67.5) 	1,714.7 (67.5)	1,714.7 (67.5)	1,714.7 (67.5)	
Overall Length 	5,816.5 (229.0) 	5,816.5 (229.0)	5,816.5 (229.0)	5,816.5 (229.0)	
Overall Width 	2,017.4 (79.4) 	2,017.4 (79.4)	2,017.4 (79.4)	2,017.4 (79.4)	
Overall Height 	1,902.1 (74.9) 	1,955.1 (77.0) 	1,979.2 (77.9) 	2,006.1 (79.0) 	
Ground Clearance					
Front Axle 	232.3 (9.1) 	232.3 (9.1)	232.3 (9.1)	232.3 (9.1)	
Rear Axle 	220.0 (8.7) 	220.0 (8.7)	220.0 (8.7)	220.0 (8.7)	
Open Tailgate to Ground 	832.8 (32.8) (832.8)	871.2 (34.3) (871.2)	889.6 (35.0) 	922.2 (36.3) 	
Pickup Body Height 	508.6 (20.0) 	508.6 (20.0)	508.6 (20.0)	508.6 (20.0)	
Approach Angle (degrees) 	13.8	18.3	20.9	22.5	
Departure Angle (degrees)	23.0	24.8	25.6	27.1	
Ramp Breakover Angle (degrees) 	15.9	19.4	21.4	23.0	
Ground Clearance without Skid Plate	171.0 (6.7) 	223.5 (8.8) 	254.0 (10.0) 	274.3 (10.8) 	
Ground Clearance with Skid Plate	153.1 (6.0) 	205.7 (8.1) 	236.2 (9.3) 	256.5 (10.1) 	
Fuel-Tank Capacity	98 litres (standard)	98 litres (standard)	98 litres (standard)	98 litres (standard)	
	121 litres (optional)	121 litres (optional)	121 litres (optional)	121 litres (optional)	

Crew Cab 5-ft. 7-in. Box Pickup - Air Suspension 4x2 and 4x4	
Tire Size 	275/60R20	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal) 	3,569.4 (140.5) 	3,569.4 (140.5)	3,569.4 (140.5)	3,569.4 (140.5)	
Track, Front 	1,742.2 (68.6) 	1,742.2 (68.6)	1,742.2 (68.6)	1,742.2 (68.6)	
Track, Rear 	1,727.4 (68.0) 	1,727.4 (68.0)	1,727.4 (68.0)	1,727.4 (68.0)	
Overall Length 	5,816.5 (229.0) 	5,816.5 (229.0)	5,816.5 (229.0)	5,816.5 (229.0)	
Overall Width 	2,017.4 (79.4) 	2,017.4 (79.4)	2,017.4 (79.4)	2,017.4 (79.4)	
Overall Height 	1,917.4 (75.5) 	1,970.4 (77.6) 	1,994.5 (78.5) 	2,021.4 (79.6) 	
Ground Clearance					
Front Axle 	248.5 (9.8) 	248.5 (9.8)	248.5 (9.8)	248.5 (9.8)	
Rear Axle 	235.0 (9.3) 	235.0 (9.3)	235.0 (9.3)	235.0 (9.3)	
Open Tailgate to Ground 	847.2 (33.4) 	885.7 (34.9) 	904.1 (35.6) 	936.7 (36.9) 	
Pickup Body Height 	508.6 (20.0) 	508.6 (20.0)	508.6 (20.0)	508.6 (20.0)	
Approach Angle (degrees) 	15.2	19.8	22.4	23.9	
Departure Angle (degrees)	23.7	25.5	26.4	27.8	
Ramp Breakover Angle (degrees) 	17.1	20.6	22.5	24.2	
Ground Clearance without Skid Plate	187.2 (7.4) 	239.8 (9.4) 	269.5 (10.6) 	290.8 (11.4) 	
Ground Clearance with Skid Plate	169.3 (6.7) 	222.8 (8.8) 	252.8 (9.9) 	273.7 (10.8) 	
Fuel-Tank Capacity 	98 litres (standard)	98 litres (standard)	98 litres (standard)	98 litres (standard)	
	121 litres (optional)	121 litres (optional)	121 litres (optional)	121 litres (optional)	

Crew Cab 6-ft. 4-in. Box Pickup - Air Suspension 4x2 and 4x4	
Tire Size 	265/70R17	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal)  	3,798.0 (149.5) )	3,798.0 (149.5)	3,798.0 (149.5)	3,798.0 (149.5)	
Track, Front 	1,728.2 (68.0) 	1,728.2 (68.0)	1,728.2 (68.0)	1,728.2 (68.0)	
Track, Rear 	1,714.7 (67.5) 	1,714.7 (67.5)	1,714.7 (67.5)	1,714.7 (67.5)	
Overall Length 	6,042.6 (237.9) )	6,042.6 (237.9)	6,042.6 (237.9)	6,042.6 (237.9)	
Overall Width 	2,017.4 (79.4)	2,017.4 (79.4)	2,017.4 (79.4)	2,017.4 (79.4)	
Overall Height 	1,897.7 (74.7)	1,950.7 (76.8) 	1,975.2 (77.8) 	2,001.7 (78.8) 	
Ground Clearance	
Front Axle 	231.6 (9.1) 	231.6 (9.1)	231.6 (9.1)	231.6 (9.1)	
Rear Axle 	217.7 (8.6) 	217.7 (8.6)	217.7 (8.6)	217.7 (8.6)	
Open Tailgate to Ground 	827.9 (32.6) 	866.6 (34.1) 	885.2 (34.8) 	917.6 (36.1) 	
Pickup Body Height 	511.1 (20.1) 	511.1 (20.1)	511.1 (20.1)	511.1 (20.1)	
Approach Angle (degrees) 	13.8	18.3	20.9	22.5	
Departure Angle (degrees)	22.8	24.6	25.5	26.9	
Ramp Breakover Angle (degrees) 	15.3	18.7	20.5	22.2	
Ground Clearance without Skid Plate	170.0 (6.7) 	222.7 (8.8) 	252.4 (9.9) 	273.7 (10.8) 	
Ground Clearance with Skid Plate	152.3 (6.0) 	205.4 (8.1) 	235.4 (9.3) 	256.4 (10.1) 	
Fuel-Tank Capacity 	98 litres (standard)	98 litres (standard)	98 litres (standard)	98 litres (standard)	
	121 litres (optional)	121 litres (optional)	121 litres (optional)	121 litres (optional)	

Crew Cab 6-ft. 4-in. Box Pickup - Air Suspension 4x2 and 4x4 	
Tire Size 	275/60R20	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal)  	3,798.0 (149.5) 	3,798.0 (149.5)	3,798.0 (149.5)	3,798.0 (149.5)	
Track, Front 	1,742.2 (68.6) 	1,742.2 (68.6)	1,742.2 (68.6)	1,742.2 (68.6)	
Track, Rear 	1,727.4 (68.0) 	1,727.4 (68.0)	1,727.4 (68.0)	1,727.4 (68.0)	
Overall Length 	6,042.6 (237.9) 	6,042.6 (237.9)	6,042.6 (237.9)	6,042.6 (237.9)	
Overall Width 	2,017.4 (79.4) 	2,017.4 (79.4)	2,017.4 (79.4)	2,017.4 (79.4)	

Crew Cab 6-ft. 4-in. Box Pickup - Air Suspension 4x2 and 4x4 (continued)	
Tire Size 	275/60R20	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Overall Height 	1,914.5 (75.4) 	1,967.5 (77.5) 	1,991.9 (78.4) 	2,018.5 (79.5) 	
Ground Clearance	
Front Axle 	247.9 (9.8) 	247.9 (9.8)	247.9 (9.8)	247.9 (9.8)	
Rear Axle 	234.7 (9.2) 	234.7 (9.2)	234.7 (9.2)	234.7 (9.2)	
Open Tailgate to Ground 	819.5 (32.3) 	883.9 (34.8) 	902.5 (35.5) 	934.9 (36.8) 	
Pickup Body Height 	511.1 (20.1) 	511.1 (20.1)	511.1 (20.1)	511.1 (20.1)	
Approach Angle (degrees) 	15.5	19.7	22.3	23.9	
Departure Angle (degrees)	22.5	25.5	26.4	27.8	
Ramp Breakover Angle (degrees) 	16.4	19.8	21.7	23.3	
Ground Clearance without Skid Plate	185.8 (7.3) 	239.0 (9.4) 	268.7 (10.6) 	290.0 (11.4) 	
Ground Clearance with Skid Plate	168.8 (6.6) 	221.7 (8.7) 	251.7 (9.9) 	272.7 (10.7) 	
Fuel-Tank Capacity 	98 litres (standard)	98 litres (standard)	98 litres (standard)	98 litres (standard)	
	121 litres (optional)	121 litres (optional)	121 litres (optional)	121 litres (optional)	

Crew Cab 5-ft. 7-in. Box Pickup - Air Suspension 4x4 Rebel	
Tire Size	285/70R17	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 	
Wheelbase (nominal) 	3,569.4 (140.5) 	3,569.4 (140.5)	3,569.4 (140.5)	
Track, Front 	1,743.2 (68.6) 	1,743.2 (68.6)	1,743.2 (68.6)	
Track, Rear 	1,727.4 (68.0) 	1,727.4 (68.0)	1,727.4 (68.0)	
Overall Length 	5,816.5 (229.0) 	5,816.5 (229.0)	5,816.5 (229.0)	
Overall Width 	2,070.8 (81.5) 	2,070.8 (81.5)	2,070.8 (81.5)	
Overall Height	1,913.7 (75.3)	1,984.6 (78.1) 	2,010.2 (79.1) 	
Ground Clearance				
Front Axle	237.3 (9.3) 	237.3 (9.3)	237.3 (9.3)	
Rear Axle	223.6 (8.8) 	223.6 (8.8)	223.6 (8.8)	
Lift In Height	835.3 (32.9) 	899.1 (35.4) 	924.1 (36.4) 	
Pickup Box Height 	508.6 (20.0) 	508.6 (20.0)	508.6 (20.0)	
Crew Cab 5-ft. 7-in. Box Pickup - Air Suspension 4x4 Rebel (continued)	
Tire Size	285/70R17	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 	
Approach Angle, degrees 	18.7	23.8	25.3	
Departure Angle, degrees	18.9	21.9	23.0	
Ramp Breakover Angle without Skid Plate	17.7	23.6	25.4	
Ramp Breakover Angle with Skid Plate	13.0	18.0	19.6	
Ground Clearance without Skid Plate 	175.5 (6.9) 	253.5 (10.0) 	279.1 (11.0) 	
Ground Clearance with Skid Plate 	157.8 (6.2)	236.3 (9.3)	261.9 (10.3) 	
Fuel-Tank Capacity 	98 litres  (Standard)	98 litres (Standard)	98 litres (Standard)	
	121 litres (Optional)	121 litres (Optional)	121 litres (Optional)	

ACCOMMODATIONS				
Model 	Regular Cab	Quad Cab	Crew Cab	
Seating Capacity, F/R 	3/0 or 2/0	3/3 or 2/3	3/3 or 2/3	
Front				
Head Room	1,013.4 (39.9) 	1.041.4 (41.0) 	1.041.4 (41.0)	
Legroom  	1.041.4 (41.0)	1.041.4 (41.0)	1.041.4 (41.0)	
Shoulder Room	1,676.4 (66.0) 	1,676.4 (66.0)	1,676.4 (66.0)	
Hip Room	1,598.7 (62.9) (1,598.7)	1,605.3 (63.2) 	1,605.3 (63.2) 	
Seat Travel	230.0 (9.0) 	230.0 (9.0)	230.0 (9.0)	
Recliner Range (degrees) 	85 (38 RWD, 47 FWD)	56 (38 RWD 18 FWD)	56 (38 RWD, 18 FWD)	
Rear				
Head Room	N/A	1,008.4 (39.7) 	1,013.5 (39.9) 	
Legroom  	N/A	880.9 (34.7) 	1,023.3 (40.3) 	
Shoulder Room	N/A	1,668.8 (65.7) 	1,668.8 (65.7)	
Hip Room	N/A	1,598.3 (62.9) 	1,605.3 (63.2) 	
Interior Volume				
Front – litres (cu. ft.)  	1769.8 (62.5) 	1817.9 (64.2) 	1817.9 (64.2) 	
Rear – litres (cu. ft.) 	N/A	1483.8 (52.4) 	1730.1 (61.1)