FCA CANADA
2017 Ram Commercial ProMaster™
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION	
Body Styles and Wheelbase	ProMaster 1500 Cargo Van 299 cm (118 inch) wheelbase low roof
ProMaster 1500 Cargo Van 345 cm (136 inch) wheelbase low roof
ProMaster 1500 Cargo Van 345 cm (136 inch) wheelbase high roof	
	ProMaster 2500 Cargo Van 345 cm (136 inch) wheelbase high roof
ProMaster 2500 Cargo Van 403 cm (159 inch) wheelbase high roof	
	ProMaster 2500 Window Van 403 cm (159 inch) wheelbase high roof
ProMaster 3500 Window Van 403 cm (159 inch) wheelbase high roof extended body
ProMaster 3500 Cargo Van 403 cm (159 inch) wheelbase high roof
ProMaster 3500 Cargo Van 403 cm (159 inch) wheelbase high roof extended body	
	ProMaster 3500 Chassis Cab 345 cm (136 inch) wheelbase 
ProMaster 3500 Chassis Cab 403 cm (159 inch) wheelbase
ProMaster 3500 Chassis Cab 403 cm (159 inch) wheelbase extended body	
	ProMaster 3500 Chassis Cab Cutaway 345 cm (136 inch) wheelbase 
ProMaster 3500 Chassis Cab Cutaway 403 cm (159 inch) wheelbase
ProMaster 3500 Chassis Cab Cutaway 403 cm (159 inch) wheelbase extended frame	
Assembly Plant	Saltillo, Mexico	
		
BODY AND CHASSIS		
Layout	Transverse front engine	
Construction	Unibody and ladder frame	
	
ENGINE: 3.6-LITRE PENTASTAR V-6 	
Type and Description	60-degree gasoline V-type	
Displacement	3,604 cu cm (220 cu in) 	
Bore x Stroke	96.0 x 83.0 (3.78 x 3.27) 	
Valve System	Chain-driven DOHC, 24 valves and hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Aluminum deep-skirt block, aluminum alloy heads	
Compression Ratio	10.2:1	
Power 	280 hp (224 kW) at 6,400 rpm	
Torque 	260 lb-ft (364 N•m) at 4,400 rpm	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity	5.7 litres (6.0 quarts) 	
Coolant Capacity	13.25 (14.0 quarts) 	
Emission Controls	Dual three-way catalytic converters, heated oxygen sensors	
		
ENGINE: 3.0-LITRE ECODIESEL I-4	
Type and Description	I-4 diesel, variable geometry turbocharger 	
Displacement	2,990 cu cm (183 cu in) 	
Bore x Stroke	95.8 x 104 (3.78 x 4.09) 	
Valve System	Gear driven DOHC	
Fuel Injection	Electronically controlled common rail MultiJet direct injection 	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps and aluminum alloy head 	
Compression Ratio	17.5:1	
Power 	174 hp (129 kW) @ 3,500 rpm	
Torque 	295 lb-ft (400 N•m) @ 1,400 rpm	
Max. Engine Speed	4,200 rpm	
Fuel Requirement	Diesel	
Oil Capacity	9.0 litres (9.5 quarts) 	
Coolant Capacity	13.3 litres (14.0 quarts) 	
Emission Controls	Selective Catalytic Reduction (SCR)	
	
TRANSMISSION: 62TE AUTOMATIC SIX-SPEED, FRONT-WHEEL DRIVE	
Availability	Standard with 3.6-litre Pentastar V6	
Description	Three planetary gear sets, one overrunning clutch, full electronic control, electronically controlled converter clutch	
Gear Ratios		
1st	3.90	
2nd	2.69	
3rd	2.16	
4th	1.37 	
5th	0.95	
6th	0.65	
Reverse	3.04	
Final Drive and Overall Top Gear Ratios	3.86	

TRANSMISSION: MT40 MANUAL AUTOMATIC SIX-SPEED, FRONT-WHEEL DRIVE	
Availability	Standard with 3.0-litre I-4 Turbo Diesel	
Description	Single disc clutch with hydraulic release	
Gear Ratios		
1st	4.17 	
2nd 	2.35	
3rd 	1.46	
4th 	0.96	
5th 	0.70	
6th 	0.55	
Reverse 	4.08	
Final Drive and Overall Top Gear Ratios	4.56	
		
AXLES		
Front	IFS	
Rear – Cargo Van	Solid axle	
Rear – Chassis Cab and Cut Away	Solid axle with new 17.7 cm (7.0 inch) wider axle 	
	
ELECTRICAL SYSTEM	
Alternator	Cargo Van models with gas engine: 180-amp (standard) or 220-amp (optional); Cargo Van with diesel engine, Chassis Cab and Cut-Away models: 220-amp (standard)	
Battery	95-amp with 800 CCA; 100-amp with 950 CCA (diesel) 	
		
SUSPENSION	
Front	MacPherson with stabilizer bar	
Rear	Solid axle with leaf springs	
		
STEERING		
Type	Rack and pinion with hydraulic power steering	
Turns lock to lock 	Short wheelbase – 11.06; medium wheelbase – 12.46; medium-long wheelbase – 13.54; long wheelbase – 14.28	
Steering ratio 	18.85	
	
BRAKES		
Front Rotor (diameter x width)	300 x 32 (11.8 x 1.26) 	
Rear Rotor (diameter x width)	280 x 16 (11.0 x 0.63) 	
Front Caliper, Lining	Cast iron, dual piston (46mm and 52mm), Brembo	
	Cast iron, dual piston (50mm and 52mm), Brembo	
Rear Caliper, Lining	Cast iron, single piston (48mm), Brembo	
	Cast iron, single piston (52mm), Brembo	

BODY DIMENSIONS / SPECIFICATIONS, cm (inches)	
Vehicle and Body Type	Wheelbase
mm (in)	Height Category	Turning Diameter metres (feet)	Body Heigh
mm (in)	Body Overall Length mm (in)	Body Width w/o mirrors
mm (in)	Vehicle Width w/ mirrors folded
mm (in)	Vehicle Width w/ mirrors extendedmm (in)	Cab to Rear Axle
mm (in)	Overhang Rear Axle to End of Frame
mm (in)	
1500 Cargo Van SWB 
low roof	2997 (118)	H1	11.0 (36.3)	2311 (91)	4953 (195)	2101 (82.7)	2299 (90.5)	2489
(98)	—	—	
1500 Cargo Van MWB 
low roof	3454 (136)	H1	12.4 (40.7)	2311 (91)	5413 (213)	2101 (82.7)	2299 (90.5)	2489
(98)	—	—	
1500 Cargo Van MWB 
high roof	3454 (136)	H2	12.4 (40.7)	2565 (101)	5413 (213)	2101 (82.7)	2299 (90.5)	2489 (98)	—	—	
2500 Cargo Van MWB 
high roof	3454 (136)	H2	12.4 (40.7)	2565 (101)	5413 (213)	2101 (82.7)	2299 (90.5)	2489 (98)	—	—	
2500 Cargo Van LWB 
high roof	4039 (159)	H2	14.2 (46.8)	2565 (101)	5994 (236)	2101 (82.7)	2299 (90.5)	2489 (98)	—	—	
3500 Cargo Van LWB 
high roof	4039 (159)	H2	14.2 (46.8)	2565 (101)	5994 (236)	2101 (82.7)	2299 (90.5)	2489 (98)	—	—	
3500 Cargo Van LWB 
high roof extended 	4039 (159)	H2	14.2 (46.8)	2565 (101)	6350 (250)	2101 (82.7)	2299 (90.5)	2489 (98)	—	—	
2500 Glazed Van LWB 
high roof	4039 (159)	H2	14.2 (46.8)	2565 (101)	5994 (236)	2101 (82.7)	2299 (90.5)	2489 (98)	—	—	
3500 Chassis Cab MWB	3454 (136)	H1	12.4 (40.7)	2311 (91)	5359 (211)	2101 (82.7)	2337 (92)	2769 (109)	2057 (81)	864   (34)	
3500 Chassis Cab LWB	4039 (159)	H1	14.2 (46.8)	2311 (91)	5944 (234)	2101 (82.7)	2337 (92)	2769 (109)	2642 (104)	864    (34)	
3500 Chassis Cab LWB extended	4039 (159)	H1	14.2 (46.8)	2311 (91)	6299 (248)	2101 (82.7)	2337 (92)	2769 (109)	2642 (104)	1219 (48)	
3500 Cutaway MWB	3454 (136)	H1	12.4 (40.7)	2311 (91)	5359 (211)	2101 (82.7)	2337 (92)	2769 (109)	2057 (81)	864 (34)	
3500 Cutaway LWB	4039 (159)	H1	14.2 (46.8)	2311 (91)	5944 (234)	2101 (82.7)	2337 (92)	2769 (109)	2642 (104)	864 (34)	
3500 Cutaway LWB extended	4039 (159)	H1	14.2 (46.8)	2311 (91)	6299 (248)	2101 (82.7)	2337 (92)	2769 (109)	2642 (104)	1219 (48)	

Vehicle and Body Type	Wheelbasemm (in)	Track Front
mm (in)	Track Rear
mm (in)	Approach Angle	Departure Angle	Ground Clearance mm (in)	Seating(1)	Width between wheel housings
cm (in)	Cargo Volume litres (cu ft)	Airbags	
1500 Cargo Van SWB low roof	2997 (118)	1811 (71.3)	1791 (70.5)	18.6°	20°	175 (6.9)	3	1422 (56)	7,334 (259)	6	
1500 Cargo Van MWB low roof	3454 (136)	1811 (71.3)	1791 (70.5)	18.6°	20°	175 (6.9)	3	1422 (56)	8,608 (304)	6	
1500 Cargo Van MWB high roof	3454 (136)	1811 (71.3)	1791 (70.5)	18.6°	20°	175 (6.9)	3	1422 (56)	9996 (353)	6	
2500 Cargo Van MWB high roof	3454 (136)	1811 (71.3)	1791 (70.5)	18.6°	20°	175 (6.9)	3	1422 (56)	9996 (353)	6	
2500 Cargo Van LWB high roof	4039 (159)	1811 (71.3)	1791 (70.5)	18.6°	20°	175 (6.9)	3	1422 (56)	11,893 (420)	6	
3500 Cargo Van LWB high roof	4039 (159)	1811 (71.3)	1791 (70.5)	18.6°	20°	175 (6.9)	3	1422 (56)	11,893 (420)	6	
3500 Cargo Van LWB high roof extended 	4039 (159)	1811 (71.3)	1791 (70.5)	18.6°	20°	175 (6.9)	3	1422 (56)	13,110 (463)	6	
2500 Glazed Van LWB high roof	4039 (159)	1811 (71.3)	1791 (70.5)	18.6°	20°	175 (6.9)	3	1422 (56)	11,893 (420)	6	
3500 Chassis Cab MWB	3454 (136)	1811 (71.3)	1981 (78)	18.6°	—	175 (6.9)	3	—	—	6	
3500 Chassis Cab LWB	4039 (159)	1811 (71.3)	1981 (78)	18.6°	—	175 (6.9)	3	—	—	6	
3500 Chassis Cab LWB extended	4039 (159)	1811 (71.3)	1981 (78)	18.6°	—	175 (6.9)	3	—	—	6	
3500 Cutaway MWB	3454 (136)	1811 (71.3)	1981 (78)	18.6°	—	175 (6.9)	3	—	—	6	
3500 Cutaway LWB	4039 (159)	1811 (71.3)	1981 (78)	18.6°	—	175 (6.9)	3	—	—	6	
3500 Cutaway LWB extended	4039 (159)	1811 (71.3)	1981 (78)	18.6°	—	175 (6.9)	3	—	—	6	
(1)	Standard seating configuration is 2-passenger with optional 3-passenger configuration available.