FCA CANADA
2017 Ram ProMaster City
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION		
Body Styles	ProMaster City Cargo Van 	
	ProMaster City Wagon	
Assembly Plant	Bursa, Turkey, at Fiat’s joint venture TOFAS plant. The van is upfitted into a cargo van at the FCA US Transformation Center in Baltimore, Maryland 	
EPA vehicle class	Small commercial van (Class 1)	
Introduction Date	June 2014 as a 2015 model year	
		
BODY AND CHASSIS		
Layout	Front transverse engine, front-wheel drive (FWD) only	
Construction	Body-frame integral (BFI, or Unibody) with electro-galvanized steel body. Integrated steel ladder H-frame with single-piece longitudinal frame rails	
		
ENGINE: 2.4-LITRE I-4 MULTIAIR2 TIGERSHARK GAS ENGINE	
Availability	Standard on all models	
Type and Description	I-4 (inline 4) 16-valve MultiAir2 with multiport fuel injection	
Displacement 	2,360 cu cm (144 cu in) 	
Bore & stroke	88.0 x 97.0 (3.46 x 3.82) 	
Block material	Aluminum	
Cylinder head material	Aluminum	
Valvetrain	DOHC, four valves per cylinder (16 total)	
Ignition system	Coil-on-plug ignition, spark plugs with dual precious metals	
Fuel delivery	Sequential, multiport, electronic, returnless	
Compression ratio	10:0:1	
Power 	178 hp (133 kW) at 6,400 rpm 	
Torque 	174 lb-ft (236 N•m) at 3,800 rpm 	
Fuel requirement	Unleaded regular, 87 octane 	
Maximum engine speed	6,500 rpm (electronically limited)	
Oil capacity	5.2 lites (5.5 quarts) 	
Coolant capacity	6.7 litres (7.1 quarts) 	
Emissions controls	GPEC3 engine-management system with close-coupled catalyst and wide-range O2 sensor	
EnerGuide (2016) Fuel Consumption Ratings L/100 km (MPG – imperial gallon) city/hwy/combined	11.2/8.1/9.8 (25/35/29)	
Based on 2016 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information, please visit the Government of Canada website: www.vehicles.nrcan.gc.ca
	
Engine assembly plant	Trenton, Michigan, USA	
	
TRANSMISSION: 948TE NINE-SPEED AUTOMATIC	
Availability	Standard on all models	
Type	Nine-speed FWD, electronically controlled automatic overdrive transmission with torque converter clutch. Clutch-to-clutch architecture with integral electro/hydraulic controls module	
Fluid capacity	6.15 litres (6.5 quarts) 	
Torque converter	242 mm	
Gear ratios:		
1st	4.70	
2nd	2.84	
3rd	1.90	
4th	1.38	
5th	1.00	
6th	0.80	
7th	0.69	
8th	0.58	
9th	0.47	
Reverse	3.81	
Final Drive Ratio	3.73	
		
SUSPENSION	
Front Suspension		
Type	MacPherson Strut, independent	
Stabilizer Bar, Solid	26	
Spring Rate (N/mm)	25	
Shock Type	Twin-tube	
Wheel Travel (mm – jounce/rebound)	57/93	
Rear Suspension		
Type	Independent bi-link with coil springs, telescopic shock absorbers and stabilizer bar	
Stabilizer Bar, Solid 	16	
Spring Rate (N/mm)	28	
Shock Type	Twin-tube	
Wheel Travel (mm – jounce/rebound)	51/31	
		
BRAKES		
Front Type (diameter x width)	Ventilated disc, 305 x 28 (12 x 1.1) 	
Rear Type (diameter x width)	Drum, 254 x 57 (10 x 2.2) 	
Front Caliper, Lining	Cast iron, single piston (57)	
Rear Brake, Lining	Leading trailing drum brake assembly with 25-mm wheel cylinder	
Anti-lock braking system (front and rear)	Standard	
Electronic Stability Control (ESC) 	Standard	
Total Front Swept Area (mm)	5,100	
Total Rear Swept Area (mm)	12,155	
		
STEERING		
Type	Specifically calibrated hydraulic power-assisted rack-and-pinion	
Ratio	15:9:1	
Turns Lock-to-Lock	2.9	
Turn Diameter (curb-to-curb)	12.8 metres (42 ft.)	
		
WHEELS AND TIRES		
Wheels	16-inch steel (aluminum available)	
Tires	215/55R16XL all-season	
		
DIMENSIONS AND CAPACITIES		
EXTERIOR		
Wheelbase 	3,109 (122.4) 	
Track, Front	1,523 (60.0) 	
Track, Rear 	1,548 (60.9) 	
Overall Length	4,752 (187.1) 	
Overall Width including mirrors	2,148 (84.6) 	
Overall Height 	1,886 (74.2) 	
Front Overhang 	903 (35.6) 	
Rear Overhang 	740 (29.1) 	
Approach Angle (degrees)	13.3	
Departure Angle (degrees)	30.8	
Windshield Slope Angle (degrees)	49.2	
Ground Clearance	131 (5.2) 	
Fuel Tank Capacity	60.6 litres (13.3 imperial gallons)	
			
	Cargo Van	Passenger Wagon	
Cargo Length 	2,215 (87.2) 	Behind rear seats = 1,389 (54.7) 
Rear seats folded = 1,758 (69.2) 	
Cargo Width	1,535 (60.4) 	1,463 (57.6) 	
Cargo Height @ Roof 	1,315.7 (51.8) 	1,237 (48.7) 	
Max. Cargo Volume, litres (cu. ft.)	3,729 (131.7)	2,880 (101.7)	
Cargo Width @ Wheel Well 	1,229 (48.4) 	1,229 (48.4)	
Load Floor Height 	592 (23.3) 	605 (23.8)	
Side Door Openings (w x h), mm (in)	655x1107 (25.8x43.6)	538x1085 (21.2x42.7)	
Rear Door Openings (w x h), mm (in)	1234x1204 (48.6x47.4)	1234x1179 (48.6x46.4)	
Rear Door Swing (degrees, first detent/full open detent)	90/180	90/180	
Rear Door Split (degrees)	60 (driver side)/
40 (passenger side)	60 (driver side)/
40 (passenger side)	
Rear Step-in Height 	592 (23.3) 	605 (23.8) 	
Side Step-in Height 	546 (21.5) 	490 (19.3) 	
			
ACCOMMODATIONS			
	Cargo Van	Passenger Wagon	
Seating Capacity (front/rear)	2/0	2/3	
			
Front Row (Passenger & Cargo Vans)		
Headroom 	1,168 (46.0) 	
Leg Room 	1,036 (40.8) 	
Shoulder Room 	1,506 (59.3) 	
Hip Room 	1,341 (52.8) 	

Second Row (Passenger Van Only)	
Headroom 	1,118 (44.0)	
Leg Room 	935 (36.8) 	
Shoulder Room 	1,473 (58.0) 	
Hip Room 	1,504 (59.2) 	
		
CAPABILITY		
	Cargo Van	Passenger Wagon	
Gross Vehicle Weight Rating (GVWR; kg, lb)	2,447 (5,395)	2,447 (5,395)	
Curb Weight, kg (lb)	2,408 (3,509)	1,648 (3,635)	
Payload, kg (lb)	862 (1900)	777 (1,713)	
Tongue Load, kg (lb)	90 (200)	90 (200)	
Towing Capacity, kg (lb)	907 (2,000)	892 (1,867)	
Gross Combined Vehicle Weight Rating, kg (lb)	2,676 (5,900)	2,676 (5,900)