FCA CANADA
2018 Chrysler Pacifica & Pacifica Hybrid
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

General Information		
Vehicle Type	Multipurpose vehicle 	
Assembly Plant	Windsor, Ontario, Canada 	
EnerGuide Vehicle Class	Multipurpose vehicle	
Introduction Date	Spring 2016	
		
BODY/CHASSIS		
Layout	Transverse front engine, front-wheel drive	
Construction	Steel unibody with hinged front doors; aluminum-skinned sliding left and right side doors — power available; magnesium-structured/aluminum-skinned rear liftgate with gas props — power available	
		
Engine: 3.6-Litre Pentastar V-6 	
Availability	Standard on gas engine models	
Type and Description	60-degree dual overhead cam engine	
Displacement	220 cu. in. (3,605 cu. cm)	
Bore x Stroke	96mm x 83mm	
Valve System	24-valve, end pivot roller finger followers with variable valve lift (intake only) and continuous variable-valve timing on both intake and exhaust cams; chain-driven	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	High-pressure die-cast A380 aluminum block with iron liners and 
semi-permanent mold A319 aluminum heads	
Compression Ratio	11.3:1	
Power (SAE net)	287 hp (214 kW) @ 6,400 rpm	
Torque (SAE net)	262 lb.-ft. (355 N•m) @ 4,000 rpm	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane, or E0 to E15	
Oil Capacity	5 quarts (4.7 litre)	
Coolant Capacity	7.2 quarts (6.8 litre)	
Emission Controls 
	Integrated cast-aluminum header manifolds; positive crankcase ventilation; inlet and exhaust cam phasers with internal cooled exhaust gas recirculation; evaporative emissions system	
	Engine stop-start technology standard on LX, Touring, Touring Plus, Touring L, Touring L Plus and Limited	
EnerGuide Fuel Consumption Ratings 
L/100km (imp. mpg) (city/hwy/combined)	12.4 (23) / 8.4 (34) / 10.6 (27) (models with engine stop-start)	
	12.9 (22) / 8.4 (34) / 10.9 (26) (Pacifica L models)	
Based on 2018 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information please visit the government of Canada website www.vehicles.nrcan.gc.ca	
Assembly Plant	Saltillo Engine Plant, Saltillo, Mexico	
		
Engine: 3.6-Litre Pentastar V-6 EHYBRID (ATKINSON CYCLE)	
Availability	Standard on hybrid models	
Type and Description	60-degree dual overhead cam engine	
Displacement	220 cu. in. (3,605 cu. cm)	
Bore x Stroke	96mm x 83mm	
Valve System	24-valve, end pivot roller finger followers and continuous variable-valve timing on both intake and exhaust cams; chain-driven	
Fuel System	Port-fuel injection (PFI)	
Construction	High-pressure die-cast A380 aluminum block with iron liners and 
semi-permanent mold A319 aluminum heads	
Compression Ratio	12.5:1	
Total System Power	Estimated 260 (194 kW) hp	
Fuel Requirement	Unleaded regular, 87 octane, or E0 to E15	
Oil Capacity	5 quarts (4.7 litre)	
Coolant Capacity	7.2 quarts (6.8 litre)	
Emission Controls 	Integrated cast-aluminum header manifolds; positive crankcase ventilation; intake and exhaust cam phasers; evaporative emissions system	
	
EnerGuide Fuel Consumption
Ratings Le/100 km (MPGe (imp.)
(city/highway/combined)	2.6 (109) / 3.0 (94) / 2.8 (101)	
Based on EnerGuide fuel consumption ratings for minivans in the WardsAuto Small Van segment. 2.8 Le/100 km (101 MPGe) highway. 2018 Chrysler Pacifica Hybrid with 3.6L Pentastar™ VVT V6 Hybrid engine and eFlite Electrically Variable Transmission. Le/100 km is an equivalent measure of gasoline fuel consumption for electric energy consumed by Plug-in Hybrid Electric Vehicles (PHEV) operating in electric mode. Miles per gallon equivalent (MPGe) ratings based on imperial gallon.  Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors.	
EnerGuide Fuel Consumption
Ratings L/100 km (imp. mpg)
(city/highway/combined)		7.3 (39) / 7.2 (39) / 7.3 (39)	
Based on 2018 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information please visit the government of Canada website www.vehicles.nrcan.gc.ca	
Assembly Plant	Trenton Engine Complex, Trenton, Mich., USA and 
Saltillo Engine Plant, Saltillo, Mexico	
		
TRANSMISSION: 948TE TORQUEFLITE NINE-SPEED AUTOMATIC		
Availability	Standard on gas engine models	
Description	Nine-speed FWD, electronically controlled automatic overdrive transmission with torque converter clutch. Clutch-to-clutch architecture, with integral electro/hydraulic control module	
Gear Ratios		
1st 	4.70	
2nd	2.84	
3rd 	1.91	
4th	1.38  	
5th 	1.00	
6th 	0.81	
7th 	0.70	
8th 	0.58	
9th 	0.48	
Reverse 	3.81    	
Spread	9.81	
Final Drive Ratio	3.25	
	
TRANSMISSION: EFLITE ELECTRICALLY VARIABLE 	
Availability	Standard on hybrid models	
Description	Electrically variable transmission with dual-motor EV drive capability 	
Motor A		
Power 		Estimated 84 hp (63 kW)	
Motor B 		
Power  	Estimated 114 hp (85 kW)	
		
HYBRID BATTERY PACK 		
Availability	Standard on hybrid models	
Description	High voltage, 96 cell Li-ion, 16kWh total energy, 360 V nominal 	
		
Suspension		
Front	Independent MacPherson strut, coil over gas-charged shock absorbers, stabilizer bar with hydroformed steel perimetre cradle 	
Rear	Independent twist-blade with coil springs, twin-tube shock absorbers with integrated rebound springs	
		
STEERING		
Type	Electric rack and pinion	
Overall Ratio	16.2:1	
Turning Diametre (curb-to-curb)	39.7 ft. (12.1 m)	
Steering Turns (lock-to-lock)	3.13	
		
BRAKES		
Power-assist Type	Vacuum assist	
Availability	Standard on all models	
Front		
Size and type	13.0 x 1.1 (330 x 28) vented rotor with (51.0) single-piston floating caliper	
Swept area	73.6 sq. in. (475 sq. cm)	
Rear		
Size and type	13.0 x 0.47 (330 x 12) solid rotor with (44.0) single-piston floating caliper	
Swept area	66.5 sq. in. (429 sq. cm)	
Parking Brake Type	Electric park brake 	
Anti-lock Brake System (ABS)	Standard    	
Electronic Stability Control (ESC) 	Standard	
Traction Control	Standard	
Brake Assist	Standard	
		
Dimensions and Capacities		
Wheelbase	121.6 (3,089)	
Overhang — Front	37.8 (960)	
Overhang — Rear	44.3 (1,127)	
Track — Front	68.3 (1,735) gas engine models
68.2 (1,734) hybrid models	
Track — Rear	68.3 (1,736) gas engine models
68.2 (1,735) hybrid models	
Overall Length	203.8 (5,176)	
Overall Width	79.6 (2,022)	
Overall Width with Mirrors	90.4 (2,297)	
Overall Height 	69.9 (1,777)	
Liftover Height 	24.3 (617)	
Cargo Width at Wheelhouse 	48.8 (1,239)	
Maximum Cargo Height 	47.6 (1,208)	
Approach Angle (degrees)	14.0 gas engine models
13.5 hybrid models	
Ramp Breakover Angle (degrees)	12.5	
Departure Angle (degrees)	18.7 gas engine models
18.6 hybrid models	
Ground Clearance 	5.1 (131) gas engine models
5.1 (130) hybrid models	
Drag Coefficient (Cd)	0.300	
Aero CdA	9.95	
Fuel Tank Capacity, gallons (L)	19 (71.9) gas engine models
16.5 (62.5) hybrid models	
	
Gross Vehicle Weight Rating (GVWR), lbs. (kg)	6,055 (2,747) gas engine models
6,300 (2,858) hybrid models	
Towing Capacity, lbs. (kg)
	3,600 (1,633) gas engine models
Not recommended for hybrid models	
EPA Curb Weight, lbs. (kg)		4,330 (1,964) gas engine models
4,987 (2,262) hybrid models	
Weight Distribution (percent front/rear)	55/45 gas engine models
56.5/43.5 hybrid models	
		
Accommodations		
Seating Capacity (front/second/third rows)	2/2/3 or 2/3/3 gas engine models
2/2/3 hybrid models	
Total SAE Volume, litres (cu. ft.)	5,587 (197.3)	
Front		
Head Room	40.1 (1,020)	
Head Room with Sunroof 	38.4 (975)	
Leg Room	41.1 (1,045)	
Shoulder Room	63.8 (1,622)	
Hip Room	59.0 (1,500) 	
Seat Travel	8.7 (220)	
Recliner Angle Range (degrees)	58	
First Row SAE Volume, litres (cu. ft.) 	1,730 (61.1) 	
Second Row 		
Head Room	39.6 (1,006)	
Head Room with Sunroof 	38.0 (966)	
Legroom	39.0 (992)	
Minimum Knee Clearance	4.8 (123)	
Shoulder Room	63.0 (1,602)	
Hip Room	64.8 (1,647)	
Second Row SAE Volume, litres (cu. ft.)	1,600 (56.5)	
Third Row 		
Head Room	38.7 (984)	
Head Room with Sunroof 	38.7 (984)	
Legroom	36.5 (929)	
Knee Clearance	3.5 (89)	
Shoulder Room	61.2 (1,555)	
Hip Room	49.5 (1,258)	
Third Row SAE Volume, litres (cu. ft.)		1,345 (47.5)	
Cargo Volume 			
Maximum Passenger Volume, litres (cu. ft.)	4,672 (165.0)	
Maximum SAE Volume 
behind First Row, litres (cu. ft.)	3,979 (140.5)	
Maximum SAE Volume 
behind Second Row, litres (cu. ft.)	2,478 (87.5)	
Maximum SAE Volume 
behind Third Row, litres (cu. ft.)	915 (32.3)	
Total Passenger plus Volume 
behind Third Row, litres (cu. ft.)	5,587 (197.3)	
		
Wheels		
Availability	Standard on L and LX	
Type and Material	Steel 	
Size	17 x 7	
Availability	Standard on Touring, Touring Plus, Touring L, Touring L Plus, Hybrid Touring Plus, Hybrid Touring L, and Hybrid Limited; Optional on LX	
Type and Material	Cast-aluminum 	
Size	17 x 7	
Availability	Standard on Limited; Optional on Touring, Touring Plus, 
Touring L, Touring L Plus, and Hybrid Limited	
Type and Material	Cast-aluminum	
Size	18 x 7.5	
Availability	Optional on Limited	
Type and Material	Cast-aluminum	
Size	20 x 7.5	
		
Tires		
Availability	Standard on L, LX, Touring, Touring Plus, Touring L, Touring L Plus, Hybrid Touring Plus,Hybrid Touring L, and Hybrid Limited	
Size and Type	235/65R17 BSW, All-season 	
Model	Kumho Solus TA31, Yokohoma Avid S34	
Availability	Standard on Limited; Optional on Touring, Touring Plus, 
Touring L, Touring L Plus, and Hybrid Limited	
Size and Type	235/60R18 BSW, All-season	
Model	Michelin Premier A/S, Bridgestone Turanza EL440, Nexen N’Priz RH7α	
Availability	Optional on Limited	
Size and Type	245/50R20 BSW, All-season 	
Model	Kumho Solus TA31, Falken Ziex CT50	

////