FCA CANADA
2018 Dodge Charger Enforcer
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

General Information		
Vehicle Type	E-segment sedan	
Assembly Plant	Brampton Assembly Plant, Canada	
EnerGuide Vehicle Class	Full-size	
Introduction Date	Third quarter 2017 as 2018 model 
(fleet customers only)	
		
Body and CHASSIS		
Layout	Longitudinal front engine, rear-wheel drive (RWD) or all-wheel drive (AWD) 	
Construction	Unitized steel body and aluminum hood	
	
Engine: 3.6-LitrE PENTAStar DOHC 24-Valve V-6	
Availability	Standard 	
Type and Description	60-degree V-type, liquid-cooled	
Displacement	220 cu. in. (3,604 cu. cm)	
Bore x Stroke	3.78 x 3.27  (96.0 x 83.0)	
Valve System	Chain-driven DOHC, 24 valves, hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Aluminum deep-skirt block with aluminum-alloy heads	
Compression Ratio	10.2:1	
Power (SAE net)	292 bhp (218 kW) @ 6,350 rpm (81.1 bhp/litre)	
Torque (SAE net)	260 lb.-ft. (353 N•m) @ 4,800 rpm	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2; and E-85 (Federal Bin 5, 37 state compliant)	
Oil Capacity	6 quarts (5.7 litres) with dry filter	
Coolant Capacity	14.0 quarts (13.25 litres)	
Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors 
and internal engine features	
Max. Gross Trailer Weight	1,000 lbs. (454 kg)	
EnerGuide (2018) Fuel Consumption Ratings L/100 km (MPG – imp. gal.) city/hwy/combined	13.7 (21) / 9.0 (31) / 11.6 (24) (RWD with five-speed automatic)	
Based on 2018 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information, please visit the Government of Canada website: www.vehicles.nrcan.gc.ca	
Engine Assembly Plant	Trenton South Engine Plant, USA	
	
ENGINE: 5.7-LitrE HEMI® V-8 WITH FUEL SAVER TECHNOLOGY	
Availability	Optional	
Type and Description	90-degree V-type, liquid-cooled with variable-cam timing (VCT)	
Displacement	345 cu. in. (5,654 cu. cm)	
Bore x Stroke	3.92 x 3.58 (99.5 x 90.9)	
Valve System	Pushrod-operated overhead valves, 16 valves, eight deactivating and eight conventional hydraulic lifters, all with roller followers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps, aluminum-alloy heads with hemispherical combustion chambers	
Compression Ratio	10.5:1	
Power (SAE net)	370 bhp (276 kW) @ 5,250 rpm (64.9 bhp/litre)	
Torque (SAE net)	395 lb.-ft. (536 N•m) @ 4,200 rpm	
Max. Engine Speed	5,800 rpm (electronically limited)	
Fuel Requirement	Unleaded midgrade, 89 octane (R+M)/2 — recommended 	
	Unleaded regular, 87 octane (R+M)/2 — acceptable	
Oil Capacity	7 quarts (6.6 litres)	
Coolant Capacity	14.7 quarts (13.9 litres)	
Emission Controls 	Dual close-coupled three-way catalytic converters, quad heated oxygen sensors and internal engine features	
Max. Gross Trailer Weight	1,000 lbs. (454 kg)	

	
EnerGuide (2018) Fuel Consumption Ratings, L/100 km (MPG – imp. Gal.) city/hwy/combined	15.6 (18) / 9.7 (29) / 12.9 (22) (RWD with five-speed automatic) 	
	16 (18) / 10.1 (28) / 13.3 (21) (AWD with five-speed automatic)	
Based on 2018 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information, please visit the Government of Canada website: www.vehicles.nrcan.gc.ca	
		
Transmission: Automatic Five-Speed Overdrive WITH AUTO STICK	
Availability	Standard 	
Description	Adaptive electronic control or Auto Stick driver-interactive manual control and electronically-modulated torque converter clutch	
Gear Ratios		
1st	3.59	
2nd	2.19	
3rd	1.41	
4th	1.00	
5th	0.83	
Reverse	3.16	
Final Drive Ratio	Standard (RWD): 2.62	
	Standard (AWD): 3.07	
Overall Top Gear	Standard (RWD): 2.20	
	Standard (AWD): 2.55	
		
Electrical System		
Alternator	220-amp — standard 	
Battery	H8 Case, 800 CCA, maintenance-free	
		
Suspension		
Front 	Independent SLA with high upper “A” arm, coil spring over gas-charged monotube shock absorbers and stabilizer bar	
	Lateral and diagonal lower links with dual ball joint knuckles 	
	One piece lower-control arms — standard on Charger V-8 AWD model only	
Rear	Five-link independent with coil springs, gas-charged load-leveling NIVOMAT rear shocks, stabilizer bar and isolated suspension cradle 	
		
Steering		
Type	Rack and pinion 	
	Electric power steering (EPS) with RWD	
	Electro hydraulic power steering (EHPS) with AWD	
Overall Ratio	RWD: 14.4:1	
	AWD: 16.5:1	
Turning Diametre (curb-to-curb)	RWD: 37.7 ft. (11.5 m)	
	AWD: 38.7 ft. (11.8 m)	
Steering Turns (lock-to-lock)	RWD: 2.6	
	AWD: 3.1	
	
Dimensions and Capacities(c)		
Wheelbase	120.2 (3,052)	
Track, Front	63.4 (1,611)	
Track, Rear	63.8 (1,620)	
Overall Length	198.4 (5,040)	
Overall Width	75.0 (1,905)	
Overall Height	Enforcer V-6 RWD — 58.4 (1,482)	
	Enforcer V-8 RWD — 58.4 (1,482)	
	Enforcer V-8 AWD — 58.4 (1,482)	
Ground Clearance	Enforcer V-6 RWD — 5.1 (130.0)	
	Enforcer V-8 RWD — 5.1 (130.0)	
	Enforcer V-8 AWD — 5.1 (130.0)	
Frontal Area, sq. ft. (sq. m)	26.2 (2.43)	
Drag Coefficient (Cd)	RWD: 0.297	
	AWD: 0.297	
Curb Weight, lb. (kg)	Enforcer V-6 RWD — 4,091 (1,855.6)	
	Enforcer V-8 RWD — 4,321 (1,969)	
	Enforcer V-8 AWD — 4,522 (2,051.1)	
	
Gross Vehicle Weight Rating (GVWR)	Enforcer V-6 RWD — 5,250 (2,381)	
	Enforcer V-6 RWD — 5,450 (2,472) (optional)	
	Enforcer V-8 RWD — 5,450 (2,472)	
	Enforcer V-8 AWD — 5,500 (2,495)	
Gross Axle Weight Rating (GAWR)	Enforcer V-6 RWD — 2,850 (1,295)	
	Enforcer V-8 RWD — 2,850 (1,295)	
	Enforcer V-8 AWD — 2,850 (1,295)	
Weight Distribution, percent F/R	Enforcer V-6 RWD — 52/48	
	Enforcer V-8 RWD — 54/46	
	Enforcer V-8 AWD — 55/45	
Fuel Tank Capacity, litres 
(imperial gal.)	70.0 (15.4)	
(c) All dimensions measured at curb weight with standard tires.	
		
Brakes		
Front		
Rotor size and type	14.5 x 1.26 (370 x 32) vented	
Caliper size and type	1.77 (45) x dual-piston sliding with cast-iron housing	
Swept area	388 sq. in. (2,503.2 sq. cm.)	
Rear		
Rotor size and type	13.8 x 1.02 (350 x 26) vented	
Caliper size and type	1.78 (45) single-piston sliding with cast-iron housing	
Swept area	300 sq. in. (1,935.5 sq. cm.)	
		
Accommodations		
Seating Capacity, F/R	2/3	
Front		
Headroom	38.6 (981)	
Legroom	41.8 (1,061)	
Shoulder room	59.5 (1,510)	
Hip room	56.2 (1,428)	
	
Seat travel	Driver — 10.6 (270)	
	Passenger — 8.66 (220)	
EPA front row interior volume, 
cu. ft. (litres)	55.6 (1,574.4)	
Rear Seat		
Headroom	36.6 (930.6)	
Legroom	40.1 (1,019)	
Knee clearance	3.9 (99)	
Shoulder room	57.9 (1,472)	
Hip room	56.1 (1,425)	
EPA second row interior volume, 
cu. ft. (litres)	49.2 (1,393)	
Total Interior Volume, cu. ft. (litres)	104.7 (2,964.8)	
EPA Luggage Compartment Volume, 
cu. ft. (litres)	16.5 (467.2)	
EPA Interior Volume Index, 
cu. ft. (litres)	121.2 (3,532.0)	
Trunk Liftover Height		Enforcer V-6 (RWD) — 30.2 (766.0) 	
	Enforcer V-8 (RWD) — 30.1 (765.7) 	
	Enforcer V-8 (AWD) — 30.1 (765.7)	
		
Tires		
Availability	Standard 	
Size and type	P225/60R18 99V BSW All-season performance	
Mfr. and model	Goodyear performance tires	
Revs per mile (km)	704 (437)	
	
Availability		Optional		
Size and type	P245/55R18 99W BSW All-season performance	
Mfr. and model	Goodyear performance tires	
Revs per mile (km)	705 (438)	
	
Wheels		
Availability	Standard 	
Type and material	Steel wheel with chromed centre cap or optional painted wheel cover	
Size	18 x 7.5	

////