FCA CANADA
2018 Dodge Durango
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

General Information		
Vehicle Type	Four-door sport-utility vehicle	
Assembly Plant	Jefferson Avenue North, Detroit, Mich., USA	
EPA Vehicle Class	Multipurpose vehicle 	
Introduction Date 	Third quarter 2017 as a 2018 model	
		
BODY AND CHASSIS		
Layout	Longitudinal front engine, rear drive (transfer case with full-time 
all-wheel drive available)	
Construction	Steel unibody	
	
Engine: 3.6-LitrE pentastar v-6	
Availability	Standard — SXT, GT and Citadel (not available on R/T)	
Type and Description	60-degree V-type, liquid-cooled	
Displacement	220 cu. in. (3604 cu. cm)	
Bore x Stroke	3.78 x 3.27 (96 x 83)	
Valve System	Chain-driven DOHC, 24 valves and hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Aluminum deep-skirt block, aluminum alloy heads	
Compression Ratio	10.2:1	
Power (SAE J2723)	Single exhaust - 293 hp @ 6400 rpm	
	Dual exhaust - 295 hp @ 6400 rpm	
Torque (SAE J2723)	260 lb.-ft. (353 N•m) at 4,000 rpm (both single and dual exhaust)	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R + M)/2  	
Oil Capacity	6.0 quarts (5.7 litres)	
Coolant Capacity	10.4 quarts (9.9 litres) without trailer tow	
	11 quarts (10.4 liters) with trailer tow	
Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors 
and internal engine features(a)	
	
Energuide Estimated Fuel Economy L/100 km (imperial mpg) (city/hwy)	 12.7 (22) / 9.6 (29)	
Based on 2018 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information please visit the government of Canada website www.vehicles.nrcan.gc.ca	
Assembly Plant	Trenton South Engine Plant, Trenton, Mich., USA	
		
ENGINE: 5.7-LITRE HEMI® V8		
Availability	Standard — R/T and optional on GT and Citadel 	
Type and Description	90-degree V-type, liquid-cooled	
Displacement	345 cu. in. (5,654 cu. cm)	
Bore x Stroke	3.92 x 3.58 (99.5 x 90.9)	
Valve System	Variable-valve timing (VVT), pushrod-operated overhead valves, 
16 valves, eight deactivating and eight conventional hydraulic lifters, 
all with roller followers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps, 
aluminum alloy heads with hemispherical combustion chambers	
Compression Ratio	10.5:1	
Power (est.) (SAE J2723)	360 hp (268 kW) at 5,150 rpm	
Torque (est.) (SAE J2723)	390 lb.-ft. (529 N•m) at 4,250 rpm	
Max. Engine Speed	5,800 rpm (electronically limited)	
Fuel Requirement	Unleaded mid-grade, 89 octane (R+M)/2—recommended;
unleaded regular, 87 octane (R+M)/2—acceptable	
Oil Capacity	7 quarts (6.6 litres)	
Coolant Capacity	15.4 quarts (14.6 litres) without trailer tow	
	16 quarts (15.2 litres) with trailer tow	
Emission Controls 	Dual close-coupled three-way catalytic converters, quad heated oxygen 
sensors and internal engine features(a)	
Energuide Estimated Fuel Economy L/100 km (imperial mpg) (city/hwy)	16.6 (17) / 10.9 (26)	
Based on 2018 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information please visit the government of Canada website www.vehicles.nrcan.gc.ca	
Assembly Plant	Saltillo Engine Plant, Saltillo, Mexico	

ENGINE: 6.4-LITRE V8	
Availability	Standard — SRT 	
Type and Description	90-degree V-type, liquid-cooled	
Displacement, cu. in. (cu. cm.)	392 (6,417)	
Bore x Stroke	4.09 x 3.72 (103.9 x 94.5)	
Valve System	Pushrod-operated overhead valves, 16 valves with sodium-filled exhaust valves and hollow stem intake valves, 16 conventional hydraulic lifters, 
all with roller tips	
Fuel Injection	Sequential, multi-port, electronic, returnless; automatic features Fuel Saver mode	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps, aluminum alloy heads with hemispherical combustion chambers	
Compression Ratio	10.9:1	
Power (SAE J2723)	475 hp (354 kW) at 6,000 rpm 	
Torque (SAE J2723)	470 lb.-ft. (637 N•m) at 4,300 rpm 	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Premium 91 octane (R+M)/2 — recommended	
Oil Capacity, qt. (litre) 	7 (6.6)	
Coolant Capacity, qt. (litre)	14 (13.25)	
Factory Oil Fill 	0W-40 Pennzoil Ultra synthetic	
Emission Controls 	Dual close-coupled three-way catalytic converters, quad-heated oxygen sensors and internal engine features(a)	
Exhaust Type 	Dual exhaust with dual 4-in. round with Nickel-chrome tips 	
Energuide Estimated Fuel Economy L/100 km (imperial mpg) (city/hwy)	18.3 (15) / 12.2 (23)	
Based on 2018 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information please visit the government of Canada website www.vehicles.nrcan.gc.ca	
Assembly Plant	Saltillo Engine Plant, Saltillo, Mexico 	
	
TRANSMISSION: torqueflite EIGHT-SPEED automatic 845TE	
Availability	Standard — all V6 models 	
Description	Driver-interactive manual control via steering wheel paddle shifters and electronically modulated torque converter clutch	
	
Gear Ratios		
1st 	4.71	
2nd 	3.14	
3rd  	2.11	
4th 	1.67	
5th 	1.29	
6th	1.000	
7th	0.84	
8th	0.67	
Reverse 	3.30 	
	
TRANSMISSION: TORQUEFLITE AUTOMATIC, EIGHT-SPEED OVERDRIVE 8HP70	
Availability	Standard — all V8 models	
Description	Driver-interactive manual control via steering wheel paddle shifters and electronically-modulated torque converter clutch with Eco mode	
Gear Ratios		
1st	4.71	
2nd 	3.14	
3rd	2.11	
4th 	1.67	
5th 	1.29	
6th	1.00	
7th	0.84	
8th 	0.67	
Reverse 	3.30	
		
TRANSFER CASE: MP 3010 		
Availability	Standard with V6 engine 	
Type	Single-speed	
Operating Mode	Full-time AWD	
Low Range Ratio	None	
Torque Split, Front/Rear	50/50	
		
TRANSFER CASE: MP 3023		
Availability	Standard with V8 engine 	
Type	Two-speed, electronically shifted	
Operating Modes	AWD Low (Lock), Neutral; full-time active AWD	
Low Range Ratio	2.72	
Torque Split, Front/Rear	Variable	
	
TRANSFER CASE: MP 3010	
Availability	Standard with 6.4-litre V-8 engine 	
Type	Single-speed, electronic proportioning	
Operating Mode	Full-time AWD	
Torque Split, Front/Rear	Variable:
Auto (40/60) 
Snow and Tow (50/50)
Sport (35/65)
Track (30/70) 	

Axles		
Front		
Differential Type	Conventional	
Availability	Standard on all models 	
Ring Gear Diametre	7.7 (195)	
Axle Ratios	3.45:1 (V-6 AWD)  	
	3.09:1 (V-8)	
	3.70:1 (SRT)	
Rear		
Differential Type	Conventional	
Availability	Standard on all engines	
Ring Gear Diametre	7.7 (195) (V6) 	
	9.1 (230) (V8)	
Axle Ratios	3.45:1 (V6) 	
	3.09:1 (V8)	
	3.70:1 (SRT)	
		
Electrical System		
Alternator	160-amp; 180-amp or 220-amp depending on option content	
Battery	Maintenance-free	
	H6 650 CCA + Auxiliary 200 CCA on Electronic Stop/Start (ESS) (V-6)	
	H7 700 CCA (V-8)	
		
Suspension (SXT, GT, R/T, Citadel)	
Front	Short- and long-arm independent (SLA), coil springs, gas-charged, twin-tube 
coil-over shock absorbers, steel upper- and aluminum lower-control arms 
(“A” arms), aluminum knuckle, stabilizer bar	
Rear	Multi-link rear suspension, coil spring, twin tube shocks (including load leveling 
for towing), aluminum lower control arm, independent upper links (tension and camber) plus a separate toe link	
Suspension (SRT)		
Front  	SRT-tuned short- and long-arm independent (SLA) with aluminum lower control arm, aluminum knuckle, aluminum clevis, coil springs, Bilstein adaptive damping suspension (ADS), upper- and lower-control arms (“A” arms), hollow stabilizer bar	
Rear 	SRT-tuned multi-link rear suspension, coil spring, Bilstein adaptive damping suspension (ADS), aluminum lower control arm, independent upper links 
(tension and camber) plus a separate toe link, hollow stabilizer bar	

STEERING		
Steering Ratio	16.7 	
Lock-to-Lock Steering Wheel Rotations	3.2 	
		
BRAKES		
Type	Power-assisted, anti-lock braking system (ABS)	
Front		
Rotor size and type	13.0 x 1.26 (330 x 32) vented disc (V6)	
	13.8 x 1.26 (350 x 32) vented disc (V8)	
	15.0 x 1.34 (380 x 34) vented disc (SRT)	
Caliper size and type	1.89 (48) two-piston pin-slider caliper	
	1.57 (40) Brembo six-piston fixed caliper (SRT)	
Swept area, (sq. in. / sq. cm)	305 (1,969) (V6) 	
	324 (2,088) (V8)	
	413 (2,666) (SRT)	
	
Rear		
Rotor size and type	13.0 x 0.55 (330 x 14) solid disc (V6) 	
	13.0 x 0.87 (330 x 22) vented disc (V8)	
	13.78 x 1.10 (350 x 28) disc (SRT)	
Caliper size and type	1.89 (48) single-piston floating caliper	
	1.34 (34) Brembo four-piston fixed caliper (SRT)	
Swept area, (sq. in. / sq. cm)	257 (1,658)	
	316 (2,039) (SRT)	
		
Dimensions and Capacities		
Wheelbase	119.8 (3,042)	
Track, Front	63.9 (1,623)	
Track, Rear	64.1 (1,627)	
Overall Length	201.2 (5,110)	
Overall Width (Width at Mirrors)	85.5 (2,172)	
Body Width	75.8 (1,924)	
Overall Height (at Roof Rail / at Antenna)	70.9 (1,800.5) / 72.7(1,847), R/T, SRT – 71.9 (1,827)	
Load Floor Height	32.2 (817), R/T, SRT – 31.4 (797.6)	
Sill Step Height	20.5 (521.5), R/T, SRT – 19.7 (500.4)	
Ground Clearance (with P265/60R18 Tire and 3.6 litre engine)	8.1 (207) 	
Chassis (Fuel Tank) 	10.0 (254)	
Front Axle	9.6 (243.2)	
Rear Axle	10.1 (256)	
Approach Angle (degrees)	16.3 	
Ramp Breakover Angle (degrees)	18.1	
Departure Angle (degrees)	21.5 	
Frontal Area	31.0 sq. ft. (2.88 sq. m)	
Drag Coefficient 	0.35	
Fuel Tank Capacity	24.6 gal. (93.1 litre)	
		
Accommodations		
Seating Capacity 
(front/second/third rows)	2/3/2 (standard on SXT, GT, R/T and Citadel), 2/2/2 (standard on SRT model and Citadel Anodized Platinum; available on SXT, GT, R/T and Citadel)	
	
Front		
Headroom	39.9 (1,013)	
Legroom	40.3 (1,025)	
Shoulder Room	58.5 (1,486)	
Hip Room	57.0 (1,449)	
Seat Travel	11.0 (280) driver, 9.0 (230) passenger	
SAE Front Volume Index	54.4 cu. ft. (1.54 cu. m)	
Second Row		
Headroom	39.8 (1,011)	
Legroom	38.6 (981)	
Shoulder Room	50.4 (1,281)	
Hip Room 	42.8 (1,088)	
SAE Volume	44.8 cu. ft. (1.27 cu. m)	
Third Row 		
Headroom	37.8 (960)	
Legroom	31.5 (800)	
Shoulder Room	50.4 (1,281)	
Hip Room 	42.8 (1,088)	
SAE Volume	34.7 cu. ft. (0.98 cu. m)	
SAE Cargo Volume		
Behind Third Row	17.2 cu. ft. (0.49 cu. m)	
Behind Second Row	47.7 cu. ft. (1.35 cu. m)	
Behind Front-row Seats with 
Rear Seats Folded	84.5 cu. ft. (2.39 cu. m)	

WEIGHTS (Estimates)		
	MODEL	ENGINE	GVWR lbs. (kg)	CURB WEIGHT lbs. (kg)	PAYLOAD lbs. (kg)	
AWD	SXT 	3.6-litre	6,500 (2,948)	4,814 (2,184)	1,460 (660)	
	GT	3.6-litre	6,500 (2,948)	4,985 (2,261)	1,350 (610)	
	Citadel	3.6-litre
5.7-litre	6,500 (2,948)
7,100 (3,221)	5,088 (2,308)
5,417 (2,457)	1,390 (630)
1,390 (630)	
	R/T	5.7-litre	7,100 (3,221)	5,381 (2,441)	1,300 (590)	
	SRT	6.4-litre	7,100 (3,221)	5,510 (2500)	1,160 (528)	

Wheels		
Availability	Standard — SXT 	
Type and Material	Painted machine cast-aluminum, 10-spoke Satin Carbon	
Size (inches)	18 x 8	
		
Availability	Standard — GT and Blacktop Package	
Type and Material	Polished machined cast-aluminum, 10-spoke	
	(Hyper Black on GT and Gloss Black on Blacktop Package)	
Size (inches)	20 x 8	
		
Availability	Standard — Brass Monkey Appearance Package available on GT and R/T 	
Type and Material	Painted machined cast-aluminum, 10-spoke 	
	(Burnished Bronze on Brass Monkey Appearance Package and Low Gloss Granite Crystal on R/T)	
Size (inches)	20 x 8	
		
Availability	Standard — Citadel and Anodized Platinum Appearance Package	
Type and Material	Polished (Satin Carbon on Anodized Platinum Appearance Package and polished aluminum on Citadel) machined cast-aluminum, 10-spoke 	
Size (inches)	20 x 8	
		
Availability	Standard — SRT	
Type and Material	Forged aluminum, polished, five-spoke Black Noise Finish	
Size (inches)	20 x 10	
		
Availability	Optional — SRT 	
Type and Material	Forged aluminum, fully painted black, split five-spoke, “Black Noise” Finish	
Size (inches)	20 x 10	
		
Parking Brake Type	Rear, mechanical, drum-in-hat	
Power Assist	Single-rate, tandem diaphragm vacuum	
Four–wheel Anti-lock Brakes	Standard	
Electronic stability control	Standard	
All-speed traction control	Standard	
Brake Assist	Standard	
		
TIRES 		
Availability 	Available — SXT 	
Size and Type	P265/60R18	
Mfr. and Model 	Kumho Crugen Black Sidewall All-season	
		
Availability 	Standard — GT, R/T and Citadel	
Size and Type 	P265/50R20	
Mfr. and Model 	Bridgestone Ecopia H/L 422 Plus Black Sidewall All-season	
		
Availability 	Optional — R/T	
Size and Type 	P265/50R20	
Mfr. and Model 	Pirelli Scorpion Verde Black Sidewall All-season Performance	
		
Availability	Standard — SRT 	
Size and Type	P295/45ZR20	
Mfr. and Model	Pirelli Scorpion Verde  — All-season Performance (run flat)	
Revs per Mile	699	
		
Availability	Optional — SRT 	
Size and Type 	P295/45ZR20	
Mfr. and Model	Pirelli P-Zero  — Three-season (run flat)	
Revs per Mile	699	
		
Parking Brake Type	Drum-in-hat	
Four–wheel Anti-lock Brakes	Standard	
Electronic stability control	Standard	
All-speed traction control	Standard	
Brake Assist	Standard	

TRAILER TOWING: must have optional towing package to achieve maximum towing capacity 	
	Engine	Axle Ratio	Maximum Trailer Weight lbs. (kg)	
AWD 	3.6-litre V-6
5.7-litre V-8
6.4-litre V-8	3.45 
3.09
3.70	6,200 (2812)
7,200 (3265)
8,700 (3946)	

////