FCA CANADA
2018 Dodge Journey
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

General Information		
Body Style	Four-door; seven-passenger	
Assembly Plant	Toluca Assembly, Mexico	
EnerGuide Vehicle Class	Sport-utility vehicle	
Introduction date	Third quarter 2017 as a 2018 model	
	
BODY/CHASSIS	
Layout	Transverse front engine, front-wheel drive or all-wheel drive	
Construction	Steel unibody	
		
Engine: 2.4-litrE dohc 16-valve, vvt, smpi i-4	
Availability	CVP, SE Plus	
Type and Description	Four cylinders in-line, tuned intake manifold with dual counter-rotating balance shafts and dual variable-valve timing	
Displacement	144 cu. in. (2,360 cu. cm)	
Bore x Stroke	3.46 x 3.82 (88 x 97)	
Compression Ratio	10.5:1	
Power (SAE net, estimated)	173 hp (129 kW) @ 6,000 rpm (71 hp/litre)	
Torque (SAE net, estimated)	166 lb.-ft. (225 N•m) @ 4,000 rpm	
Maximum Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity	4.5 quarts with filter (4.26 litres) SAE 5W-20	
Coolant Capacity	7.9 quarts (7.5 litres) — single-zone climate control 	
Emission Controls	Single catalytic converter, dual heated oxygen sensors 
and internal engine features	
	
EnerGuide Fuel Consumption Ratings 
L/100km (imp. mpg) (city/hwy/combined)	TBD	
Based on 2018 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information please visit the government of Canada website www.vehicles.nrcan.gc.ca	
Engine Assembly Plant	Dundee Engine Plant, Dundee, Mich., USA	
	
Engine: 3.6-litrE V-6 dohc 24-valve, vvt	
Availability	SXT, Crossroad, GT	
Type and Description	60-degree bank angle, liquid-cooled, three-plenum intake manifold with electronically controlled manifold tuning valve and short-runner valves 	
Displacement	220 cu. in. (3,605 cu. cm) 	
Bore x Stroke	3.78 x 3.19 (96 x 81)	
Compression Ratio	10.2:1	
Valve System	DOHC, 24 valves, hydraulic, centre-pivot roller rocker arms 	
Fuel Injection	  Sequential, multiport, electronic 	
Power (SAE net, estimated)	283 hp (211 kW) @ 6,350 rpm (67.1 hp/litre)	
Torque (SAE net, estimated)	260 lb.-ft. (353 N•m) @ 4,400 rpm 	
Maximum Engine Speed	6,800 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2 	
	Ethanol E85	
Oil Capacity	5.5 quarts with filter (5.2 litres) SAE 10W-30 MAF 	
Coolant Capacity	10.6 quarts (10 litres) — single- or dual-zone climate control 	
	11.6 quarts (11 litres) — tri-zone climate control	
Emission Controls	Three-way catalytic converter, electronic EGR, 
and internal engine features	
EnerGuide Fuel Consumption Ratings 
L/100km (imp. mpg) (city/hwy/combined)	TBD FWD; TBD AWD	
Based on 2018 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information please visit the government of Canada website www.vehicles.nrcan.gc.ca	
Engine Assembly Plant	Trenton Engine Plant, Trenton, Mich.	

Transmission: 40TES Automatic four-speed overdrive	
Availability	CVP, SE Plus with 2.4-litre engine	
Description	Four-speed overdrive, adaptive electronic control, 
electronically modulated converter clutch	
Gear Ratios		
1st	2.842	
2nd	1.57	
3rd	1.0	
4th	0.69	
Reverse	2.21	
Final-drive Ratio	4.28	
Overall Top-gear	2.95	
	
Transmission: 62te/62tea Automatic six-speed overdrive	
Availability	SXT, Crossroad, GT with 3.6-litre V-6	
Description	Six-speed, adaptive electronic control and electronically 
modulated torque converter clutch	
Gear Ratios		
1st	4.127	
2nd	2.842	
3rd	2.283	
4th	1.452 — Upshift 	
	1.570 — WOT kickdown	
5th	1.00	
6th	0.690	
Reverse	3.214	
Transfer Ratio	0.95	
Final-drive Ratio	3.16	
Overall Top-gear	2.06	

	
	
Drivetrain 	
Front-wheel Drive		
Availability	CVP, SE Plus, SXT, Crossroad	
All-wheel Drive		
Availability	SXT, Crossroad, GT with 3.6-litre V-6	
Type	Electronically controlled coupling (ECC) with variable torque output	
Rear Differential	Open	
	
Electrical System	
Alternator	160-amp — Standard on all Journey models	
Battery	525-amp maintenance-free	
	
Suspension	
Front	Independent MacPherson strut, coil spring over gas-charged shock absorbers, stabilizer bar with isolated suspension cradle	
Rear	Multi-link independent with coil springs, link-type stabilizer bar, 
gas-charged shock absorbers and isolated rear suspension cradle	
	
STEERING	
Type	Power rack and pinion	
Overall Ratio	16.45	
Turning Diametre (curb-to-curb) (ft./m)	38.5 (11.7) — 17-in. wheels and tires 	
	39.0 (11.9) — 19-in. wheels and tires	
Steering Turns (lock-to-lock)	2.92	
P/S pump	Hydraulic	
	
BRAKES	
Front		
Rotor size and type	13.0 x 1.1 (330 x 28) vented rotor	
Caliper size and type	2.0 (51.0) two-piston floating caliper	
Swept area, (sq. in. / sq. cm)	73.6 (475)	
Rear		
Rotor size and type	12.9 x 0.47 (328 x 12) solid rotor	
Caliper size and type	1.8 (45.0) single-piston floating caliper	
Swept area, (sq. in. / sq. cm)	66.5 (429)	
	
Dimensions and Capacities	
Wheelbase	113.8 (2,889.8)	
Overhang — Front	38.9 (989.3)	
Overhang — Rear	39.7 (1,008.5)	
Track — Front	61.8 (1,570.8)	
Track — Rear	62.3 (1,581.8)	
Overall Length	192.4 (4,887.6)	
Overall Width	72.2 (1,834.5)	
Overall Width with Mirrors 	83.7 (2,127.0)	
Overall Height	66.6 (1,692.6)	
Vehicle Height including Roof Rack Assembly	69.5 (1,765.2)	
Drag Coefficient (Cd)	0.368	
Fuel Tank Capacity, gallons (litres)	2.4-litre and 3.6-litre FWD — 20.5 (77.6)	
	3.6-litre AWD — 21.1 (79.87)	
Gross Vehicle Weight Rating (GVWR), lbs. (kg) 		
Seven-passenger vehicle, FWD 2.4-litre	5,250 (2,381)	
Seven-passenger vehicle, FWD 3.6-litre	5,475 (2,483)	
Seven-passenger vehicle, AWD 3.6-litre	5,600 (2,540)	
Towing Capabilities, lbs. (kg) 		
2.4-litre I-4 with Automatic Transaxle	1,000 (450)	
3.6-litre V-6 with Automatic Transaxle, 
FWD or AWD	2,500 (1,135)	
	
Accommodations	
Seating Capacity (front/second/third rows)	2/3/2 standard	
EPA Volume Index, cu. ft. (cu. m)	134.552 (3.810) – five-passenger	
	133.975 (3.794) – seven-passenger 	
Total Interior Passenger Compartment Volume, 
cu. ft. (cu. m)	99.614 (2.821) – five-passenger	
	123.701 (3.503) – seven-passenger	
Front row		
Headroom without Sunroof	40.8 (1,036.3)	
Headroom with Sunroof	39.2 (995.0)	
Legroom	40.8 (1,036.3)	
Shoulder Room	57.5 (1,459.7)	
Hip Room	53.8 (1,366.5)	
Seat Travel	10.23 (260)	
Front Compartment Volume, cu. ft. (cu. m)	55.39 (1.57)	
Second row	
Headroom without Sunroof	39.9 (1,013.0)	
Headroom with Sunroof	39.2 (994.8)	
Legroom	36.1 (916.7)	
Couple, First to Second Row	30.5 (773.8)	
Shoulder Room	56.9 (1,444.4)	
Hip Room	54.4 (1,381.9)	
EPA Rear Seat Volume Index or Third row Volume, (cu. ft. / cu. m) 	44.1 (1.2)	
Third row 		
Headroom	37.7 (957.4)	
Legroom	23.4 (595.5)	
Couple, Second to Third Row	30.1 (765.1)	
Shoulder Room	43.5 (1,104.9)	
Hip Room	40.0 (1,016.3)	
Rear Passenger Volume, (cu. ft. / cu. m)	22.2 (0.63)	
Cargo Width @ Wheelhouse	41.4 (1,050.5)	
Trunk Liftover Height	30.8 (782.4)	
	
Cargo Volume				
Behind First-Row Seat, cu. ft. (cu. m)	67.6 (1.915)	
Behind Second-Row Seat, cu. ft. (cu. m) 	37.0 (1.0)	
Behind Third-Row Seat, cu. ft. (cu. m)	10.7 (0.3)	
	
Wheels	
Availability	Available — CVP	
Type and Material	Steel with wheel covers 	
Size	17 x 6.5	
		
Availability	Standard — CVP and SE Plus	
Type and Material	Machined cast-aluminum, five-spoke	
Size	17 x 6.5	
		
Availability	Standard — SXT	
Type and Material	Machined cast-aluminum, twin five-spoke	
Size	17 x 6.5	
		
Availability	Standard — GT		
	Optional — SXT	
Type and Material	Machined cast-aluminum, 10-spoke Tech Silver 
(Optional – SXT) or Gloss Black finish (SXT Blacktop package)	
Size	19 x 7.0	
	
Availability		Standard — Crossroad		
Type and Material	Machined cast-aluminum, five-spoke Black finish 	
Size	19 x 7.0	
		
Availability	Optional — GT	
Type and Material	Chrome-clad cast-aluminum, six-spoke	
Size	19 x 7.0	
		
Availability	Standard — all models	
Type and Material		Temporary spare steel wheel	
		
Tires	
Availability	Standard — CVP, SE Plus and SXT	
Size and Type	P225/65R17, All-season Touring	
Model	Kumho Solus KH16	
Revs per Mile (km)	725 (471)	
		
Availability	Standard — Crossroad and GT	
Size and Type	225/55R19, All-season Touring	
Model	Kumho Solus KH16	
Revs per Mile (km)	711 (444)	
		
Availability	Standard — all Journey models	
Size and Type	T145/70R17 temporary spare tire	
		
Parking Brake Type	Standard — all Journey models	
Power-assist Type	9 x 9 (230 x 230) tandem-diaphragm vacuum	
Four–wheel Anti-lock Brakes	Standard	
Electronic Stability Control	Standard	
All-speed Traction Control	Standard	
Brake Assist	Standard	

////