FCA CANADA
2018 Fiat 124 Spider
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION	
Body Style 	Roadster 	
Assembly Plant	Hiroshima, Japan	
EnerGuide Vehicle Class 	Two-seater	
Introduction Date	Summer 2016 as a 2017 model	
	
BODY AND CHASSIS	
Layout	Monocoque unibody; front and rear suspension subframes	
Construction 	High-tensile strength steel body to improve rigidity; double-wishbone suspension at the front and multi-link at the rear; sport suspension	

ENGINE: 1.4-LITRE TURBOCHARGED MULTIAIR I-4	
Availability	Standard	
Type and Description	In-line four-cylinder, liquid-cooled, turbocharged	
Displacement	83.48 cu. in. (1,368 cc) 	
Bore x Stroke	2.83 x 3.31 (72.0 x 84.0)	
Valve System	Belt-driven, MultiAir, SOHC, 16 valves,hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Cast-iron block with aluminum-alloy head and aluminum-alloy bedplate	
Compression Ratio	9.8:1	
Maximum Turbo Boost (psi / bar)	22 psi / 2.49 bar	
Power (SAE)	160 hp (119 kW) @ 5,500 rpm (Classica and Lusso)
164 hp (123 kW) @ 5,500 rpm (Abarth)	
Torque (SAE)	184 lb.-ft. (250 N•m) @ 2,500 rpm (Abarth in sport mode)
184 lb.-ft. (250 N•m) @ 3,200 rpm (Classica, Lusso, Abarth)	
Max. Engine Speed	6,250 rpm (electronically limited)	
Fuel Requirement	87 octane (R+M)/2 acceptable 
91 octane recommended	
Oil Capacity	4.0 qt. (3.8 litre) with dry filter	
Coolant Capacity
		7.6 qt. (7.2 litre) six-speed manual
7.5 qt. (7.1 litre) six-speed automatic	
Emission Controls 	Three-way catalytic converter, heated oxygen sensors and internal engine features	
EnerGuide Fuel Consumption Ratings
L/100km (imp. mpg) (city/hwy/combined)	TBD six-speed manual transmission
TBD six-speed automatic transmission	
Based on 2018 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information please visit the government of Canada website www.vehicles.nrcan.gc.ca	
Towing	Not recommended 	
Engine Assembly Plant	Termoli, Italy	
		
B400 AISIN SIX-SPEED AUTOMATIC TRANSMISSION 	
Availability	Classica, Lusso, Abarth	
Description 	Planetary gear train, longitudinal layout
Paddle-shifted driver-interactive manual control (Abarth)	
Gear Ratios		
1st	3.53	
2nd	2.06	
3rd	1.40	
4th	1.00	
5th	0.71	
6th	0.58	
Reverse	3.16	
Axle Ratios	3.583	
Mechanical limited-slip differential	Standard on Abarth	
		
C635 SIX-SPEED MANUAL TRANSMISSION		
Availability	Classica, Lusso, Abarth	
Description	1st, 2nd, 3rd, 4th gear: Triple cone 	
	
Gear Ratios		
1st	4.363	
2nd	2.348	
3rd	1.647	
4th	1.262	
5th	1.000	
6th	0.844	
Reverse	3.863	
Final-drive Ratio	3.454	
Mechanical limited slip differential	Standard on Abarth	
		
ELECTRICAL SYSTEM		
Alternator 	Denso SC2 150 A with LIN regulator	
Battery	Q85	
		
SUSPENSION		
Front 	Double-wishbone front with stabilizer bars
Tower strut bar (Abarth)	
Rear	Multi-link rear with stabilizer bars	
		
STEERING		
Type 	Double pinion electric power assist system (DP-EPAS) – 
rack-and-pinion	
Overall Ratio 	15.5 	
Turning Diametre (curb-to-curb) 	30.8 ft. (9.4 m)	
Steering Turns (lock-to-lock)	2.7	
		
BRAKES		
Availability	Standard: Classica, Lusso, Abarth	
Front	Ventilated front disc	
Size and Type	11-in. floating	
Swept Area (per caliper)	10.5 sq. in. (67.8 sq. cm)	
Rear	Solid rear disc	
Size and Type 	11-in. floating	
Swept Area (per caliper)	9.8 sq. in. (63.0 sq. cm)	
		
Availability	Optional: Abarth	
Front	Brembo ventilated front disc	
Size and Type	11-in. opposed	
Swept Area (per caliper)	18.6 sq. in. (120 sq. cm)	
Rear	Solid rear disc	
Size and Type 	11-in. floating	
Swept Area (per caliper)	9.8 sq. in. (63.0 sq. cm)	
Power-assist Type 	Vacuum booster	
Four-wheel anti-lock brake system (ABS)	Standard	
Electronic stability control (ESC)	Standard	
Parking Brake Type	Mechanical (lever type)　	
		
DIMENSIONS AND CAPACITIES		
Wheelbase	90.9 (2,309)	
Track, Front	58.9 (1,496)	
Track, Rear	59.1 (1,503)	
Overall Length	159.6 (4,054)	
Overall Width	68.5 (1,740)	
Overall Height 	48.5 (1,232) 	
Approach angle, degrees	13.1	
Curb Weight, pounds (kg)	2,436 (1,105) six-speed manual (Classica, Lusso)
2,477 (1,124) six-speed manual (Abarth)
2,476 (1,123) six-speed automatic (Classica, Lusso)
2,516 (1,141) six-speed automatic (Abarth)	
Fuel-tank Capacity	9.9 imp. gal. (45 litres)	

ACCOMMODATIONS		
Seating Capacity — Front 	2	
Head Room 	37.4 (950)	
Legroom 	43.1 (1,096)	
Shoulder Room 	52.1 (1,325)	
Hip Room	52.0 (1,320)	
Seat Travel 	8.3 (210) driver / 6.7 (170) passenger 	
Recliner Range (degrees)	From 25 nominal, 12 forward and 22 rearward	
Cargo space, cu. ft. 	4.94 (140 litre)	
		
TIRES		
Availability	Standard: Classica	
Size and Type 	195/50R16 three-season	
Mfr. and Model 	Yokohama Advan Sport V105	
Revs per Mile (km)	879 (1,414.6)	
		
Availability	Standard: Lusso and Abarth	
Size and Type 	205/45R17 three-season	
Mfr. and Model 	Bridgestone Potenza S001 (Lusso)
Bridgestone Potenza RE-050A (Abarth)		
Revs per Mile (km)	856 (1,377.6)	

////