FCA CANADA
2018 Fiat 500L
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION	
Vehicle Type	B-segment multipurpose vehicle (MPV)	
EPA Vehicle Class	Small Station Wagon	
Assembly Plant	Kragujevac, Serbia	
Introduction Date	Mid-2013 as a 2014 model	
	
BODY AND CHASSIS	
Layout	Transverse-mounted front engine, front-wheel drive	
Construction	Unitized steel body 	
	
ENGINE: 1.4-LITRE SOHC 16-VALVE TURBOCHARGED MULTIAIR INLINE FOUR-CYLINDER	
Availability	Standard — all 500L models	
Type and Description	Inline four-cylinder, liquid-cooled, turbocharged	
Displacement	83.48 cu. in. (1,368 cu. cm)	
Bore x Stroke	2.83 x 3.31 (72 x 84)	
Valve System	Belt-driven, MultiAir, SOHC, 16 valves, hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Cast-iron block with aluminum-alloy head and aluminum-alloy bedplate	
Compression Ratio	9.8:1	
Maximum Turbo Boost (psi / bar)	21 psi / 1.45 bar	
Power (SAE)	160 hp (119 kW) @ 5,500 rpm	
Torque (SAE)	184 lb.-ft. (250 N•m) @ 2,500-4,000 rpm	
Max. Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	87 octane (R+M)/2 acceptable 
91 octane recommended	
Oil Capacity	4.0 quarts  (3.8 litres) with dry filter	
Coolant Capacity	4.6 quarts  (14.4 litres)	
Emission Controls 	Three-way catalytic converters, heated oxygen sensors and internal engine features	
Max. Gross Trailer Weight	Not rated for trailer tow	
EnerGuide Fuel Consumption Ratings
L/100km (imp. mpg) (city/highway/combined)	10.7 (26) / 7.9 (36) / 9.4 (30) 	
Based on 2018 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information please visit the government of Canada website www.vehicles.nrcan.gc.ca	
Engine Assembly Plant	Termoli, Italy	
		
AISIN SIX-SPEED AUTOMATIC TRANSMISSION	
Availability	Standard — all 500L models	
Gear Ratios		
1st	4.04	
2nd	2.37	
3rd	1.56	
4th	1.16	
5th	0.85	
6th	0.67	
Reverse	3.19	
Final-drive Ratio	3.683	
Overall Top Gear	2.47	
Steering Turns (lock-to-lock)	3.0	
		
BRAKES		
Availability	Standard — all 500L models	
Front		
Rotor size and type	12.0 x 1.10 (305 x 28) vented	
Caliper size and type	2.24 (57) single-piston with cast iron	
Swept area	345 sq. in. (876.1 sq. cm)	
Rear		
Rotor size and type	10.4 x 0.4 (264 x 10) solid	
Caliper size and type	1.49 (38) single-piston with aluminum housing	
Swept area	233 sq. in. (591.8 sq. cm)	
		
DIMENSIONS AND CAPACITIES		
Wheelbase	102.8 (2,612)	
Track, Front	59.9 (1,522)	
Track, Rear	59.8 (1,519)	
Overall Length	167.0 (4,242)
168.3 (4,276) — 500L Trekking	
Overall Width

		70.2 (1,784) — without mirrors 
79.4 (2,018) — with mirrors
70.9 (1,800)  — 500L Trekking	
Overall Height	65.3 (1,658) — 500L Sport
66.1 (1,679) — 500L Trekking
66.1 (1,678) — 500L Lounge	
Ground Clearance	4.7 (120) 	
Drag Coefficient (Cd) (estimated)	0.310 — 500L Sport/Lounge
0.320 — 500L Trekking		
Curb Weight, lb. (kg) (estimated)	3,254 (1,476) 	
Weight Distribution, percent F/R	60/40 	
Fuel Tank Capacity, imp. gal. (litre)	10.8 (49)	
		
ACCOMMODATIONS		
Seating Capacity, F/R	2/3	
Front Seat		
Headroom	40.7 (1,034)
40.5 (1,028) with dual-pane sunroof		
Legroom	40.0 (1,015)	
Shoulder room	57.3 (1,456)	
Hip room	54.9 (1,394)	
Total seat travel	8.3 (210) — driver
9.0 (230) — passenger 		
EPA front row interior volume	54.0 cu. ft. (1,529 litres)	
	
Rear Seat		
Headroom	38.7 (983)
38.0 (966) with dual-pane sunroof		
Legroom	36.7 (931)	
Shoulder room	54.6 (1,388)	
Hip room	49.4 (1,256)	
Total seat travel	4.7 (120)	
EPA second row interior volume	44.8 cu. ft. (1,268 litres)	
Total Interior Volume	98.8 cu. ft. (2,797 litres)	
EPA Luggage Compartment Volume	22.4 cu. ft. (633 litres)	
EPA Volume behind front row 
(maximum cargo)	68.0 cu. ft. (1,927 litres)	
EPA Interior Volume Index	121.1 cu. ft. (3,430 litres)	
Trunk Liftover Height	25.9 (657)	
		
TIRES		
Availability 	Standard — 500L Sport 	
Size and Type	205/55R16 BSW All-season 	
Mfr. and Model	Continental Conti ProContact or Goodyear Eagle LS2 or Nexen CP671 Classe Premiere	
Revs per mile (km)	836 (519)	
		
Availability	Standard — 500L Trekking and 500L Lounge		
Size and Type	225/45R17 BSW All-Season	
Mfr. and Model	Continental Conti ProContact or Goodyear Eagle LS2 or Nexen CP671 Classe Premiere	
Revs per mile (km)	832 (517)	

////