FCA CANADA
2018 Fiat 500X
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION	
Body Style 	Crossover	
Assembly Plant	Melfi, Italy	
EPA Vehicle Class 	Multipurpose vehicle	
	
BODY AND CHASSIS	
Layout	Transverse front engine	
Construction 	Steel uniframe	

ENGINE: 1.4-LITRE TURBOCHARGED MULTIAIR I-4	
Availability	Standard — Pop (FWD)	
Type and Description	In-line four-cylinder, liquid-cooled, turbocharged	
Displacement	83.48 cu. in. (1,368 cc) 	
Bore x Stroke	2.83 x 3.31 (72.0 x 84.0)	
Valve System	Belt-driven, MultiAir, SOHC, 16 valves,
hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Cast-iron block with aluminum-alloy head and aluminum-alloy bedplate	
Compression Ratio	9.8:1	
Maximum Turbo Boost (psi / bar)	22 psi / 2.49 bar	
Power (SAE)	160 hp (119 kW) @ 5,500 rpm	
Torque (SAE)	184 lb.-ft. (250 N•m) @ 2,500-4,000 rpm	
Max. Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	87 octane (R+M)/2 acceptable 	
	91 octane recommended	
Oil Capacity	4.0 quarts (3.8 litres) with dry filter	
Coolant Capacity	5.5 quarts (5.2 litres)	
Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors and internal engine features	
EnerGuide Fuel Consumption Ratings
L/100km (imp. mpg) (city/hwy/combined)	9.5 (30) / 7.1 (40) / 8.4 (34)	
Based on 2018 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information please visit the government of Canada website www.vehicles.nrcan.gc.ca		
Towing	Not recommended 	
Engine Assembly Plant	Termoli, Italy	
		
ENGINE: 2.4-LITRE MULTIAIR TIGERSHARK 		
Availability	Standard — All models excluding Pop FWD	
	Available — Pop (FWD)	
Type and Description	In-line four-cylinder, 16-valve MultiAir with multiport fuel injection	
Displacement	144 cu. in. (2,360 cc) 	
Bore x Stroke	3.46 X 3.82 (88 X 97)	
Valve System	SOHC, four valves per cylinder 	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Aluminum block, aluminum cylinder head	
Compression Ratio	10:1	
Power (SAE net) 	180 hp (134 kW) @ 6,400 rpm	
Torque (SAE net) 	175 lb.-ft. (237 N•m) @ 3,900 rpm	
Max. Engine Speed	6,400 rpm	
Fuel Requirement	Unleaded regular, 87 octane	
Oil Capacity	5.5 quarts (5.2 litres) (total)	
Coolant Capacity	6.8 quarts (6.45 litres)	
Emission Controls	Single catalytic converter, heated wide band lambda sensor upstream and mid-catalyst heated oxygen sensor	
EnerGuide Fuel Consumption Ratings
L/100km (imp. mpg) (city/hwy/combined)	10.7 (26) / 7.7 (37) 9.3 (30) (FWD)	
	11.0 (26) / 8.0  (35) / 9.7 (35) (AWD)	
Based on 2018 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information please visit the government of Canada website www.vehicles.nrcan.gc.ca	
Towing	1,000 lbs. (454 kg) (not recommended for FWD)	
Engine Assembly Plant 	Dundee Engine Plant, Dundee, Mich., USA	
		
TRANSMISSION: 948TE NINE-SPEED AUTOMATIC	
Availability	2.4-litre MultiAir Tigershark engine (FWD or AWD)	
Description 	Planetary gear train, transverse layout	
Ratio Spread	9.81	
Gear Ratios		
1st	4.71	
2nd	2.84	
3rd	1.91	
4th	1.38	
5th	1.00	
6th	0.81	
7th	0.70	
8th	0.58	
9th	0.48	
Reverse	3.83	
Axle Ratio	3.734	
		
C635 SIX-SPEED MANUAL TRANSMISSION		
Availability	1.4-litre MultiAir Turbo engine 	
Description	1st, 2nd, 3rd gear: Triple cone 	
	4th: Double cone	
Gear Ratios		
1st	4.154	
2nd	2.118	
3rd	1.361	
4th	0.978	
5th	0.756	
6th	0.622	
Reverse	4.00	
Final-drive Ratio	4.438 	
Overall Top Gear	2.38	
Axle Ratio	4.438	
		
ELECTRICAL SYSTEM		
Alternator 	150-amp (1.4-litre MultiAir Turbo) 		
	160-amp (2.4-litre Tigershark with MultiAir)	
Battery	500-amp  (1.4-litre MultiAir Turbo)		
	600-amp (2.4-litre Tigershark with MultiAir)	
SUSPENSION		
Front 	MacPherson strut, coil springs, high-strength steel front cross member, high-strength steel mono shell lower control arms, stabilizer bar	
Rear	Chapman strut, high-strength steel links, isolated steel rear cradle, coil springs, stabilizer bar	
		
STEERING		
Type 	Electric power rack and pinion	
Overall Ratio 	15.7 	
Turning Diametre (curb-to-curb) 	36.3 (11.07) 	
Steering Turns (lock-to-lock)	2.68 	
		
BRAKES		
Front		
Size and Type	12 x 1.1 (305 x 28) vented rotor with 
2.36 (60) single-piston floating caliper	
Swept Area (per caliper)	138.77 sq. in. (895.3 sq. cm), 1 x 60	
Rear		
Size and Type 	10.95 x 0.47 (278 x 12) solid rotor with 
1.5 (38) single-piston floating caliper	
Swept Area (per caliper)	101.7 sq. in. (656.4 sq. cm), 1 x 38	
Power-assist Type 	10 in. (254) vacuum assist 	
Four-wheel anti-lock brake system (ABS)	Standard	
Electronic stability control (ESC)	Standard	
Parking Brake Type	Electric motor on caliper	
		
DIMENSIONS AND CAPACITIES		
Wheelbase	101.2 (2,570)	
Track, Front	60.9 (1,548) front-wheel drive	
	60.7 (1,543) all-wheel drive	
Track, Rear	61.0 (1,549) front-wheel drive	
	60.7 (1,543) all-wheel drive	
Overall Length	167.2 (4,248) Pop, Lounge 	
	168.2 (4,273) Trekking	
Overall Width	75.5 (1,796) with mirrors folded	
	79.7 (2,025) 	
	
Overall Height 	63.1 (1,602) front-wheel drive	
	63.7 (1,617) all-wheel drive	
Load-floor Height	29.8 (758) 	
Sill-step Height	19.4 (494) front, 19.6 (497) rear 	
Ground Clearance	7.0 (178) front-wheel drive		
	7.9 (202) all-wheel drive	
Curb Weight, lb. (kg)	2,989 (1,356) manual transmission	
	3,124 (1,417) automatic transmission, front-wheel drive	
	3,305 (1,499) automatic transmission, all-wheel drive	
Aero Cd	0.350	
Fuel-tank Capacity, imp gallon (litre)	10.6  (48)	
	
ACCOMMODATIONS		
Seating Capacity — F/R	2/3	
Front Row		
Headroom	39.1 (993)	
Legroom	41.4 (1,053) 	
Shoulder Room 	54.3 (1,380)	
Hip Room	53.3 (1,354)	
Seat Travel 	9.0 (230) driver / 10.2 (260) front passenger	
Recliner Range (degrees)	From 25 nominal, 38 forward and 30 rearward 
(from vertical 13 forward, 55 rearward)	
First Row Interior Volume (standard roof), 
cu. ft. (litres)	51.5 cu. ft (1,460)	
Second Row		
Headroom 	37.8 (961) 	
Legroom 	34.8 (883) 	
Shoulder Room	52.8 (1,342) 	
Hip Room	52.2 (1,326)	
Second Row Interior Volume, cu. ft. (litres)	40.2 cu. ft. (1,140) 	
Cargo Access		
Liftover Height	30.5 (774) front-wheel drive	
	31.4 (797) all-wheel drive	
Maximum Cargo Width at Liftgate Opening	41.3 (1,048)	
Minimum Cargo Width at Liftgate Opening	37.1 (943) (at floor)	
Cargo Height 	28.8 (731)	
Rear Opening Height 	26.6 (676)	
Distance Between Wheelhouse Interior Trim	37.8 (960)	
ISO Cargo Volume		
Rear Seats Up, cu. ft. (litres) 	12.2 (350)	
Rear Seats Folded, cu. ft. (litres) 	19.9 (560)	
Rear Seats Folded (to headliner), cu. ft. (litres) 	32.1 (910)	
Consumer Reports Cargo, cu. ft. (litres)	20 (566) 	
		
TIRES		
Availability	Standard — Pop 	
Size and Type 	215/60R16 All-season 	
Mfr. and Model 	Continental, Procontact TX	
		
Availability	Standard — Sport, Trekking, Lounge (FWD)	
Size and Type 	215/55R17 BSW All-season 	
Mfr. and Model 	Continental, Procontact TX or Nexen Class Premiere	
		
Availability	Standard — Sport, Trekking, Lounge (AWD)	
Size and Type 	215/60R17 BSW All-season 	
Mfr. and Model	Nexen Class Premiere 	

////