FCA CANADA
2017 Fiat 500 / 500c
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION	
Vehicle Type	A-segment hatchback (500) or cabrio (500c)	
EPA Vehicle Class	Mini-compact	
Assembly Plant	Toluca, Mexico	
		
BODY AND CHASSIS	
Layout	Transverse-mounted front engine, front-wheel drive (FWD)	
Construction	Unitized steel body 	
	
ENGINE: 1.4-LITRE MULTIAIR I-4	
Availability	Standard — Fiat 500 and 500c Pop and Lounge	
Type and Description	Inline four-cylinder, liquid-cooled	
Displacement	1,368 cu. cm  (83.48 cu. in.)	
Bore x Stroke	72.0 x 84.0 (2.83 x 3.31)	
Valve System	Belt-driven, MultiAir, SOHC, 16 valves, hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Cast iron block with aluminum-alloy heads and aluminum-alloy bedplate	
Compression Ratio	10.8:1	
Power (SAE net)	101 hp @ 6,500 rpm (73.8 bhp/litre)	
Torque (SAE net)	97 lb.-ft. @ 4,000 rpm	
Max. Engine Speed	6,900 rpm (electronically limited)	
Fuel Requirement	87 octane (R+M)/2 acceptable 
91 octane recommended	
Oil Capacity	3.8 litres (4.0 quarts)  with dry filter	
Coolant Capacity	4.4 litres (4.6 quarts) 	
Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors and internal engine features	
Max. Gross Trailer Weight	Not rated for trailer tow	

EnerGuide (2016) Fuel Consumption Ratings L/100 km (MPG – imperial gallon) city/hwy/combined	Fiat 500 Pop and Lounge:
8.5(33) / 6.9(41) / 7.8(36) (five-speed manual) 
8.7(32) / 6.9(41) / 7.9(36) (six-speed automatic)	
	Fiat 500c Pop and Lounge:
7.9(36) / 6.3(45) / 7.2(39) (five-speed manual) 
8.7(32) / 6.9(41) / 7.9(36) (six-speed automatic)	
Based on 2016 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information, please visit the Government of Canada website: www.vehicles.nrcan.gc.ca	
Engine Assembly Plant	Dundee, Mich. USA	

TRANSMISSION: C514 FIVE-SPEED MANUAL	
Availability	Standard — 500 and 500c Pop and Lounge 	
Description	1st, 2nd gear: Double Cone 3rd, 4th, 5th, gear: Single Cone	
Gear Ratios		
1st	3.909	
2nd	2.174	
3rd	1.345	
4th	0.974	
5th	0.766	
Reverse	3.818	
Final-drive Ratio	3.44 (500 and 500c Pop and Lounge)	
Overall Top Gear	2.63 (500 and 500c Pop and Lounge)	
		
TRANSMISSION: AISIN AUTOMATIC SIX-SPEED OVERDRIVE WITH AUTO STICK	
Availability	Optional — 500 and 500c Pop and Lounge 	
Description	Auto Stick driver-interactive manual control and electronically modulated torque converter clutch	
Gear Ratios		
1st	4.044	
2nd	2.371	
3rd	1.556	
4th	1.159	
5th	0.852	
6th	0.672	
Reverse	3.193	
Final Drive Ratio	4.103	
Overall Top Gear	2.76	

ELECTRICAL SYSTEM		
Alternator	105-amp — Standard on 500 Pop (with automatic transmission) and 500c Pop and Lounge 	
	120-amp — Standard on 500 Pop (with manual transmission)	
Battery	500 CCA, maintenance free	
		
SUSPENSION		
Front 	MacPherson suspension, coil spring with twin-tube shock absorbers and 
stabilizer bar 	
Rear	Rear twist-beam axle with coil springs and twin-tube shock absorbers 	
		
STEERING		
Type	Power rack and pinion with electric power steering (EPS) column	
Overall Ratio	16.3:1	
Turning Diameter (curb-to-curb)	9.32 m (30.6 ft.) 	
Steering Turns (lock-to-lock)	3.0	

BRAKES		
Availability	Standard — 500 and 500c Pop and Lounge	
Front		
Rotor size and type	257 x 22 (10.1 x 0.86) vented	
Caliper size and type	54 (2.12) single-piston with aluminum housing	
Swept area	1,244 sq. cm  (193 sq. in.) 	
Rear		
Rotor size and type	240 x 11 (9.4 x 0.4) solid	
Caliper size and type	34 (1.33) single-piston with aluminum housing	
Swept area	984 sq. cm (153 sq. in.) 	
		
DIMENSIONS AND CAPACITIES(D)		
Wheelbase	2,300 (90.6) 	
Track, Front	500 — 1,406.8 (55.4) 
500c — 1,406.8 (55.4) 		
Track, Rear	500 — 1,397.0 (55.0) 
500c — 1,397.0 (55.0) 		
Overall Length	500 — 3,546.7 (139.6)
500c — 3,546.7 (139.6) 		
Overall Width	1,627.0 (64.1)	
Overall Height
	500 — 1,519 (59.8) 
500c — 1,519 (59.8) 	
Ground Clearance	500 Pop — 114 (4.5) 
500 Lounge — 114 (4.5)
500c — 118.0 (4.6)		
Drag Coefficient (Cd)	500 Pop — 0.332
500 Lounge — 0.359
500c Pop and Lounge — 0.364		
Curb Weight, kg (lb.)		500 with five-speed manual — 1,074 (2,366) 
500 with six-speed automatic — 1,112 (2,452) 
500c with five-speed manual — 1,099 (2,424) 
500c with six-speed automatic — 1,139 (2,511)		
Weight Distribution, % F/R	500 with five-speed manual — 63/37 
500 with six-speed automatic — 65/35 
500c with five-speed manual — 62/38
500c with six-speed automatic — 64/36		
Fuel Tank Capacity, litres 
(imperial gallons)	40 (8.8) 	
(d) All dimensions measured at curb weight with standard tires.	

ACCOMMODATIONS		
Seating Capacity, F/R	2/2	
Front Seat		
Headroom	500 —989.1 (38.9) 
500 with sunroof — 956.3 (37.6) 
500c — 980 (38.6) 		
Legroom	1,034.8 (40.7) 	
Shoulder room	1,254.8 (49.4) 	
Hip room	1,215 (47.9) 	
Total seat travel	Driver — 210.0 (8.2) 
Passenger — 210.0 (8.2)		
EPA front row interior volume	500 — 1,283 litres (45.3 cu. ft.) 
500c — 1,217litres (44.9 cu. ft.) 		

Rear Seat		
Headroom	500 — 904 (35.6)
500c — 935 (36.8) 		
Legroom	805.1 (31.7) 	
Shoulder room	1,177.5 (46.4) 	
Hip room	1,083.1 (42.6) 	
EPA second row interior volume	500 — 855 litres (30.2 cu. ft.) 
500c — 866 litres (31.3 cu. ft.)  	
Total Passenger Interior Volume	500 — 2,138 litres (75.5 cu. ft.) 
500c — 2,158 litres (76.2 cu. ft.)  	
EPA Luggage Compartment Volume	500 — 269 litres (9.5 cu. ft.) 500c — 153 litres (5.4 cu. ft.) 	
EPA Interior Volume Index	500 — 2,404 litres (84.9 cu. ft.)
500c — 2,311 litres (81.6 cu. ft.) 	
Trunk Liftover Height	703.6 (27.7)	
		
WHEELS	
Availability 	Standard — 500 and 500c Pop	
Type and material	Steel wheels with wheel covers	
Size	15 x 6.0	
		
Availability 	Optional — 500 Pop	
Type and material	Cast-Aluminum Hyper Black	
Size	16 x 16.5	
		
Availability 	Optional — 500c Pop	
Type and material	Cast-aluminum Tech Silver 	
Size	15 x 6.0	
		
Availability	Standard — 500 and 500c Lounge	
Type and material	Cast-aluminum, nine split-spoke design Satin Carbon	
Size	15 x 6.0	
		
Availability	Optional on 500 and 500c Lounge	
Type and material	Cast-aluminum, polished face with Tech Silver painted pockets 	
Size	16 x 6.5	
		
TIRES		
Availability 	Standard — 500 and 500c Pop and Lounge	
Size and type	185/55R15 BSW All-season 	
Mfr. and model	Continental ContiProContact or Firestone Firehawk GTH or Pirelli Cinturato P7 A/S	
Revs per kilometre (mile)	563 (906) 	
		
Availability 	Optional — 500 and 500c Pop and Lounge	
Size and type	195/45R16 XL 84V BSW All-season 	
Mfr. and model	Pirelli Cinturato P7 A/S	
Revs per kilometre (mile)	560 (901) 	

////