FCA CANADA
2018 Jeep® Compass
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION	
Body Style 	Sport Utility Vehicle (SUV)	
Assembly Plant	Toluca, Mexico	
Energuide Vehicle Class 	Multipurpose vehicle	
	
BODY AND CHASSIS	
Layout	Transverse front engine, 4x2 and 4x4	
Construction 	Steel uniframe	
	
ENGINE: 2.4-PZEV TIGERSHARK WITH MULTIAIR	
Availability	Standard — All Models	
Type and Description	In-line four-cylinder, 16-valve MultiAir with multiport fuel injection	
Displacement	144 cu. in. (2,360 cc) 	
Bore x Stroke	3.46 X 3.82 (88 X 97)	
Valve System	SOHC, four valves per cylinder 	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Aluminum block, aluminum cylinder head	
Compression Ratio	10:1	
Power (SAE net) 	180 hp (134 kW) @ 6,400 rpm	
Torque (SAE net) 	175 lb.-ft. (237 N•m) @ 3,900 rpm	
Max. Engine Speed	6,400 rpm	
Fuel Requirement	Unleaded regular, 87 octane	
Oil Capacity	5.5 quarts (5.2 litres) (total)	
Coolant Capacity	6.8 quarts (6.45 litres)	
Emission Controls	Single catalytic converter, heated wide band lambda sensor upstream and mid-catalyst heated oxygen sensor	
EnerGuide Fuel Consumption Ratings
L/100km (imp. mpg) (city/hwy/combined)	10.4 (27) / 7.3 (39) (FWD, MTX)	
	10.8 (26) / 7.6 (37) (AWD, MTX)	
	10.6 (27) / 7.6 (37) (FWD, ATX)	
	10.8 (26) / 7.8 (36)  (AWD, ATX)	
Based on 2018 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information please visit the government of Canada website www.vehicles.nrcan.gc.ca	
Towing	2,000 lbs. (907 kg) (not recommended for FWD)	
Engine Assembly Plant 	Saltillo Engine Plant, Saltillo, Mexico	
	
TRANSMISSION: 9HP48 NINE-SPEED AUTOMATIC	
Availability	2.4-litre Tigershark engine with MultiAir (4x4)	
Description 	Planetary gear train, transverse layout	
Ratio Spread	9.81	
Gear Ratios		
1st	4.71	
2nd	2.84	
3rd	1.91	
4th	1.38	
5th	1.00	
6th	0.81	
7th	0.70	
8th	0.58	
9th	0.48	
Reverse	3.81	
Final-drive Ratio	3.734	
	4.334 (Trailhawk)	
		
C635 SIX-SPEED MANUAL TRANSMISSION		
Availability	2.4-litre Tigershark engine with MultiAir (Sport)	
Description	Planetary gear train, transverse layout	
Gear Spread	6.635	
	
Gear Ratios		
1st	4.459	
2nd	2.508	
3rd	1.556	
4th	1.142	
5th	0.852	
6th	0.672	
		
AT6 AISIN SIX-SPEED AUTOMATIC TRANSMISSION	
Availability	2.4-litre Tigershark engine with MultiAir (4x2)	
Description	Planetary gear train, transverse layout	
Gear Spread	6.635	
		
Gear Ratios		
1st	4.459	
2nd	2.508	
3rd	1.556	
4th	1.142	
5th	0.852	
6th	0.672	
	
4X4 SYSTEMS: JEEP ACTIVE DRIVE, JEEP ACTIVE DRIVE LOW	
Availability 	Jeep Active Drive is optional on all models
Jeep Active Drive Low is standard on Trailhawk	
Type	Fully disconnecting 4x2 mode with automatic 4x4 engagement
Full-time 4x4 mode with active on demand clutch	
Operating Modes	Auto 4x2/4x4, Neutral	
Centre Differential Type	None	
Terrain Response	Unique tuning in all terrain modes	
Crawl Ratio	20:1 (with Jeep Active Drive Low)	
		
ELECTRICAL SYSTEM		
Alternator 	160-amp (2.4-litre Tigershark with MultiAir)  	
Battery	Dual batteries when equipped with electronic stop-start system: 
500-amp (primary) 150-amp (secondary) (2.4-litre Tigershark 
with MultiAir with ESS)	
		
SUSPENSION		
Front 	MacPherson strut, coil springs, flat front steel crossmember,
high-strength steel double shell lower control stabilizer bar	
Rear	Chapman strut, high-strength steel links, isolated steel rear cradle for 4x4 and not-isolated for 4x2, coil springs, stabilizer bar	
		
STEERING		
Type 	Electric power rack and pinion	
Overall Ratio 	15.7	
Turning Diametre (curb-to-curb) 	36.3 (11.07) 4x2 and 4x4
35.3 (10.76) Trailhawk 4x4	
Steering Turns (lock-to-lock)	2.68 (4x2 and 4x4)
2.76 (Trailhawk 4x4)	
		
BRAKES		
Front		
Size and Type	12 x 1.1 (305 x 28) vented rotor with 2.36 (60) single-piston floating caliper	
Swept Area (per caliper)	138.77 sq. in. (895.3 sq. cm), 1 x 60	
115.88 sq. in. (747.6 sq. cm), 1 x 57		
Rear		
Size and Type 	10.95 x 0.47 (278 x 12) solid rotor with 1.5 (38) single-piston floating caliper	
Swept Area (per caliper)	101.7 sq. in. (656.4 sq. cm), 1 x 38	
Power-assist Type 	10 (254) vacuum assist	
Four-wheel anti-lock brake system (ABS)	Standard	
Electronic stability control (ESC)	Standard	
Parking Brake Type	Electric motor	
		
DIMENSIONS AND CAPACITIES		
Wheelbase	103.8 (2,636) 	
Track, Front	60.7 (1,542) 	
Track, Rear	60.3 (1,532) 	
Overall Length	173 (4,394) 	
Overall Width (with folded side mirrors)	73.8 (1,874) 	
Overall Width (with open side mirrors)	80 (2,033) 	
Overall Height 	64.6 (1,641) without rails; 64.8 (1,647) with rails	
Load-floor height	29.7 (754) (height measured from curb ground to load floor)	
Sill-step height	19.4 (494) (height measured from curb ground to sill trim)	
Ground Clearances 	4x2 7.8 (198)
4x4 8.2 (208)
Trailhawk 4x4 8.5 (216)	
Approach Angle, (with air dam) (degrees)	4x2 15.8
4x4 16.8
Trailhawk 4x4 30.3	
Breakover Angle (degrees)	4x2 21.8
4x4 22.9
Trailhawk 4x4 24.4	
Departure Angle (degrees)	4x2 30.8
4x4 31.7
Trailhawk 4x4 33.6	
		
Curb Weight (kg)	3,184 (1,444) 4x2 and 2.4-litre Tigershark with MultiAir
3,327 (1,509) 4x4 and 2.4-litre Tigershark with MultiAir
3,633 (1,648) Trailhawk 4x4 with 2.4-litre Tigershark 
with MultiAir	
Fuel-tank Capacity	13.5 gal. (51 litres) 	
		
ACCOMMODATIONS		
Seating Capacity — Front/Rear 	2/3 	
Front Row		
Headroom without Sunroof	39.2 (995)	
Headroom with Sunroof	38.6 (981)	
Legroom 	41.8 (1,046) 	
Shoulder Room 	56.7 (1,439)	
Hip Room	54.1 (1,375) 	
Seat Travel 	8.7 (220) fore/aft travel range	
Recliner Range (degrees)	Manual/power recliner travel: 69 degrees
Manual fold FWD recliner travel: 107.5 degrees	
SAE Volume (standard roof), cu. ft. (cu. m)	52.9 (1.49) front passenger volume	
Second Row		
Headroom 	38.5 (978)	
Legroom 	38.3 (973)	
Shoulder Room 	55.1 (1,400)	
Hip Room	49.2 (1,250) 	
SAE Volume, cu. ft. (cu. m)	46.7 (1.35) Second-row passenger volume	
Cargo Access		
Liftover Height	31.1 (792) (Height measured from Curb Ground to Liftgate 
Scuff Trim)	
Maximum Cargo Width at Liftgate Opening	42.1 (1,069) 	
Minimum Cargo Width at Liftgate Opening 	36.9 (938) 	
Maximum Cargo Height at Liftgate Opening	27.2 (691) 	
Distance Between Wheelhouse Interior Trim	38.1 (968)	
SAE Cargo Volume		
Rear Seats Up, cu. ft. (cu. m)	27.2 (0.8)	
Rear Seats Folded, cu. ft. (cu. m)	59.8 (1.7)	
EPA Interior Volume Index, cu. ft. (cu. m)	126.7 (3.6)	
		
TIRES		
Availability	Standard — Sport 4x2, Sport 4x4	
Size and Type 	215/65R16 BSW All-season 	
Mfr. and Model 	Continental CrossContact LX Sport (standard) or Kumho Crugen Premium	
Revs per Mile (km)	770 (479)	

Availability	Standard — North 4x2, North 4x4	
Size and Type 	225/60R17 BSW All-season 	
Mfr. and Model 		Bridgestone (standard) or Kumho 	
Revs per Mile (km)	749 (466) 	
		
Availability	Optional — Limited 4x4	
Size and Type 	235/45R19 BSW All Season	
Mfr. and Model	Continental ContiProContact	
Revs per Mile (km)	766 (476)	
		
Availability	Standard  — Trailhawk	
Size and Type	215/65R17 OWL All-season	
Mfr. and Model	Falken WildPeak H/T	
Revs per Mile (km)	744 (462.8) 	
		
Availability	Standard  — Limited	
	Optional  — North	
Size and Type	225/55 R18 BSW All-season 	
Mfr. and Model	Continental 	
Revs per Mile (km)	744 (462)	
		
Availability	Optional — North,  Limited 	
Size and Type	225/55 R18 BSW All-season	
Mfr. and Model	Yokohama 	
Revs per Mile (km)	744 (462)	

////