FCA CANADA
2018 Jeep® Grand Cherokee / Grand Cherokee SRT
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION		
Vehicle Type	Four-door sport-utility vehicle	
Assembly Plant	Jefferson Avenue North Assembly Plant, Detroit, Mich., USA	
EPA Vehicle Class	Multipurpose vehicle	
Introduction Date	Spring 1992 as a 1993 model	
		
BODY AND CHASSIS		
Layout	Front engine, four-wheel drive	
Construction	Steel uniframe	
		
ENGINE: 3.6-LITRE PENTASTAR V6		
Availability	Standard on Laredo, Limited, Trailhawk, Overland and Summit	
Type and Description	60-degree V-type, liquid-cooled	
Displacement	220 cu. in. (3,604 cu. cm)	
Bore x Stroke	3.77 x 3.26 (96 x 83)	
Valve System	Chain-driven DOHC, 24 valves and hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Aluminum deep-skirt block, aluminum alloy heads	
Compression Ratio	10.2:1	
Power (SAE J2723)	Up to 295 hp at 6,400 rpm	
Torque (SAE J2723)	260 lb.-ft. at 4,000 rpm	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R + M)/2	
Oil Capacity	6.0 quarts (5.7 litres)	
Coolant Capacity	14.0 quarts (13.25 litres)	
Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors  and internal engine features(a)	
Max. Gross Trailer Weight	2,812 kg (6,200 lbs.) —  4WD	
Energuide Estimated Fuel Economy L/100 km (imperial mpg) (city/hwy)	12.7 (22) / 9.6 (29)	
Based on 2018 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information please visit the government of Canada website www.vehicles.nrcan.gc.ca	
Assembly Plant	Trenton South Engine Plant, Trenton, Mich., USA	

ENGINE: 5.7-LITRE V8		
Availability	Optional — Limited, Trailhawk, Overland and Summit	
Type and Description	90-degree V-type, liquid-cooled	
Displacement	345 cu. in. (5,654 cu. cm)	
Bore x Stroke	3.92 x 3.58 (99.5 x 90.9)	
Valve System	Variable-valve timing (VVT), pushrod-operated overhead valves, 16 valves, eight deactivating and eight conventional hydraulic lifters, all with roller followers	
Fuel Injection	Sequential, multi-port, electronic, returnless	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps, aluminum alloy heads with hemispherical combustion chambers	
Compression Ratio	10.5:1	
Power (SAE J2723)	360 hp (268 kW) at 5,150 rpm	
Torque (SAE J2723)	390 lb.-ft. (520 N•m) at 4,250 rpm	
Max. Engine Speed	5,800 rpm (electronically-limited)	
Fuel Requirement	Unleaded mid-grade, 89 octane (R+M)/2 — recommended; unleaded regular, 87 octane (R+M)/2 — acceptable	
Oil Capacity	7 quarts (6.6 litres)	
Coolant Capacity	14.5 quarts (13.72 litres)	
Emission Controls 	Dual close-coupled three-way catalytic converters, quad heated oxygen sensors and internal engine features(a)	
Max. Gross Trailer Weight	3,266 kg (7,200 lbs.) 	
2017 Energuide Estimated Fuel Economy L/100 km (imperial mpg) (city/hwy)	16.7 (17) / 10.9 (26)	
Based on 2018 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information please visit the government of Canada website www.vehicles.nrcan.gc.ca
Assembly Plant	Saltillo North Engine Plant, Saltillo, Mexico	
		
ENGINE:  3.0-LITRE DOHC ECODIESEL V6	
Availability	Optional — Limited, Trailhawk, Overland and Summit	
Type and Description	60-degree V-type, liquid-cooled	
Displacement	182 cu. in. (2988 cu. cm)	
Bore x Stroke	3.27 x 3.60 (83 x 92)	
Valve System	Chain-driven DOHC, 24 valves 	
Fuel Injection	Common-rail, 2000 bar, Solenoid Injectors	
Construction	Iron block, aluminum alloy heads	
Compression Ratio	16.5:1	
Power (SAE J2723)	240 hp (179 kW) at 3,600 rpm 	
Torque (SAE J2723)	420 lb.-ft. (569 N•m) at 2,000 rpm	
Max. Engine Speed	4,800 rpm (electronically limited)	
Fuel Requirement	Ultra Low-sulfur diesel	
Oil Capacity	8.2 quarts (7.8 litres)	
Coolant Capacity	12 quarts (11.4 litres)	
Emission Controls 	Cooled EGR, Oxidation catalyst, Diesel particulate filter, SCR with urea injection	
Max. Gross Trailer Weight	3,266 kg (7,200 lbs.)	
	
2017 Energuide Estimated Fuel Economy L/100 km (imperial mpg) (city/hwy)	 11.2 (25) / 8.4 (34)	
Based on 2018 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information please visit the government of Canada website www.vehicles.nrcan.gc.ca
Assembly Plant	VM Motoric Cento, Ferrara, Italy	
		
ENGINE: 6.4-LITRE V8	
Availability	Standard — SRT 	
Type and Description	90-degree V-type, liquid-cooled	
Displacement, cu. in. (cu. cm.)	392 (6,417)	
Bore x Stroke	4.09 x 3.72 (103.9 x 94.5)	
Valve System	Pushrod-operated overhead valves, 16 valves with sodium-filled exhaust valves and hollow stem intake valves, 16 conventional hydraulic lifters, all with roller tips	
Fuel Injection	Sequential, multi-port, electronic, returnless; automatic features Fuel Saver mode	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps, aluminum alloy heads with hemispherical combustion chambers	
Compression Ratio	10.9:1	
Power (SAE J2723)	475 hp (354 kW) at 6,000 rpm 	
Torque (SAE J2723)	470 lb.-ft. (637 N•m) at 4,300 rpm 	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Premium 91 octane (R+M)/2 — recommended	
Oil Capacity, qt. (litre) 	7 (6.6)	
Coolant Capacity, qt. (litre)	14 (13.25)	
Factory Oil Fill 	0W-40 Pennzoil Ultra synthetic	
Emission Controls 	Dual close-coupled three-way catalytic converters, quad-heated oxygen sensors and internal engine features(a)	
Exhaust Type 	Dual exhaust with dual 4-in. oval black chrome tips 	
	
2017 Energuide Estimated Fuel Economy L/100 km (imperial mpg) (city/hwy)	18.3 (15) / 12.6 (22)	
Based on 2018 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information please visit the government of Canada website www.vehicles.nrcan.gc.ca
Assembly Plant	Saltillo Engine Plant, Saltillo, Mexico 	
		
ENGINE: 6.2-LITRE SUPERCHARGED V8	
Availability	Standard – Trackhawk 	
Type and Description	90-degree V-type, liquid-cooled	
Displacement	376 cu. in. (6,166 cu. cm)	
Bore x Stroke	4.09 x 3.58 (103.9 x 90.9)	
Valve System	Pushrod-operated overhead valves, 16 valves with sodium-filled exhaust valves and hollow stem intake valves, 16 conventional hydraulic lifters, all with roller tips	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps, unique aluminum alloy heads with hemispherical combustion chambers	
Compression Ratio	9.5:1	
Power (SAE J2723)	707 hp (527 kW) @ 6,000 rpm	
Torque (SAE J2723)	645 lb.-ft. (875 N•m) torque at 4,800 rpm	
Max. Engine Speed	6,200 rpm (electronically limited)	
Fuel Requirement	Premium 91 octane (R+M)/2 — recommended	
Oil Capacity	8.3 quarts (7.9 litres)	
Factory Oil Fill 	0W-40 Pennzoil Ultra synthetic	
Coolant Capacity	14.7 quarts (13.9 litres)	
Emission Controls 	Dual close-coupled three-way catalytic converters heated wide range upstream and switching downstream O2 sensors and internal engine features. (a)	
Exhaust Type 	Dual 2.75-in. straight-thru exhaust system with quad 4-in. Black Chrome round tips	
2017 Energuide Estimated Fuel Economy L/100 km (imperial mpg) (city/hwy)	TBD	
Based on 2018 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information please visit the government of Canada website www.vehicles.nrcan.gc.ca	
Assembly Plant	Saltillo Engine Plant, Saltillo, Mexico	

TRANSMISSION:  TORQUEFLITE 8HP70 AUTOMATIC, EIGHT-SPEED OVERDRIVE	
Availability	Standard — 3.6-litre, 5.7-litre, 3.0-litre and 6.4-litre equipped models	
Description	Driver-interactive manual control via steering wheel paddle shifters and electronically-modulated torque converter clutch with Eco mode	
Gear Ratios		
1st	4.71	
2nd 	3.14	
3rd	2.11	
4th 	1.67	
5th 	1.29	
6th	1.00	
7th	0.84	
8th 	0.67	
Reverse 	3.30	
	
TRANSMISSION: TORQUEFLITE 8HP95 AUTOMATIC, EIGHT-SPEED OVERDRIVE	
Availability	Standard - Trackhawk	
Description	Adaptive electronic control with driver-interactive manual control via steering wheel paddle shifters, and electronically-modulated torque converter clutch with seven available drive modes including: Auto, Sport, Track, Snow, Tow, Eco and Valet 	
Gear Ratios		
1st	4.71	
2nd 	3.14	
3rd	2.11	
4th 	1.67	
5th 	1.29	
6th	1.00	
7th	0.84	
8th 	0.67	
Reverse 	3.30	
		
TRANSFER CASE: MP 3010		
Availability	Optional with 3.6-litre V6 engine 	
Type	Single-speed	
Operating Mode	Full-time 4WD	
Low Range Ratio	None	
Torque Split, Front/Rear	50/50 	

TRANSFER CASE: MP 3010	
Availability	Standard —  6.4-litre V8 engine 	
Type	Single-speed, electronic proportioning	
Operating Mode	Full-time 4WD	
Torque Split, Front/Rear	Variable – 40/60 Auto, 50/50 Snow and Tow, 35/65 Sport and 30/70 Track	

TRANSFER CASE: MP 3022		
Availability	Optional — 3.6-litre V6, 5.7-litre V8 and 3.0-litre V6 EcoDiesel engines	
Type	Two-speed, electronically shifted	
Operating Modes	4x4 Low (Lock), Neutral; full-time active 4x4	
Low Range Ratio	2.72	
Torque Split, Front/Rear	Variable	
	
TRANSFER CASE: MP 3015C	
Availability	Standard — supercharged 6.2-litre V8 engine 	
Type	Single-speed, electronic proportioning	
Operating Mode	Full-time four-wheel drive 	
Torque Split, Front/Rear	Variable – 40/60 Auto, 50/50 Snow, 60/40 Tow, 35/65 Sport and 30/70 Track	
AXLES		
Front		
Differential Type	Conventional	
Availability	Standard on 4x4 models 	
Ring Gear Diametre	7.7 (195)	
Axle Ratios	3.45:1 — 3.6-litre V6 and EcoDiesel	
	3.09:1 — 5.7-litre V8	
	3:70:1 — 6.4-litre V8 and 6.2-litre V8 	
Rear		
Differential Type	Conventional (optional Electronic Limited Slip on 5.7-litre V8 and EcoDiesel, Standard on 6.4-litre V8)	
Availability	Standard on all engines	
Ring Gear Diametre (in/mm)	7.7 (195) — V6 4x4 	
	9.1 (230) — V6 4x2, EcoDiesel, 5.7-litre V8 and 6.4-litre V8	
Axle Ratios	3.27:1 — V6 4x2	
	3.45:1 — V6 and EcoDiesel	
	3.09:1 — 5.7-litre V8	
	3:70:1 — 6.4-litre V8 and 6.2-litre V8	
		
ELECTRICAL SYSTEM		
Alternator	160-amp; 180-amp or 220-amp depending on model	
Battery	Maintenance-free 	
	H6 650 CCA + Auxiliary 200 CCA on Electronic Stop/Start (ESS)	
	H7 700 CCA on V8, H8 800 CCA on 3.0-litre EcoDiesel 
(not equipped with ESS)	

SUSPENSION		
Front	Short- and long-arm independent (SLA), coil springs, gas-charged, twin-tube coilover shock absorbers, steel upper- and aluminum lower-control arms 
(“A” arms), aluminum knuckle, hollow stabilizer bar	
Front – SRT and Trackhawk 	Short- and long-arm independent (SLA) with aluminum lower control arm, aluminum knuckle, aluminum clevis, coil springs, Bilstein adaptive damping suspension (ADS), upper- and lower-control arms (“A” arms), hollow stabilizer bar	
Rear	Multi-link rear suspension, coil spring, twin tube shocks (including load leveling for towing), aluminum lower control arm, independent upper links (tension and camber) plus a separate toe link, hollow stabilizer bar	
Rear – SRT and Trackhawk 	Multi-link rear suspension, coil spring, Bilstein adaptive damping suspension (ADS), aluminum lower control arm, independent upper links (tension and camber) plus a separate toe link, hollow stabilizer bar	
		
STEERING		
Type	Electric rack and pinion, SRT-tuned on SRT model	
Overall Ratio	17.9:1 (V6 4x2); 16.5:1 on SRT and Trackhawk; 16.7:1 (all other vehicles)	
Turning Diametre (curb-to-curb) (ft./m)	37.1 (11.3); 38.0 (11.6) for SRT and Trackhawk  	
Steering Turns (lock-to-lock)	3.4 (V6 4x2), 3.2 (all other vehicles)	
		
BRAKES		
Type	Power, single-rate, tandem diaphragm vacuum, anti-lock braking system (ABS)	
Availability	Standard	
Front		
Rotor size and type	13.0 x 1.3 (330 x 32) vented disc – V6	
	13.8 x 1.3 (350 x 32) – EcoDiesel and 5.7-litre V8	
	15.0 x 1.34 (380 x 34) vented disc with Brembo six-piston caliper and ABS – SRT 6.4-litre V8	
	15.0 x 1.34 (380 x 34) two-piece aluminum hat performance rotor, directionally slotted with Brembo six-piston caliper and ABS – available on SRT model	
	15.75 x 1.42 (400 x 36) two-piece aluminum hat performance rotor, directionally slotted with Brembo six-piston caliper and ABS – standard on Trackhawk	
	
Caliper size and type		1.89 (48) two-piston pin-slider caliper	
	6 x 40 six-piston fixed caliper on SRT and Trackhawk	
Swept area, (sq. in. / sq. cm)

		282 (1,820)		
	413 (2,666) — SRT	
	498.6 (3,217) — Trackhawk	
Rear		
Rotor size and type	13.0 x 0.55 (330 x 14) disc – V6	
	13.0 x 0.87 (330 x 22) vented disc – EcoDiesel and V8	
	13.78 x 1.10 (350 x 28) disc with Brembo four-piston caliper and single-channel ABS – SRT	
	13.78 x 1.10 (350 x 28) Performance disc, directionally slotted with Brembo four-piston caliper and single-channel ABS on Trackhawk and available on SRT	
Caliper size and type	1.89 (48) single-piston pin-slider caliper
4 x 34 four piston fixed caliper on SRT and Trackhawk 	
Swept area, (sq. in. / sq. cm)	257 (1,658)	
	316 (2,039)  — SRT and Trackhawk 	
		
DIMENSIONS AND CAPACITIES	
Wheelbase	114.7 (2,914)	
Track, Front	63.9 (1,623)	
	65.7  (1,636) — SRT and Trackhawk 	
Track, Rear	64.1 (1,627)	
	64.8 (1,645) — SRT and Trackhawk 	
Overall Length	189.8 (4,822)	
Overall Width (Width at Mirrors)	84.8 (2,154)	
Body Width	76.5 (1,943)	
Overall Height (at Roof Rail / at Antenna)	69.3 (1,761) / 70.0 (1,779)	
	67.9/70.0 (1,724/1,778) — SRT and Trackhawk 	
	
Load Floor Height	32.4 (822) — standard suspension 	
	32.6 (829) – SRT and Trackhawk	
	31.8 (807) — air suspension	
Sill Step Height	20.5 (520) — standard suspension	
	20.0 (508) — air suspension	
	20.7 (527) — SRT	
Ground Clearance  (with P265/60R18 Tire and 3.6-litre engine)	8.6 (218) — standard suspension	
	10.4 (264) — air suspension (Pos#2)	
	10.8 (264) — air suspension (Pos#2) – Trailhawk with 265/60R18 Tire 	
Ground Clearance – SRT and Trackhawk	8.1 (215.4) 	
Chassis (Fuel Tank) 	9.6 (243) — standard suspension	
	10.7 (271) — air suspension (Pos#2)	
	9 (230) — SRT and Trackhawk 	
Front Axle 	9.3 (236) — standard suspension	
	9.7 (246) — air suspension (Pos#2)	
	8.97 (227.8) — SRT and Trackhawk 	
Rear Axle 	10.0 (253) — standard suspension	
	11.1 (282) — air suspension (Pos#2)	
	8.99 (228.3) — SRT and Trackhawk 	
Approach Angle (degrees)	26.2 — standard suspension	
	36.1 — air suspension (Pos#2, air-dam off)	
	29.8 (Off-Road II w/air dam on)	
	18 — SRT and Trackhawk 	
Ramp Breakover Angle (degrees)	19.0 — standard suspension	
	22.8 — air suspension (Pos#2)	
	25.7—Trailhawk	
	18.4  — SRT and Trackhawk 	
Departure Angle (degrees)	24.0 — standard suspension	
	27.1 — air suspension (Pos#2)	
	23.1 — SRT and Trackhawk 	
Frontal Area sq. ft. (sq. m)	31.0 (2.88)	
	31.5 (2.93) — SRT and Trackhawk 	
Drag Coefficient 	0.371	
	0.37  — SRT and Trackhawk 	
Aero CdA	11.5 (Cd x cross-sectional area)	
	11.75  (Cd x cross-sectional area) — SRT and Trackhawk 	
Fuel Tank Capacity, (gallons / (litre)	24.6 (93.1)	

ACCOMMODATIONS		
Seating Capacity (front/rear) 	2/3	
SAE Total Interior Passenger Volume, 
(cu. ft. / cu. m)	105.4 (2.98)	
Front		
Headroom	39.9 (1,013)	
Legroom	40.3 (1,025)	
Shoulder Room	58.7 (1,491)	
Hip Room	57.0 (1,449)	
Seat Travel	11.0 (280)	
EPA Front Volume Index 
(cu. ft. / cu. m)	54.6 (1.55)	
Rear 		
Headroom	39.2 (995)	
Legroom	38.6 (981)	
Knee Clearance	4.3 (110)	
Shoulder Room	58.0 (1,474)	
Hip Room	56.2 (1,428)	
EPA Rear Seat Volume Index 
(cu. ft. / cu. m)	50.8 (1.4)	
Maximum Cargo Volume (cu. ft. / cu. m) 	68.3 (1.93)	
Behind Second-row Seats 
(cu. ft. / cu. m)	36.3 (1.03)	
Total Passenger plus Cargo Volume 
(cu. ft. / cu. m)	140.5 (3.98)	

WEIGHTS (Estimates)	

	

	
MODEL	
ENGINE	
GVWR(a) lbs. (kg)	
CURB WEIGHT(b) lbs. (kg)	
PAYLOAD(c) lbs. (kg)	

4WD	
Laredo	
3.6-litre	
6,500 (2,948)	
4,625 (2,098)	
1,370 (620)	

Limited	
3.6-litre
5.7-litre
3.0-litre EcoDiesel	
6,500 (2,948)
6,800 (3,084)
6,800 (3,084)	
4,746 (2,153)
5,010 (2,273)
5,174 (2,347)	
1,380 (625)
1,410 (640)
1,410 (640)	

Trailhawk	
3.6-litre
5.7-litre
3.0-litre EcoDiesel	
6,500 (2,948)
6,800 (3,084)
6,800 (3,084)	
5,004 (2,270)
5,253 (2,383)
5,412 (2,455)	
1,130 (515)
1,130 (515)
1,130 (515)	

	
Overland	
3.6-litre
5.7-litre
3.0-litre EcoDiesel	
6,500 (2,948)
6,800 (3,084)
6,800 (3,084)	
4,965 (2,252)
5,185 (2,352)
5,361 (2,432)	
1,280 (580)
1,220 (555)
1,220 (555)	

Summit	
3.6-litre
5.7-litre
3.0-litre EcoDiesel	
6,500 (2,948) 
6,800 (3,084)
6,800 (3,084)	
5,000 (2,268)
5,258 (2,385)
5,434 (2,465)	
1,160 (525)
1,160 (525)
1,160 (525)	

SRT	
6.4-litre	
6,500 (2,948)	
5,104 (2,315)	
1,350 (612)	

Trackhawk	
6.2-litre	
6,600 (2,994)	
5,363 (2,433)	
1,350 (612)	

(a) Gross Vehicle Weight Rating.
(b) Curb weight includes standard equipment and full quantities of fuel, lubricant and coolant.
(c) Payload is the maximum allowable weight of driver, passengers, cargo, and options, rounded to the nearest 10 lbs. (5kg).	

WEIGHT DISTRIBUTION, F/R	
	MODEL	ENGINE	DISTRIBUTION	
4WD	Limited	3.6-litre
5.7-litre
3.0-litre EcoDiesel	52/48
54/46
54/46	
	Trailhawk	3.6-litre
5.7-litre
3.0-litre EcoDiesel	52/48
54/46
52/48	
	Overland	3.6-litre
5.7-litre
3.0-litre EcoDiesel	52/48
53/47
53/47	
	Summit	3.6-litre
5.7-litre
3.0-litre EcoDiesel	51/49
53/47
53/47	
	SRT	6.4-litre	55/45	
	Trackhawk	6.2-litre	55/45	

Wheels	
Availability	Standard on Laredo 	
Type and Material	Painted machine cast-aluminum, five-spoke 	
Size (inches)	17 x 8	
		
Availability		Standard on Limited, available on Laredo and Overland 	
Type and Material	Painted machine cast-aluminum, 10-spoke 	
Size (inches)	18 x 8	
	
Availability 		Standard on Trailhawk	
Type and Material	Polished machine cast-aluminum with low gloss painted pockets	
Size (inches)	18x8	
	
Availability	Standard on Overland, available on Limited	
Type and Material	Polished machined cast-aluminum, five-spoke	
Size (inches)	20 x 8	
		
Availability	Standard on Summit	
Type and Material	Polished Machine cast-aluminum with platinum finish	
Size (inches)	20 x 8	
		
Availability 	Optional on Summit 	
Type and Material	Polished machined cast-aluminum, twin five-spoke (Satin Carbon painted with California Edition)	
Size (inches)	20 x 8 	
		
Availability	Standard on SRT	
Type and Material	Forged aluminum, polished, five-spoke “Goliath”	
Size (inches)	20 x 10	
		
Availability	Standard – Trackhawk 	
Type and Material	Forged aluminum, polished with Titanium II pockets and Satin Chrome centre caps	
Size (inches)	20 x 10 	
		
Availability		Optional – SRT and Trackhawk 	
Type and Material	Lightweight forged aluminum, Low Gloss Black with Low Gloss Black centre cap	
Size (inches)	20 x 10	

		
TIRES		
Availability	Standard — Laredo	
Size and Type	P245/70R17	
Mfr. and Model	Goodyear Fortera HL Black Sidewall All-Season 	
Revs per Mile	681	
	
Availability	Standard — Limited; Optional — Laredo and Overland	
Size and Type	265/60R18 	
Mfr. and Model	Michelin Premier LTX Black Sidewall All-Season 	
Revs per Mile	686	
		
Availability 	Standard on Trailhawk	
Size and Type 	265/60R18	
Mfr. And Model 	Goodyear All-Terrain Adventure with Kevlar reinforcement	
Revs per Mile 	687	

Availability 	Standard — Overland; Optional - Limited	
Size and Type	265/50R20	
Mfr. and Model	Bridgestone Ecopia H/L 422 Plus Black Sidewall All-Season 	
Revs per Mile	684	
	
Availability	Standard — Summit; Optional – Overland/Limited	
Size and Type	265/50R20 	
Mfr. and Model	Pirelli Scorpion Verde Black Sidewall All-Season	
Revs per Mile	674	
	
Availability	Packaged with Off-road Adventure II (AWY)	
Size and Type	265/60R18	
Mfr. and Model	Goodyear Wrangler All-Terrain Adventure with Kevlar Black Sidewall	
Revs per Mile	685	
		
Availability	Standard — SRT	
Size and Type	P295/45ZR20	
Mfr. and Model	Pirelli Scorpion Verde —  All-season Performance (run flat)	
Revs per Mile	682	
		
Availability	Optional — SRT	
Size and Type 	P295/45ZR20	
Mfr. and Model	Pirelli P-Zero — Three-season (run flat)	
Revs per Mile	685	
		
Availability	Standard – Trackhawk 	
Size and Type	P295/45ZR20	
Mfr. and Model	Pirelli Scorpion Verde — All-season Performance (run flat)	
Revs per Mile	682 	
		
Availability	Optional – Trackhawk 	
Size and Type 	P295/45ZR20	
Mfr. and Model	Pirelli P-Zero — Three-season (run flat)	
Revs per Mile	685	
		
Parking Brake Type	Drum-in-hat	
Four–wheel Anti-lock Brakes	Standard	
Electronic stability control	Standard	
All-speed traction control	Standard	
Brake Assist	Standard	

TRAILER TOWING				
	Engine	Axle Ratio	Maximum Trailer  
Weight lbs. (kg)	
2WD 	3.6-litre V6
3.0-litre EcoDiesel V6	3.27
3.45	6,200 (2818)
7,400 (3400)	
4WD 	3.6-litre V6
5.7-litre V8
3.0-litre EcoDiesel V6
6.4-litre V8
6.2-litre V8	3.45 
3.09
3.45
3.70
3.70	6,200 (2818)
7,200 (3300)
7,200 (3300)
7,200 (3266)
7,200 (3266)	

////