FCA CANADA
2018 Jeep® Renegade
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION	
Body Style 	Sport-utility vehicle (SUV)	
Assembly Plant	Melfi, Italy	
Energuide Vehicle Class 	Multipurpose vehicle	
	
BODY AND CHASSIS	
Layout	Transverse front engine, 4x2 and 4x4	
Construction 	Steel uniframe	

ENGINE: 1.4-LITRE TURBOCHARGED MULTIAIR I-4	
Availability	Standard — Renegade Sport (4x2 and 4x4) and North (4x2 and 4x4)	
Type and Description	In-line four-cylinder, liquid-cooled, turbocharged	
Displacement	83.48 cu. in. (1,368 cc) 	
Bore x Stroke	2.83 x 3.31 (72.0 x 84.0)	
Valve System	Belt-driven, MultiAir, SOHC, 16 valves,
hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Cast-iron block with aluminum-alloy head and aluminum-alloy bedplate	
Compression Ratio	9.8:1	
Maximum Turbo Boost (psi / bar)	22 psi / 2.49 bar	
Power (SAE)	160 hp (119 kW) @ 5,500 rpm	
Torque (SAE)	184 lb.-ft. (250 N•m) @ 2,500-4,000 rpm	
Max. Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	87 octane (R+M)/2 acceptable 	
	91 octane recommended	
Oil Capacity	4.0 quarts (3.8 litres) with dry filter	
Coolant Capacity	5.5 quarts (5.2 litres)	
Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors and internal engine features	
EnerGuide Fuel Consumption Ratings
L/100km (imp. mpg) (city/hwy/combined)	9.9 (29) / 7.7 (37) (4x2 and 4x4)	
Based on 2018 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information please visit the government of Canada website www.vehicles.nrcan.gc.ca	
Towing	Not recommended 	
Engine Assembly Plant	Termoli, Italy	
		
ENGINE: 2.4-LITRE TIGERSHARK WITH MULTIAIR	
Availability	Standard — Renegade Limited and Trailhawk 	
	Available — Renegade Sport and North (4x2 and 4x4)	
Type and Description	In-line four-cylinder, 16-valve MultiAir with multiport fuel injection	
Displacement	144 cu. in. (2,360 cc) 	
Bore x Stroke	3.46 X 3.82 (88 X 97)	
Valve System	SOHC, four valves per cylinder 	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Aluminum block, aluminum cylinder head	
Compression Ratio	10:1	
Power (SAE net) 	180 hp (134 kW) @ 6,400 rpm	
Torque (SAE net) 	175 lb.-ft. (237 N•m) @ 3,900 rpm	
Max. Engine Speed	6,400 rpm	
Fuel Requirement	Unleaded regular, 87 octane	
Oil Capacity	5.5 quarts (5.2 litres) (total)	
Coolant Capacity	6.8 quarts (6.45 litres)	
Emission Controls	Single catalytic converter, heated wide band lambda sensor upstream and mid-catalyst heated oxygen sensor	
EnerGuide Fuel Consumption Ratings
L/100km (imp. mpg) (city/hwy/combined)	10.8 (26) / 7.8 (36) (4x2)	
	11.2 (25) / 8.2 (34) (4x4)	
Based on 2018 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information please visit the government of Canada website www.vehicles.nrcan.gc.ca	
Towing	2,000 lbs. (907 kg) (not recommended for FWD)	
Engine Assembly Plant 	Dundee Engine Plant, Dundee, Mich.	
		
TRANSMISSION: 948TE NINE-SPEED AUTOMATIC	
Availability	2.4-litre Tigershark engine with MultiAir2 (4x2 or 4x4)	
Description 	Planetary gear train, transverse layout	
Ratio Spread	9.81	
Gear Ratios		
1st	4.71	
2nd	2.84	
3rd	1.91	
4th	1.38	
5th	1.00	
6th	0.81	
7th	0.70	
8th	0.58	
9th	0.48	
Reverse	3.83	
Final-drive Ratio	3.734	
	4.334 (Trailhawk)	
		
C635 SIX-SPEED MANUAL TRANSMISSION		
Availability	1.4-litre MultiAir Turbo engine (4x2 or 4x4)	
Description	1st, 2nd, 3rd gear: Triple cone 	
	4th: Double cone	
Gear Ratios		
1st	4.154	
2nd	2.118	
3rd	1.361	
4th	0.978	
5th	0.756	
6th	0.622	
Reverse	4.00	
Final-drive Ratio	4.438	
Overall Top Gear	2.38	
	
4X4 SYSTEMS: JEEP ACTIVE DRIVE, JEEP ACTIVE DRIVE LOW	
Availability 	Jeep Active Drive is optional on all models
Jeep Active Drive Low is standard on Trailhawk	
Type	Fully disconnecting 4x2 mode with automatic 4x4 engagement
Full-time 4x4 mode with active on demand clutch		
Operating Modes	Auto 4x2/4x4	
Centre Differential Type	None	
Terrain Response	Unique tuning in all terrain modes	
Crawl Ratio	20:1 (with Jeep Active Drive Low)	
		
ELECTRICAL SYSTEM		
Alternator 	150-amp (1.4-litre MultiAir Turbo) 	
	160-amp (2.4-litre Tigershark with MultiAir)  	
Battery	500-amp  (1.4-litre MultiAir Turbo)	
	600-amp (2.4-litre Tigershark with MultiAir)	

SUSPENSION		
Front 	MacPherson strut, coil springs, flat front steel crossmember, high-strength steel double shell lower control arms for 4x4 and high-strength steel mono shell lower control arms for 4x2, stabilizer bar	
Rear	Chapman strut, high-strength steel links, isolated steel rear cradle for 4x4 and not-isolated for 4x2, coil springs, stabilizer bar	
		
STEERING		
Type 	Electric power rack and pinion	
Overall Ratio 	15.7 	
Turning Diametre (curb-to-curb) 	36.3 (11.07) 4x2 and 4x4		
	35.3 (10.76) Trailhawk 4x4	
Steering Turns (lock-to-lock)	2.68 (4x2 and 4x4)		
	2.76 (Trailhawk 4x4)	
BRAKES		
Front		
Size and Type	12 x 1.1 (305 x 28) vented rotor with 
2.36 (60) single-piston floating caliper	
Swept Area (per caliper)	138.77 sq. in. (895.3 sq. cm), 1 x 60		
	115.88 sq. in. (747.6 sq. cm), 1 x 57	
Rear		
Size and Type 	10.95 x 0.47 (278 x 12) solid rotor with 
1.5 (38) single-piston floating caliper	
Swept Area (per caliper)	101.7 sq. in. (656.4 sq. cm), 1 x 38	
Power-assist Type 	10 (254) vacuum assist 	
Four-wheel anti-lock brake system (ABS)	Standard	
Electronic stability control (ESC)	Standard	
Parking Brake Type	Electric motor on caliper	
		
DIMENSIONS AND CAPACITIES		
Wheelbase	101.2 (2,570) 	
Track, Front	60.6 (1,540)	
Track, Rear	60.6 (1,540)	
Overall Length	166.6 (4,232)	
Overall Width (with folded side mirrors)	74.2 (1,886.8)	
Overall Width (with open side mirrors)	79.6 (2,023.1)	
Overall Height 	66.5 (1,689) 	
Load-floor height	29.8 (758) 	
Sill-step height	19.4 (494) front, 19.6 (497) rear	
Ground Clearances 	6.7 (170) 4x2		
	8.0 (203) 4x4  (8.0 – 203)	
	8.7 (220) Trailhawk 4x4	
Approach Angle, (with air dam) (degrees)	17.9 4x2		
	21.0 4x4	
	30.5 Trailhawk 4x4	
Breakover Angle (degrees)	21.2 4x2		
	24.0 4x4	
	25.7 Trailhawk 4x4	
	
Departure Angle (degrees)	29.7 4x2		
	32.1 4x4 	
	34.3 Trailhawk 4x4	
Curb Weight (kg)	3,056 (1,386) 4x2 and 1.4-litre MultiAir Turbo	
	3,210 (1,456) 4x4 and 1.4-litre MultiAir Turbo	
	3,166 (1,436) 4x2 and 2.4-litre Tigershark with MultiAir	
	3,327 (1,509) 4x4 and 2.4-litre Tigershark with MultiAir	
	3,532 (1,602) Trailhawk 4x4 with 2.4-litre Tigershark with MultiAir	
Aero Cd	0.35 4x2		
	0.36 4x4	
	0.37 Trailhawk 4x4	
Fuel-tank Capacity	12.7 gal. (48 litres)	
		
ACCOMMODATIONS		
Seating Capacity — Front/Rear 	2/3	
Front Row		
Headroom without Sunroof	41.1 (1,045)	
Headroom with Sunroof	39.7 (1,009)	
Legroom 	41.2 (1,046)	
Shoulder Room 	55.9 (1,419)	
Hip Room	53.1 (1,348)	
Seat Travel 	9.0 (230) driver / 10.2 (260) front passenger	
Recliner Range (degrees)	From 25 nominal, 38 forward and 30 rearward (from vertical 
13 forward, 55 rearward)	
SAE Volume (standard roof), cu. ft. (cu. m)	54.8 (1.55)	
Second Row		
Headroom 	40.5 (1,029)	
Legroom 	35.1 (891)	
Shoulder Room 	55.1 (1,400)	
Hip Room	51.9 (1,319)	
SAE Volume, cu. ft. (cu. m)	45.3 (1.28)	
Cargo Access		
Liftover Height	30.2 (766)	
Maximum Cargo Width at Liftgate Opening	40.1 (1,020)	
Minimum Cargo Width at Liftgate Opening 	39.0 (990) at bottom of opening	
Maximum Cargo Height at Liftgate Opening	29.5 (749)	
Minimum Cargo Height at Liftgate Opening	29.0 (739)	
Distance Between Wheelhouse Interior Trim	37.6 (956)	
SAE Cargo Volume		
Rear Seats Up, cu. ft. (cu. m)	18.5 (0.525)	
Rear Seats Folded, cu. ft. (cu. m)	50.8 (1.440)	
EPA Interior Volume Index, cu. ft. (cu. m)	118.6 (3.359)	
Behind Rear Seat, cu. ft. (cu. m)	18.5 (0.525) (rear seat at design position)	
Behind Front-row Seats with Rear Seats Folded, cu. ft. (cu. m)	50.8 (1.440) 	
		
TIRES		
Availability	Standard — Sport / North	
Size and Type 	215/65R16 BSW All-season 	
Mfr. and Model 	Continental, CrossContact LX Sport	
Revs per Mile (km)	749 (464)	
		
Availability	Standard — North (with 2.4-litre Tigershark with MultiAir) 	
	Optional — Sport	
Size and Type 	215/60R17 BSW All-season 	
Mfr. and Model 	Continental, CrossContact LX Sport	
Revs per Mile (km)	768 (478)	
		
Availability	Standard — Limited 		
	Optional — North	
Size and Type 	225/55R18 BSW All-season 	
Mfr. and Model	Goodyear Eagle Sport or Kumho Crugen 	
Revs per Mile (km)	729 (452)	
		
Availability	Standard — Trailhawk	
Size and Type	215/65R17 BSW On/Off-Road All-season	
Mfr. and Model	Falken WildPeak H/T	
Revs per Mile (km)	722 (448)	

////