FCA CANADA
2018 Ram Commercial ProMaster™
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION	
Body Styles and Wheelbase	ProMaster 1500 Cargo Van 118-in. wheelbase low roof
ProMaster 1500 Cargo Van 136-in. wheelbase low roof
ProMaster 1500 Cargo Van 136-in. wheelbase high roof	
	ProMaster 2500 Cargo Van 136-in. wheelbase high roof
ProMaster 2500 Cargo Van 159-in. wheelbase high roof	
	ProMaster 2500 Window Van 159-inch wheelbase high roof
ProMaster 3500 Window Van 159-inch wheelbase high roof extended body
ProMaster 3500 Cargo Van 159-in. wheelbase high roof
ProMaster 3500 Cargo Van 159-in. wheelbase high roof extended body	
	ProMaster 3500 Chassis Cab 159-in. wheelbase
ProMaster 3500 Chassis Cab 159-in. wheelbase extended body	
	ProMaster 3500 Chassis Cab Cutaway 159-in. wheelbase
ProMaster 3500 Chassis Cab Cutaway 159-in. wheelbase extended frame	
Assembly Plant	Saltillo Van Assembly, Saltillo, Mexico	
		
BODY AND CHASSIS		
Layout	Transverse front engine	
Construction	Unibody and ladder frame	
	
ENGINE: 3.6-LITRE PENTASTAR V-6 	
Type and Description	60-degree gasoline V-type	
Displacement	220 cu. in. (3,604 cu. cm)	
Bore x Stroke	3.78 x 3.27 (96.0 x 83.0)	
Valve System	Chain-driven DOHC, 24 valves and hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Aluminum deep-skirt block, aluminum alloy heads	
Compression Ratio	10.2:1	
Power 	280 hp (224 kW) at 6,400 rpm	
Torque 	260 lb.-ft. (364 N•m) at 4,400 rpm	
Max. Engine Speed	6,400 rpm (electronically limited) 	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity	6.0 quarts (5.7 litres)	
Coolant Capacity	14.0 quarts (13.25 litres)	
Emission Controls	Dual three-way catalytic converters, heated oxygen sensors	
		
ENGINE: 3.0-LITRE ECODIESEL I-4 (late availability)	
Type and Description	I-4 diesel, variable geometry turbocharger 	
Displacement	183 cu. in. (2,998 cu. cm)	
Bore x Stroke	3.78 x 4.09 (95.8 x 104)	
Valve System	Gear-driven DOHC	
Fuel Injection	Electronically controlled common rail MultiJet direct injection 	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps and aluminum alloy head 	
Compression Ratio	17.5:1	
Power 	174 hp (129 kW) @ 3,500 rpm	
Torque 	295 lb.-ft. (400 N•m) @ 1,400 rpm	
Max. Engine Speed	4,200 rpm	
Fuel Requirement	Diesel	
Oil Capacity	9.5 quarts (9 litres)	
Coolant Capacity	14.0 quarts (13.3 litres)	
Emission Controls	Selective Catalytic Reduction (SCR)	
	
TRANSMISSION: 62TE AUTOMATIC SIX-SPEED, FRONT-WHEEL DRIVE	
Availability	Standard with 3.6-litre Pentastar V6	
Description	Three planetary gear sets, one overrunning clutch, full electronic control, electronically controlled converter clutch	
Gear Ratios		
1st	3.90	
2nd	2.69	
3rd	2.16	
4th	1.37 	
5th	0.95	
6th	0.65	
Reverse	3.04	
Final Drive and Overall Top Gear Ratios	3.86	

TRANSMISSION: MT40 MANUAL AUTOMATIC SIX-SPEED, FRONT-WHEEL DRIVE	
Availability	Standard with 3.0-litre I-4 turbo diesel	
Description	Single disc clutch with hydraulic release	
Gear Ratios		
1st	4.17 	
2nd 	2.35	
3rd 	1.46	
4th 	0.96	
5th 	0.70	
6th 	0.55	
Reverse 	4.08	
Final Drive and Overall Top Gear Ratios	4.56	
		
AXLES		
Front	IFS	
Rear – Cargo Van	Solid axle	
Rear – Chassis Cab and Cut Away	Solid axle 	
	
ELECTRICAL SYSTEM	
Alternator	Cargo van with gas engine: 180-amp standard; 220-amp optional; Cargo van with diesel, all Chassis cab and all cut-away: 220-amp standard	
Battery	95 amp with 800 CCA; 100 amp with 950 CCA (diesel) 	

		
SUSPENSION	
Front	MacPherson with stabilizer bar	
Rear	Solid axle with leaf springs	
		
STEERING		
Type	Rack and pinion with hydraulic power steering	
Turns lock to lock 	Short wheelbase – 11.06; medium wheelbase – 12.46; medium-long wheelbase – 13.54; long wheelbase – 14.28	
Steering ratio 	18.85	
		
BRAKES		
Front Rotor (diameter x width)	11.8 x 1.26 (300 x 32)	
Rear Rotor (diameter x width)	11.0 x 0.63 (280 x 16)	
Front Caliper, Lining	Cast iron, dual piston (46mm and 52mm), Brembo	
	Cast iron, dual piston (50mm and 52mm), Brembo	
Rear Caliper, Lining	Cast iron, single piston (48mm), Brembo	
	Cast iron, single piston (52mm), Brembo	

BODY DIMENSIONS / SPECIFICATIONS – mm (in) unless otherwise noted	
Vehicle and Body Type	Wheelbase	Height Category	Turning Diametre m (feet)	Body Height	Body Overall Length	Body Width w/o mirrors	Vehicle Width w/ mirrors folded	Vehicle Width w/ mirrors extended	Cab to Rear Axle	Overhang Rear Axle to End of Frame	
1500 Cargo Van SWB 
low roof	118	H1	11.1 (36.3)	2,311 (91)	4,953 (195)	2,101 (82.7)	2,299 (90.5)	2,489 
(98)	—	—	
1500 Cargo Van MWB 
low roof	136	H1	12.4 (40.7)	2,311 (91)	5,413 (213.1)	2,101 (82.7)	2,299 (90.5)	2,489 
(98)	—	—	
1500 Cargo Van MWB 
high roof	136	H2	12.4 (40.7)	2,565 (101)	5,413 (213.1)	2,101 (82.7)	2,299 (90.5)	2,489 (98)	—	—	
2500 Cargo Van MWB 
high roof	136	H2	12.4 (40.7)	2,565 (101)	5,413 (213.1)	2,101 (82.7)	2,299 (90.5)	2,489 (98)	—	—	
2500 Cargo Van LWB 
high roof	159	H2	14.3 (46.8)	2,565 (101)	5,994 (236)	2,101 (82.7)	2,299 (90.5)	2,489 (98)	—	—	
3500 Cargo Van LWB 
high roof	159	H2	14.3 (46.8)	2,565 (101)	5,994 (236)	2,101 (82.7)	2,299 (90.5)	2,489 (98)	—	—	
3500 Cargo Van LWB 
high roof extended 	159	H2	14.3 (46.8)	2,565 (101)	6,350 (250)	2,101 (82.7)	2,299 (90.5)	2,489 (98)	—	—	
2500 Window Van LWB 
high roof	159	H2	14.3 (46.8)	2,565 (101)	5,994 (236)	2,101 (82.7)	2,299 (90.5)	2,489 (98)	—	—	
											
3500 Chassis Cab LWB	159	H1	14.3 (46.8)	2,311 (91)	5,944 (234)	2,101 (82.7)	2,337 (92)	2,769 (109)	2,642 (104)	864 
(34)	
3500 Chassis Cab LWB extended	159	H1	14.3 (46.8)	2,311 (91)	6,299 (248)	2,101 (82.7)	2,337 (92)	2,769 (109)	2,642 (104)	1,219 
(48)	
											
3500 Cutaway LWB	159	H1	14.3 (46.8)	2,311 (91)	5,944 (234)	2,101 (82.7)	2,337 (92)	2,769 (109)	2,642 (104)	864 
(34)	
3500 Cutaway LWB extended	159	H1	14.3 (46.8)	2,311 (91)	6,299 (248)	2,101 (82.7)	2,337 (92)	2,769 (109)	2,642 (104)	1,219 
(48)	

Vehicle and Body Type	Wheelbase	Track Front	Track Rear	Approach Angle	Depart Angle	Ground Clearance	Seating(1)	Width between wheel housings	Cargo Volume	Airbags	
1500 Cargo Van SWB low roof	2,997 (118)	1,811 (71.3)	1,791 (70.5)	18.6°	20°	175 (6.9)	3	1,422 (56)	6,589 (259)	6	
1500 Cargo Van MWB low roof	3,454 (136)	1,811 (71.3)	1,791 (70.5)	18.6°	20°	175 (6.9)	3	1,422 (56)	7,722 (304)	6	
1500 Cargo Van MWB high roof	3,454 (136)	1,811 (71.3)	1,791 (70.5)	18.6°	20°	175 (6.9)	3	1,422 (56)	1,422 (56)	6	
2500 Cargo Van MWB high roof	3,454 (136)	1,811 (71.3)	1,791 (70.5)	18.6°	20°	175 (6.9)	3	1,422 (56)	1,422 (56)	6	
2500 Cargo Van LWB high roof	4,039 (159)	1,811 (71.3)	1,791 (70.5)	18.6°	20°	175 (6.9)	3	1,422 (56)	10,668 (420)	6	
3500 Cargo Van LWB high roof	4,039 (159)	1,811 (71.3)	1,791 (70.5)	18.6°	20°	175 (6.9)	3	1,422 (56)	10,668 (420)	6	
3500 Cargo Van LWB high roof extended 	4,039 (159)	1,811 (71.3)	1,791 (70.5)	18.6°	20°	175 (6.9)	3	1,422 (56)	11,760 (463)	6	
2500 Window Van LWB high roof	4,039 (159)	1,811 (71.3)	1,791 (70.5)	18.6°	20°	175 (6.9)	3	1,422 (56)	10,668 (420)	6	
											
3500 Chassis Cab LWB	4,039 (159)	1,811 (71.3)	1,981 (78)	18.6°	—	175 (6.9)	3	—	—	6	
3500 Chassis Cab LWB extended	4,039 (159)	1,811 (71.3)	1,981 (78)	18.6°	—	175 (6.9)	3	—	—	6	
											
3500 Cutaway LWB	4,039 (159)	1,811 (71.3)	1,981 (78)	18.6°	—	175 (6.9)	3	—	—	6	
3500 Cutaway LWB extended	4,039 (159)	1,811 (71.3)	1,981 (78)	18.6°	—	175 (6.9)	3	—	—	6	
(1)	Standard seating configuration is 2-passenger with optional 3-passenger configuration available.

////