FCA CANADA
2018 Ram ProMaster City
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION		
Body Styles	ProMaster City Cargo Van 	
	ProMaster City Wagon	
Assembly Plant	Bursa, Turkey, at Fiat’s joint venture TOFAS plant	
EPA Vehicle Class	Small commercial van (Class 1)	
		
BODY AND CHASSIS		
Layout	Front transverse engine, front-wheel drive (FWD) only	
Construction	Body-frame integral (BFI, or Unibody) with electro-galvanized steel body. Integrated steel ladder H-frame with single-piece longitudinal frame rails	
		
ENGINE: 2.4-LITRE I-4 MULTIAIR2 TIGERSHARK GAS ENGINE	
Availability	Standard on all models	
Type and Description	I-4 (inline 4) 16-valve MultiAir2 with multiport fuel injection	
Displacement 	144 cu.in. (2,360 cu. cm)	
Bore & Stroke	3.46 x 3.82 (88.0 x 97.0)	
Block Material	Aluminum	
Cylinder Head Material	Aluminum	
Valvetrain	DOHC, four valves per cylinder (16 total)	
Ignition System	Coil-on-plug ignition, spark plugs with dual precious metals	
Fuel Delivery	Sequential, multiport, electronic, returnless	
Compression Ratio	10.0:1	
Power 	178 hp (133 kW) at 6,400 rpm 	
Torque 	174 lb.-ft. (236 N•m) at 3,800 rpm 	
Fuel Requirement	Unleaded regular, 87 octane 	
Maximum Engine Speed	6,500 rpm (electronically limited)	
Oil Capacity	5.5 quarts (5.2 litres)	
Coolant Capacity	7.1 quarts (6.7 litres)	
Emissions Controls	GPEC3 engine-management system with close-coupled catalyst and wide-range O2 sensor	
Energuide Estimated Fuel Economy L/100 km (imperial mpg) (city/hwy)	11.2 (25) / 8.3 (34)	
Based on 2018 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information please visit the government of Canada website www.vehicles.nrcan.gc.ca	
		
TRANSMISSION: 948TE NINE-SPEED AUTOMATIC	
Availability	Standard on all models	
Type	Nine-speed FWD, electronically controlled automatic overdrive transmission with torque converter clutch. Clutch-to-clutch architecture with integral electro/hydraulic controls module	
Fluid Capacity	6.5 quarts (6.15 litres)	
Torque Converter	242 mm	
Gear Ratios:		
1st	4.70	
2nd	2.84	
3rd	1.90	
4th	1.38	
5th	1.00	
6th	0.80	
7th	0.69	
8th	0.58	
9th	0.47	
Reverse	3.81	
Final Drive Ratio	3.73	
		
SUSPENSION	
Front Suspension		
Type	MacPherson Strut, independent	
Stabilizer Bar, Solid	26	
Spring Rate (N/mm)	25	
Shock Type	Twin-tube	
Wheel Travel (mm – jounce/rebound)	57/93	
Rear Suspension		
Type	Independent bi-link with coil springs, telescopic shock absorbers and stabilizer bar	
Stabilizer Bar, Solid 	16	
Spring Rate (N/mm)	28	
Shock Type	Twin-tube	
Wheel Travel (mm – jounce/rebound)	51/31	
		
BRAKES		
Front Type (diametre x width)	Ventilated disc, 12 x 1.1 (305 x 28)	
Rear Type (diametre x width)	Drum, 10 x 2.2 (254 x 57)	
Front Caliper, Lining	Cast iron, single piston (57)	
Rear Brake, Lining	Leading trailing drum brake assembly with 25-mm wheel cylinder	
Anti-lock Braking System (front and rear)	Standard	
Electronic Stability Control (ESC) 	Standard	
Total Front Swept Area (mm)	5,100	
Total Rear Swept Area (mm)	12,155	
		
STEERING		
Type	Specifically calibrated hydraulic power-assisted rack-and-pinion	
Ratio	15.9:1	
Turns Lock-to-Lock	2.9	
Turn Diametre – ft. (m) (curb-to-curb)	42 (12.8)	
		
WHEELS AND TIRES		
Wheels	16-in. steel or aluminum	
Tires	215/55R16XL all-season	

		
DIMENSIONS AND CAPACITIES		
EXTERIOR		
Wheelbase 	122.4 (3,109)	
Track, Front	60 (1,523)	
Track, Rear 	60.9 (1,548)	
Overall Length	187.1 (4,752)	
Overall Width (including mirrors)	84.6 (2,148)	
Overall Height 	74.2 (1,886)	
Front Overhang 	35.6 (903)	
Rear Overhang 	29.1 (740)	
Approach Angle (degrees)	13.3	
Departure Angle (degrees)	30.8	
Windshield Slope Angle (degrees)	49.2	
Ground Clearance	5.2 (131)	
Fuel Tank Capacity	16 gallons (60.6 litres)	
			
	Cargo Van	Passenger Wagon	
Cargo Length 	87.2 (2,215)	Behind rear seats = 54.7 (1,389)
Rear seats folded = 69.2 (1,758)	
Cargo Width	60.4 (1,534)	57.6 (1,463)	
Cargo Height @ Roof 	51.8 (1,315.7)	48.7 (1,237)	
Max. Cargo Volume L (cu. ft.)	3,729 (131.7)	2,880 (101.7)	
Cargo Width @ Wheel Well 	48.4 (1,229.4)	48.4 (1,229.4)	
Load Floor Height 	23.3 (592)	23.8 (605)	
Side Door Openings (w x h)	25.8 x 43.6	21.2 x 42.7	
Rear Door Openings (w x h)	48.6 x 47.4	48.6 x 46.4	
Rear Door Swing (degrees, first detent/full open detent)	90/180	90/180	
Rear Door Split (degrees)	60 (driver side)/
40 (passenger side)	60 (driver side)/
40 (passenger side)	
Rear Step-in Height 	23.3 (592)	23.8 (605)	
Side Step-in Height 	21.5 (546)	19.3 (490)	
			
ACCOMMODATIONS			
	Cargo Van	Passenger Wagon	
Seating Capacity (front/rear)	2/0	2/3	
			
Front Row (Passenger & Cargo Vans)		
Headroom 	46.0 (1,169)	46.0 (1,169)	
Leg Room 	40.8 (1,036)	40.8 (1,036)	
Shoulder Room 	59.3 (1,506)	59.3 (1,506)	
Hip Room 	52.8 (1,340)	52.8 (1,340)	
Second Row (Passenger Wagon Only)		
Headroom 		44.0 (1,118)	
Leg Room 		36.8 (935)	
Shoulder Room 		58.0 (1,472)	
Hip Room 	 	59.2 (1,503)	
		
CAPABILITY		
	Cargo Van	Passenger Wagon	
Gross Vehicle Weight Rating (GVWR) kg ((lbs.)	2,447 (5,395)	2,447 (5,395)	
Curb Weight kg (lbs.)	1,592 (3,509)	1,649 (3,635)	
Payload kg (lbs.)	862 (1,901)	798 (1,760)	
Tongue Load kg (lbs.)	91 (200)	91 (200)	
Towing Capacity kg (lbs.)	907 (2,000)	868 (1,914)	
Gross Combined Vehicle Weight Rating kg (lbs.)	2,676 (5,900)	2,676 (5,900)	

////